**3GPP TSG-CT3 Meeting #112e C3-205058\_r1**

**E-Meeting, 04th – 13th November 2020**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.525** | **CR** | **0114** | **rev** | **1** | **Current version:** | **16.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Essential corrections and alignments |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | SBIProtoc16 |  | ***Date:*** | 2020-10-?? |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The following corrections and alignments are necessary:* The "Resource URI" column of Table 5.3.1-1 and Table 5.3.3.4.1-1 should contain a "<relative URI below root>" instead of a full resource URI, as per the API TS skeleton provided in TS 29.501.
* The "Notifications overview" table needs to be updated to align with the SBI TS skeleton provided in TS 29.501.
 |
|  |  |
| ***Summary of change:*** | * Update the "Resource URI" column of Table 5.3.1-1 and Table 5.3.3.4.1-1 by replacing the full resource URI with the associated "<relative URI below root>", i.e. by removing the part "{apiRoot}/<apiName>/<apiVersion>".
* Update the "Notifications overview" table to align with the updated SBI TS skeleton provided in TS 29.501.
* Some additional editorial corrections to improve the text.
 |
|  |  |
| ***Consequences if not approved:*** | Necessary corrections are not applied. |
|  |  |
| ***Clauses affected:*** | 5.3.1, 5.3.3.4.1, 5.5.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact OpenAPI specification files. |
|  |  |
| ***This CR's revision history:*** | Rev 1: Further update the "Notifications overview" table by correcting the content of the "HTTP method or custom operation" column. |

\* \* \* Start of changes \* \* \* \*

5.3.1 Resource Structure

**x**

**Figure 5.3.1-1: Resource URI structure of the Npcf\_UEPolicyControl API**

Table 5.3.1-1 provides an overview of the resources and applicable HTTP methods.

**Table 5.3.1-1: Resources and methods overview**

|  |  |  |  |
| --- | --- | --- | --- |
| **Resource name** | **Resource URI** | **HTTP method or custom operation** | **Description** |
| UE Policy Associations | /policies/ | POST | Create a new Individual UE policy association resource. |
| Individual UE Policy Association | /policies/{polAssoId} | GET | Read an Individual UE Policy Association resource. |
| DELETE | Delete an Individual UE Policy Association resource. |
| /policies/{polAssoId}/update | update (POST) | Report observed event trigger and obtain updated UE policies. |

\* \* \* Next changes \* \* \* \*

##### 5.3.3.4.1 Overview

Table 5.3.3.4.1-1: Custom operations

|  |  |  |  |
| --- | --- | --- | --- |
| Operation name | Custom operation URI | Mapped HTTP method | Description |
| Update | /policies/{polAssoId}/update | POST | Report observed event trigger and obtain updated policies. |

\* \* \* Next changes \* \* \* \*

### 5.5.1 General

Table 5.5.1-1: Notifications overview

|  |  |  |  |
| --- | --- | --- | --- |
| Notification | Callback URI | HTTP method or custom operation | Description (service operation) |
| Policy Update Notification | {notificationUri}/update | update (POST) | Policy Update Notification. |
| Request for termination of the UE policy association | {notificationUri}/terminate | terminate (POST) | Request for termination of the policy association. |

\* \* \* End of changes \* \* \* \*