**3GPP TSG-CT3 Meeting #122e C3-223133**

**E-Meeting, 12th – 20th May 2022**

**Source: Huawei**

**Title: Update of Service descriptions**

**Spec: 29.565 1.3.0**

**Agenda item: 17.16**

**Document for: Decision**

**1. Introduction**

<Introduction part (optional)>

**2. Reason for Change**

Current descriptions of service are clear to indicate the functionality of the service.

**3. Conclusions**

Make above correction.

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 29.565 1.3.0.

\* \* \* First Change \* \* \* \*

## 5.1 Introduction

Table 5.1-1 summarizes the corresponding APIs defined for this specification.

Table 5.1-1: API Descriptions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Service Name** | **Clause** | **Description** | **OpenAPI Specification File** | **apiName** | **Annex** |
| Ntsctsf\_TimeSynchronization | 6.1 |  Provides the support to subscribe/unsubscribe to the notification about time synchronization capabilities and to activate and deactivate the time synchronization configuration. | TS29565\_Ntsctsf\_TimeSynchronization.yaml | ntsctsf-time-sync | A.2 |
| Ntsctsf\_QoSandTSCAssistance | 6.2 | Provides the support to request specific QoS and provide assistance for handling traffic characterized by TSC QoS parameters. | TS29565\_Ntsctsf\_QoSandTSCAssistance.yaml | ntsctsf-qos-tscai | A.3 |
| Ntsctsf\_ASTI | 6.3 | Provides support for time synchronization service based on 5G access stratum time distribution method. | TS29565\_Ntsctsf\_ASTI.yaml | ntsctsf-asti | A.4 |

\* \* \* End of Changes \* \* \* \*