**3GPP TSG- Meeting #C3-242xxx**

**Changsha, China, – was C3-242365**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **1256** | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Various corrections to the definition of the PdtqPolicyNegotiation API |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | AIMLsys |  | ***Date:*** | 2024-04-18 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The definition of the PdtqPolicyNegotiation API needs various corrections and alignments with the drafting rules and NBI TS skeleton. |
|  |  |
| ***Summary of change:*** | This CR proposes to:* Correct the above-detailed issues.
 |
|  |  |
| ***Consequences if not approved:*** | * The provisions related to the definition of the PdtqPolicyNegotiation API continue to contain errors and misalignments with the drafting rules and NBI TS skeleton.
 |
|  |  |
| ***Clauses affected:*** | 5.31.0 (new clause), 5.31.1.1, 5.31.1A (new clause), 5.31.3.4 (new clause), 5.31.4, 5.31.5.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ... |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ... |
|  |  |
| ***Other comments:*** | This CR does not impact the OpenAPI descriptions of the APIs defined in this specification. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* Start of changes \* \* \* \*

### 5.31.0 Introduction

The Nnef\_PdtqPolicyNegotiation service shall use the PdtqPolicyNegotiation API.

The API URI of PdtqPolicyNegotiation API shall be:

**{apiRoot}/<apiName>/<apiVersion>**

The request URIs used in HTTP requests shall have the Resource URI structure defined in clause 5.2.4 of 3GPP TS 29.122 [4], i.e.:

**{apiRoot}/<apiName>/<apiVersion>/<apiSpecificSuffixes>**

with the following components:

- "apiRoot" is set as defined in clause 5.2.4 of 3GPP TS 29.122 [4].

- "apiName" shall be set to "3gpp-pdtq-policy-negotiation".

- "apiVersion" shall be set to "v1" for the current version defined in the present document.

- The <apiSpecificSuffixes> shall be set as described in clause 5.2.4 of 3GPP TS 29.122 [4].

All resource URIs in the clauses below are defined relative to the above API URI.

\* \* \* \* Next changes \* \* \* \*

#### 5.31.1.1 Overview

This clause describes the structure for the Resource URIs as shown in figure 5.29.2.1-1 and HTTP methods used for the PdtqPolicyNegotiation API.

The structure of the resource URIs of the PdtqPolicyNegotiation API is shown in Figure 5.31.1.1-1.



Figure 5.31.1.1-1: Resource URI structure of the PdtqPolicyNegotiation API

Table 5.31.1.1-1 provides an overview of the resources and applicable HTTP methods.

Table 5.31.1.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| PDTQ Policy Subscriptions | /{afId}/subscriptions | GET | Read all active PDTQ Policy Subscription resources for a given AF. |
| POST | Create a new PDTQ Policy Subscription resource. |
| Individual PDTQ Policy Subscription | /{afId}/subscriptions/{subscriptionId} | GET | Read a PDTQ Policy Subscription resource. |
| PATCH | Modify a PDTQ Policy Subscription resource. |
| DELETE | Delete a PDTQ Policy Subscription resource. |

\* \* \* \* Next changes \* \* \* \*

### 5.31.1A Custom Operations without associated resources

There are no custom operations without associated resources defined for this API in this release of the specification.

\* \* \* \* Next changes \* \* \* \*

#### 5.31.3.4 Data types describing alternative data types or combinations of data types

There are no data types describing alternative data types or combinations of data types defined for this API in this release of the specification.

\* \* \* \* Next changes \* \* \* \*

### 5.31.4 Used Features

The optional features listed in table 5.31.4-1 are defined for the PdtqPolicyNegotiation API. They shall be negotiated using the extensibility mechanism defined in clause 5.2.7 of 3GPP TS 29.122 [4].

Table 5.31.4-1: Features used by PdtqPolicyNegotiation API

|  |  |  |
| --- | --- | --- |
| Feature number | Feature Name | Description |
|  |  |  |

\* \* \* \* Next changes \* \* \* \*

#### 5.31.5.1 General

For the PdtqPolicyNegotiation API, HTTP error responses shall be supported as specified in clause 5.2.6 of 3GPP TS 29.122 [4]. Protocol errors and application errors specified in clause 5.2.6 of 3GPP TS 29.122 [4] shall be supported for the HTTP status codes specified in table 5.2.6-1 of 3GPP TS 29.122 [4].

In addition, the requirements in the following clauses are applicable for the PdtqPolicyNegotiation API.

\* \* \* \* End of changes \* \* \* \*