**3GPP TSG-CT WG3 Meeting #134 *C3-242283***

**Changsha, China, 15 - 19 April, 2024 *(Revision of C3-242xxx)***

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.549** | **CR** | **0279** | **rev** | **-** | **Current version:** | **18.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Various updates and corrections about APIs | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NBI18 | | | | |  | ***Date:*** | | | 2024-03-30 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The following issues have been identified in the current specification:   1. The Resource URI in clause 7.10.4.2.1 is incorrect. 2. Additional editorial issues. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Fix the above issues. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incomplete specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 7.10.2, 7.10.3, 7.10.4, 7.10.4.2.1, 7.10.5, 7.10.7 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR does not impact on the OpenAPI files. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

### 7.10.2 SS\_ADAE\_SlicePerformanceAnalytics API

\*\*\* Next Change \*\*\*

### 7.10.3 SS\_ADAE\_Ue2UePerformanceAnalytics API

\*\*\* Next Change \*\*\*

### 7.10.4 SS\_ADAE\_LocationAccuracyAnalytics API

\*\*\* Next Change \*\*\*

7.10.4.2.1 Overview

This clause describes the structure for the Resource URIs and the resources and methods used for the service.

Figure 7.10.4.2.1-1 depicts the resource URIs structure for the SS\_ADAE\_LocationAccuracyAnalytics API.

****

**Figure 7.10.4.2.1-1: Resource URI structure of the SS\_ADAE\_LocationAccuracyAnalytics API**

Table 7.10.4.2.1-1 provides an overview of the resources and applicable HTTP methods.

**Table 7.10.4.2.1-1: Resources and methods overview**

|  |  |  |  |
| --- | --- | --- | --- |
| **Resource name** | **Resource URI** | **HTTP method** | **Description** |
| Location accuracy event subscription | /location-accuracy | POST | Subscription to the event of the location accuracy performance analytics |
| Individual location accuracy event subscription | /location-accuracy/{locAccId} | GET | Request the retrieval of an existing "Individual subscription to the event of the location accuracy analytics" resource. |
| DELETE | Request the deletion of an existing "Individual subscription to the event of the location accuracy analytics" resource. |

\*\*\* Next Change \*\*\*

### 7.10.5 SS\_ADAE\_ServiceApiAnalytics API

\*\*\* Next Change \*\*\*

### 7.10.7 SS\_ADAE\_EdgeLoadAnalytics API

\*\*\* End of Changes \*\*\*