**3GPP TSG CT WG3 Meeting #137 *C3-245484***

**Hefei, CN, 14 - 18 October, 2024 (Revision of C3-245100)**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | TscEvent description addition |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** | **D** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | In the Ntsctsf\_QoSandTSCAssistance openAPI, TscEvent’s description is missing. |
|  |  |
| ***Summary of change:*** | TscEvent description is added.The description update in the enumeration description as well. |
|  |  |
| ***Consequences if not approved:*** | The quality of the openAPI in the specificatin is not up to mark and missing clarity for TSC Event. |
|  |  |
| ***Clauses affected:*** | 6.2.6.3.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact the OpenAPI descriptions defined in this specification. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* First Change \* \* \* \*

##### 6.2.6.3.3 Enumeration: TscEvent

The enumeration TscEvent represents event for TSC. It shall comply with the provisions defined in table 6.2.6.3.3-1.

Table 6.2.6.3.3-1: Enumeration TscEvent

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| FAILED\_RESOURCES\_ALLOCATION | Indicates that one or more of the SDFs of an Individual TSC Application Session Context are deactivated. It also indicates that the resources requested for a particular service information cannot be successfully allocated. |  |
| SUCCESSFUL\_RESOURCES\_ALLOCATION | Indicates that the resources requested for particular service information have been successfully allocated. |  |
| QOS\_GUARANTEED | Indicates that the QoS targets of one or more SDFs are guaranteed again. |  |
| QOS\_NOT\_GUARANTEED | Indicates that the QoS targets of one or more SDFs are not being guaranteed. |  |
| QOS\_MONITORING | Indicates a QoS monitoring event. |  |
| USAGE\_REPORT | Indicates that the volume and/or time usage for sponsored data connectivity. |  |
| BAT\_OFFSET\_INFO | Indicates the BAT offset and the optionally adjusted periodicity. | EnTSCAC |
| QOS\_MON\_CAP\_REPO | Indicates the report of the capability of the QoS Monitoring. | QoSMonCapRepo |

\* \* \* \* End of Changes \* \* \* \*