**3GPP TSG RAN WG2#119bis electronic R2-2210857**

**Online, 10th-19th October, 2022**

Title: DRAFT LS on validity of assistance information

Response to: -

Release: Release 17

**Work Item: NR\_NTN\_solutions**

Source: OPPO (to be RAN2)

To: RAN1

Cc: -

**Contact Person:**

Name: Haitao Li

E-mail Address: lihaitao@oppo.com

**Send any reply LS to: 3GPP Liaisons Coordinator, <mailto:3GPPLiaison@etsi.org>**

Attachments: None

**1. Overall Description:**

Regarding RAN1’s agreement on serving cell’s explicit Epoch time referring to the current SFN or the next upcoming SFN after the frame where the message indicating the Epoch time is received, RAN2 has discussed and thinks that there could be an issue with latency (e.g. for initial access) when Epoch time points to a future time and validity timer has not started.

To solve this issue, RAN2 would like to ask RAN1 whether backwards propagation of satellite assistance information would be needed, or whether the problem could be mitigated by making Epoch time for serving cell the frame nearest to the frame where the message indicating the Epoch time is received, or whether this can be addressed by simply setting the Epoch time properly by the network (i.e. no spec changes).

**2. Actions:**

**To** **RAN1**

**ACTION:** RAN2 respectively requests RAN1 to provide feedback to the above questions.

**3. Date of Next RAN2 Meetings:**

TSG-RAN WG2#120 2022-11-14 to 2022-11-18 Toulouse, FR

TSG-RAN WG2#121 2023-02-27 to 2023-03-03 Athens, GR