{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Cover","PUSCH-CP OFDM","PUSCH- DFT-S-OFDM","PUCCH","PRACH"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #98-bis-e",null,null,null,null,null,null,null,"R4-2106786"]
[null,"Electronic Meeting, Apr.12th - 20th, 2021"]
[]
[null,"Source: Huawei, HiSilicon"]
[null,"Title: Summary of ideal and impairment results for NR-U BS demodulation requirements"]
[null,"Agenda: 5.1.4.4.1"]
[null,"Document for: Information"]

{"sheet":"PUSCH-CP OFDM","index":1,"n_rows":75,"n_cols":22,"rows_kept":75,"cut":false,"hidden":false,"merged":[[0,0,0,16383],[43,5,50,5],[43,6,44,6],[43,7,44,7],[45,6,46,6],[45,7,46,7],[47,6,48,6],[47,7,48,7],[49,6,50,6],[49,7,50,7],[35,5,42,5],[35,6,36,6],[35,7,36,7],[37,6,38,6],[37,7,38,7],[39,6,40,6],[39,7,40,7],[41,6,42,6],[41,7,42,7],[27,5,34,5],[27,6,28,6],[27,7,28,7],[29,6,30,6],[29,7,30,7],[31,6,32,6],[31,7,32,7],[33,6,34,6],[33,7,34,7],[67,5,74,5],[67,6,68,6],[67,7,68,7],[69,6,70,6],[69,7,70,7],[71,6,72,6],[71,7,72,7],[73,6,74,6],[73,7,74,7],[59,5,66,5],[59,6,60,6],[59,7,60,7],[61,6,62,6],[61,7,62,7],[63,6,64,6],[63,7,64,7],[65,6,66,6],[65,7,66,7],[51,5,58,5],[51,6,52,6],[51,7,52,7],[53,6,54,6],[53,7,54,7],[55,6,56,6],[55,7,56,7],[57,6,58,6],[57,7,58,7],[51,0,74,0],[51,1,74,1],[51,2,74,2],[51,3,74,3],[51,4,58,4],[59,4,66,4],[67,4,74,4],[19,5,26,5],[19,6,20,6],[19,7,20,7],[21,6,22,6],[21,7,22,7],[23,6,24,6],[23,7,24,7],[25,6,26,6],[25,7,26,7],[19,4,26,4],[3,0,26,0],[3,1,26,1],[3,2,26,2],[3,3,26,3],[27,0,50,0],[27,1,50,1],[27,2,50,2],[27,3,50,3],[27,4,34,4],[35,4,42,4],[43,4,50,4],[11,4,18,4],[11,5,18,5],[11,6,12,6],[11,7,12,7],[7,6,8,6],[3,7,4,7],[5,7,6,7],[7,7,8,7],[1,7,2,7],[13,6,14,6],[13,7,14,7],[15,6,16,6],[15,7,16,7],[17,6,18,6],[17,7,18,7],[3,5,10,5],[5,6,6,6],[1,16,1,17],[1,18,1,19],[1,20,1,21],[1,1,2,1],[1,4,2,4],[3,4,10,4],[9,6,10,6],[9,7,10,7],[1,2,2,2],[1,3,2,3],[1,0,2,0],[1,5,2,5],[1,8,2,8],[1,9,2,9],[1,10,1,11],[1,6,2,6],[1,12,1,13],[1,14,1,15],[3,6,4,6]]}
[]
["SCS","Bandwidth","PDSCH\nmapping type","DMRS \nconfiguration","PN model","PN \ncompensation","MCS","Propagation conditions","Antenna configurations","Test metric","Huawei",null,"Ericsson",null,"Nokia",null,"Samsung",null,"Span","SPAN","AVE","38.104 req"]
[null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["120kHz","100MHz","Type B","1+1 ","No ","No ",4,"TDLA30-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,{"$f":"MAX(K4,M4,O4,Q4)-MIN(K4,M4,O4,Q4)","v":0},{"$f":"MAX(L4,N4,P4,R4)-MIN(L4,N4,P4,R4)","v":0},{"$f":"AVERAGE(K4,M4,O4,Q4)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(L4,N4,P4,R4)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,{"$f":"MAX(K5,M5,O5,Q5)-MIN(K5,M5,O5,Q5)","v":0},{"$f":"MAX(L5,N5,P5,R5)-MIN(L5,N5,P5,R5)","v":0},{"$f":"AVERAGE(K5,M5,O5,Q5)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(L5,N5,P5,R5)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,16,"TDLA30-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,18,"TDLD30-200","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,20,"TDLD30-200","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,"Set 1","CPE only",4,"TDLA30-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,16,"TDLA30-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,18,"TDLD30-200","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,20,"TDLD30-200","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,"Set 2","CPE only",4,"TDLA30-650","1T1R Low","70% of maxTP",-2,null,null,null,-3.0100153891015702,null,null,null,1.0100153891015702,0,-2.5050076945507849,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",-2.6,null,null,null,1.00316803451946,null,null,null,3.6031680345194603,0,-0.79841598274027004,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,16,"TDLA30-650","1T1R Low","70% of maxTP",9.8000000000000007,null,null,null,8.4703298576430708,null,null,null,1.3296701423569299,0,9.1351649288215349,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",19.600000000000001,null,null,null,16.0138858760651,null,null,null,3.5861141239349017,0,17.806942938032549,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,18,"TDLD30-200","1T1R Low","70% of maxTP",null,null,null,null,8.2332664374211095,null,null,null,0,0,8.2332664374211095,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,24.2746549367737,null,null,null,0,0,24.2746549367737,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,20,"TDLD30-200","1T1R Low","70% of maxTP",10.9,null,null,null,10.205990557154699,null,null,null,0.69400944284530119,0,10.552995278577349,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",15.2,null,null,null,null,null,null,null,0,0,15.2,{"$error":"#DIV/0!"}]
["120kHz","400MHz","Type B","1+1 ","No ","No ",4,"TDLA30-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,16,"TDLA30-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,18,"TDLD30-200","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,20,"TDLD30-200","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,"Set 2","CPE+ICI",4,"TDLA30-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,16,"TDLA30-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,18,"TDLD30-200","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,20,"TDLD30-200","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,"Set 2","CPE only",4,"TDLA30-650","1T1R Low","70% of maxTP",null,null,null,null,-3.1626422841437898,null,null,null,0,0,-3.1626422841437898,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,1.1538723672301601,null,null,null,0,0,1.1538723672301601,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,16,"TDLA30-650","1T1R Low","70% of maxTP",null,null,null,null,8.3364090208717396,null,null,null,0,0,8.3364090208717396,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,17.4498238796076,null,null,null,0,0,17.4498238796076,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,18,"TDLD30-200","1T1R Low","70% of maxTP",null,null,null,null,8.1673516981947891,null,null,null,0,0,8.1673516981947891,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,24.5217925589019,null,null,null,0,0,24.5217925589019,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,20,"TDLD30-200","1T1R Low","70% of maxTP",null,null,null,null,10.151398408592399,null,null,null,0,0,10.151398408592399,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["480kHz","400MHz","Type B","1+1 ","No ","No ",4,"TDLA10-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,16,"TDLA10-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,18,"TDLD10-200","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,20,"TDLD10-200","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,"Set 1","CPE only",4,"TDLA10-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,16,"TDLA10-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,18,"TDLD10-200","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,20,"TDLD10-200","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,"Set 2","CPE only",4,"TDLA10-650","1T1R Low","70% of maxTP",-3.5,null,null,null,-3.4915924322123599,null,null,null,8.407567787640069E-3,0,-3.49579621610618,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",0.2,null,null,null,0.76116055497849,null,null,null,{"$f":"MAX(K69,M69,O69,Q69)-MIN(K69,M69,O69,Q69)","v":0.56116055497848993},{"$f":"MAX(L69,N69,P69,R69)-MIN(L69,N69,P69,R69)","v":0},{"$f":"AVERAGE(K69,M69,O69,Q69)","v":0.48058027748924503},{"$f":"AVERAGE(L69,N69,P69,R69)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,16,"TDLA10-650","1T1R Low","70% of maxTP",7.3,null,null,null,7.8928176773602496,null,null,null,0.59281767736024982,0,7.5964088386801247,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",11.3,null,null,null,15.823864650449,null,null,null,4.5238646504489992,0,13.5619323252245,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,18,"TDLD10-200","1T1R Low","70% of maxTP",null,null,null,null,8.2061184954050006,null,null,null,0,0,8.2061184954050006,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",null,null,null,null,25.0940534207631,null,null,null,0,0,25.0940534207631,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,20,"TDLD10-200","1T1R Low","70% of maxTP",10.1,null,null,null,10.23510186633,null,null,null,0.13510186633000032,0,10.167550933165,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,"2T2R Low","70% of maxTP",15.1,null,null,null,null,null,null,null,0,0,15.1,{"$error":"#DIV/0!"}]

{"sheet":"PUSCH- DFT-S-OFDM","index":2,"n_rows":9,"n_cols":20,"rows_kept":9,"cut":false,"hidden":false,"merged":[[1,14,1,15],[1,16,1,17],[1,18,1,19],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[1,8,1,9],[3,0,5,0],[3,1,5,1],[6,0,8,0],[6,1,8,1],[1,12,1,13],[1,10,1,11],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[3,4,8,4],[3,5,5,5],[6,5,8,5],[3,6,8,6]]}
[]
["SCS","Bandwidth","PN model","PN \ncompensation","MCS","Propagation conditions","Antenna configurations","Test metric","Huawei",null,"Ericsson",null,"Nokia",null,"Samsung",null,"Span","SPAN","Average","38.104 req"]
[null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["120kHz","100MHz","No ","No ",4,"TDLA30-650","1T1R Low","70% of maxTP",null,null,null,null,null,null,null,null,{"$f":"MAX(I4,K4,M4,O4)-MIN(I4,K4,M4,O4)","v":0},{"$f":"MAX(J4,L4,N4,P4)-MIN(J4,L4,N4,P4)","v":0},{"$f":"AVERAGE(I4,K4,M4,O4)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(J4,L4,N4,P4)","v":{"$error":"#DIV/0!"}}]
[null,null,"Set1","CPE only",null,null,null,"70% of maxTP",null,null,null,null,null,null,null,null,{"$f":"MAX(I5,K5,M5,O5)-MIN(I5,K5,M5,O5)","v":0},{"$f":"MAX(J5,L5,N5,P5)-MIN(J5,L5,N5,P5)","v":0},{"$f":"AVERAGE(I5,K5,M5,O5)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(J5,L5,N5,P5)","v":{"$error":"#DIV/0!"}}]
[null,null,"Set2","CPE only",null,null,null,"70% of maxTP",-1.8,null,null,null,-2.8,null,null,null,0.99999999999999978,0,-2.2999999999999998,{"$error":"#DIV/0!"}]
["480kHz","400MHz","No ","No ",null,"TDLA10-650",null,"70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,"Set1","CPE only",null,null,null,"70% of maxTP",null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,"Set2","CPE only",null,null,null,"70% of maxTP",-2.2999999999999998,null,null,null,-3.3,null,null,null,1,0,-2.8,{"$error":"#DIV/0!"}]

{"sheet":"PUCCH","index":3,"n_rows":32,"n_cols":23,"rows_kept":32,"cut":false,"hidden":false,"merged":[[0,0,1,0],[28,5,31,5],[31,9,31,10],[24,6,31,6],[24,7,31,7],[2,4,31,4],[24,9,24,10],[25,9,25,10],[27,9,27,10],[28,9,28,10],[29,9,29,10],[30,9,30,10],[26,9,26,10],[28,1,31,2],[28,3,31,3],[24,1,27,2],[18,9,18,10],[19,9,19,10],[18,6,20,6],[20,9,20,10],[21,9,21,10],[21,6,23,6],[22,9,22,10],[23,9,23,10],[17,9,17,10],[16,6,17,6],[16,9,16,10],[14,0,17,0],[16,1,16,2],[15,9,15,10],[14,9,14,10],[14,6,15,6],[14,1,14,2],[15,1,15,2],[18,0,23,0],[24,0,31,0],[17,1,17,2],[18,1,20,2],[21,1,23,2],[21,3,23,3],[24,3,27,3],[24,5,27,5],[18,5,20,5],[21,5,23,5],[18,3,20,3],[6,0,13,0],[2,1,3,2],[2,9,2,10],[3,9,3,10],[2,5,3,5],[6,7,13,7],[6,1,9,2],[10,1,13,2],[6,5,9,5],[6,9,6,10],[7,9,7,10],[8,9,8,10],[9,9,9,10],[6,3,9,3],[10,3,13,3],[2,6,5,6],[10,5,13,5],[10,9,10,10],[11,9,11,10],[12,9,12,10],[13,9,13,10],[6,6,13,6],[0,21,0,22],[2,0,5,0],[0,1,1,2],[0,5,1,5],[0,9,1,10],[0,11,0,12],[0,8,1,8],[4,1,5,2],[4,5,5,5],[4,9,4,10],[5,9,5,10],[0,3,1,3],[2,3,3,3],[4,3,5,3],[0,4,1,4],[0,6,1,6],[0,19,0,20],[0,7,1,7],[0,13,0,14],[0,15,0,16],[0,17,0,18]]}
["Format","SCS",null,"Bandwidth ","Antennna\n configurations","Propoagation conditions\n and correlation matirx","Number \nof bits","Number of \nOFDM symbols","Number \nof PRBs","Note",null,"Huawei",null,"Ericsson",null,"Nokia",null,"Samsung",null,"Span","SPAN","Average","38.104 req"]
[null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["PF0","120kHz",null,"100MHz","1T2R","TDLA30-650 Low",1,1,1," 1% ACK miss",null,5.4,null,null,null,7.5,null,null,null,{"$f":"MAX(L3,N3,P3,R3)-MIN(L3,N3,P3,R3)","v":2.0999999999999996},{"$f":"MAX(M3,O3,Q3,S3)-MIN(M3,O3,Q3,S3)","v":0},{"$f":"AVERAGE(L3,N3,P3,R3)","v":6.45},{"$f":"AVERAGE(M3,O3,Q3,S3)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,2,16," 1% ACK miss",null,-10.3,null,null,null,-8.6,null,null,null,{"$f":"MAX(L4,N4,P4,R4)-MIN(L4,N4,P4,R4)","v":1.7000000000000011},{"$f":"MAX(M4,O4,Q4,S4)-MIN(M4,O4,Q4,S4)","v":0},{"$f":"AVERAGE(L4,N4,P4,R4)","v":-9.4499999999999993},{"$f":"AVERAGE(M4,O4,Q4,S4)","v":{"$error":"#DIV/0!"}}]
[null,"480kHz",null,"400MHz",null,"TDLA10-650 Low",null,1,1," 1% ACK miss",null,5.8,null,null,null,7.89,null,null,null,2.09,0,6.8449999999999998,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,2,16," 1% ACK miss",null,-7.4,null,null,null,-8.4499999999999993,null,null,null,1.0499999999999989,0,-7.9249999999999998,{"$error":"#DIV/0!"}]
["PF1","120kHz",null,"100MHz",null,"TDLA30-650 Low",2,14,1," 1% ACK miss",null,-6.4,null,null,null,-7.1,null,null,null,0.69999999999999929,0,-6.75,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,1,"0.1%  NACK to ACK",null,-4.8,null,null,null,-5.2,null,null,null,0.40000000000000036,0,-5,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,16," 1% ACK miss",null,-16.399999999999999,null,null,null,-17.2,null,null,null,0.80000000000000071,0,-16.799999999999997,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,16,"0.1%  NACK to ACK",null,-14.6,null,null,null,-16,null,null,null,1.4000000000000004,0,-15.3,{"$error":"#DIV/0!"}]
[null,"480kHz",null,"400MHz",null,"TDLA10-650 Low",null,null,1," 1% ACK miss",null,-6.5,null,null,null,-7.3,null,null,null,0.79999999999999982,0,-6.9,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,1,"0.1%  NACK to ACK",null,-5,null,null,null,-5.2,null,null,null,0.20000000000000018,0,-5.0999999999999996,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,16," 1% ACK miss",null,-14.3,null,null,null,-17,null,null,null,2.6999999999999993,0,-15.65,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,16,"0.1%  NACK to ACK",null,-12.4,null,null,null,-16,null,null,null,3.5999999999999996,0,-14.2,{"$error":"#DIV/0!"}]
["PF2","120kHz",null,"100MHz",null,"TDLA30-650 Low",4,1,4," 1% ACK miss",null,1.8,null,null,null,4.2,null,null,null,2.4000000000000004,0,3,{"$error":"#DIV/0!"}]
[null,"480kHz",null,"400MHz",null,"TDLA10-650 Low",null,1,4," 1% ACK miss",null,1.4,null,null,null,4,null,null,null,2.6,0,2.7,{"$error":"#DIV/0!"}]
[null,"120kHz",null,"100MHz",null,"TDLA30-650 Low",22,2,9," 1% UCI BLER",null,-1.2,null,null,null,-0.5,null,null,null,0.7,0,-0.85,{"$error":"#DIV/0!"}]
[null,"480kHz",null,"400MHz",null,"TDLA10-650 Low",null,2,9," 1% UCI BLER",null,-1.3,null,null,null,-0.7,null,null,null,0.60000000000000009,0,-1,{"$error":"#DIV/0!"}]
["PF3","120kHz",null,"100MHz",null,"TDLA30-650 Low",16,14,1," DMRS 1+1",null,-2.6,null,null,null,-1.1000000000000001,null,null,null,1.5,0,-1.85,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,14,1," DMRS 1+0",null,-2.2000000000000002,null,null,null,-1.7,null,null,null,0.50000000000000022,0,-1.9500000000000002,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,4,3," DMRS 1+0",null,-0.5,null,null,null,-1.1000000000000001,null,null,null,0.60000000000000009,0,-0.8,{"$error":"#DIV/0!"}]
[null,"480kHz",null,"400MHz",null,"TDLA10-650 Low",16,14,1," DMRS 1+1",null,-3,null,null,null,-1.1000000000000001,null,null,null,1.9,0,-2.0499999999999998,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,14,1," DMRS 1+0",null,-2.5,null,null,null,-1.7,null,null,null,0.8,0,-2.1,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,4,3," DMRS 1+0",null,-0.4,null,null,null,-1.1000000000000001,null,null,null,0.70000000000000007,0,-0.75,{"$error":"#DIV/0!"}]
["PF4","120kHz",null,"100MHz",null,"TDLA30-650 Low",22,14,1," DMRS 1+1",null,1.3,null,null,null,0.7,null,null,null,0.60000000000000009,0,1,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,1," DMRS 1+0",null,1.4,null,null,null,0.2,null,null,null,1.2,0,0.79999999999999993,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,16," DMRS 1+1",null,-11.8,null,null,null,-11.8,null,null,null,0,0,-11.8,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,16," DMRS 1+0",null,-10.8,null,null,null,-12.1,null,null,null,1.2999999999999989,0,-11.45,{"$error":"#DIV/0!"}]
[null,"480kHz",null,"100MHz",null,"TDLA10-650 Low",null,null,1," DMRS 1+1",null,2,null,null,null,0.7,null,null,null,1.3,0,1.35,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,1," DMRS 1+0",null,2.5,null,null,null,0.1,null,null,null,2.4,0,1.3,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,16," DMRS 1+1",null,-11,null,null,null,-11.7,null,null,null,0.69999999999999929,0,-11.35,{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,16," DMRS 1+0",null,-10.6,null,null,null,-12.2,null,null,null,1.5999999999999996,0,-11.399999999999999,{"$error":"#DIV/0!"}]

{"sheet":"PRACH","index":4,"n_rows":33,"n_cols":18,"rows_kept":33,"cut":false,"hidden":false,"merged":[[19,2,20,2],[9,1,14,1],[15,1,20,1],[21,0,32,0],[21,1,24,1],[21,2,22,2],[23,2,24,2],[25,1,28,1],[25,2,26,2],[27,2,28,2],[29,1,32,1],[29,2,30,2],[31,2,32,2],[1,0,2,0],[3,0,20,0],[1,12,1,13],[1,14,1,15],[1,16,1,17],[3,2,4,2],[5,2,6,2],[1,8,1,9],[1,10,1,11],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[7,2,8,2],[3,1,8,1],[17,2,18,2],[1,5,2,5],[1,6,1,7],[13,2,14,2],[15,2,16,2],[9,2,10,2],[11,2,12,2]]}
[]
["SCS","Format","LRA","Propagation \nconditions","Frequency \noffset","Test \nmetric","Huawei",null,"Ericsson",null,"Nokia",null,"Samsung",null,"Span","SPAN","Avcrage","38.104 req"]
[null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["120kHz","A2",1151,"AWGN",0,"1% Pmd",null,null,null,null,-23.63,null,null,null,{"$f":"MAX(G4,I4,K4,M4)-MIN(G4,I4,K4,M4)","v":0},{"$f":"MAX(H4,J4,L4,N4)-MIN(H4,J4,L4,N4)","v":0},{"$f":"AVERAGE(G4,I4,K4,M4)","v":-23.63},{"$f":"AVERAGE(H4,J4,L4,N4)","v":{"$error":"#DIV/0!"}}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-16.989999999999998,null,null,null,{"$f":"MAX(G5,I5,K5,M5)-MIN(G5,I5,K5,M5)","v":0},{"$f":"MAX(H5,J5,L5,N5)-MIN(H5,J5,L5,N5)","v":0},{"$f":"AVERAGE(G5,I5,K5,M5)","v":-16.989999999999998},{"$f":"AVERAGE(H5,J5,L5,N5)","v":{"$error":"#DIV/0!"}}]
[null,null,571,"AWGN",0,"1% Pmd",null,null,null,null,-20.57,null,null,null,0,0,-20.57,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-13.87,null,null,null,0,0,-13.87,{"$error":"#DIV/0!"}]
[null,null,139,"AWGN",0,"1% Pmd",null,null,null,null,-14.33,null,null,null,0,0,-14.33,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-6.22,null,null,null,0,0,-6.22,{"$error":"#DIV/0!"}]
[null,"B4",1151,"AWGN",0,"1% Pmd",null,null,null,null,-27.87,null,null,null,0,0,-27.87,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-20,null,null,null,0,0,-20,{"$error":"#DIV/0!"}]
[null,null,571,"AWGN",0,"1% Pmd",null,null,null,null,-24.87,null,null,null,0,0,-24.87,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-16.829999999999998,null,null,null,0,0,-16.829999999999998,{"$error":"#DIV/0!"}]
[null,null,139,"AWGN",0,"1% Pmd",null,null,null,null,-18.66,null,null,null,0,0,-18.66,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-9.77,null,null,null,0,0,-9.77,{"$error":"#DIV/0!"}]
[null,"C2",1151,"AWGN",0,"1% Pmd",null,null,null,null,-23.61,null,null,null,0,0,-23.61,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-16.95,null,null,null,0,0,-16.95,{"$error":"#DIV/0!"}]
[null,null,571,"AWGN",0,"1% Pmd",null,null,null,null,-20.58,null,null,null,0,0,-20.58,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-13.76,null,null,null,0,0,-13.76,{"$error":"#DIV/0!"}]
[null,null,139,"AWGN",0,"1% Pmd",null,null,null,null,-14.31,null,null,null,0,0,-14.31,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-6.32,null,null,null,0,0,-6.32,{"$error":"#DIV/0!"}]
["480kHz","A2",571,"AWGN",0,"1% Pmd",null,null,null,null,-20.58,null,null,null,0,0,-20.58,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-13.99,null,null,null,0,0,-13.99,{"$error":"#DIV/0!"}]
[null,null,139,"AWGN",0,"1% Pmd",null,null,null,null,-14.27,null,null,null,0,0,-14.27,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-6.72,null,null,null,0,0,-6.72,{"$error":"#DIV/0!"}]
[null,"B4",571,"AWGN",0,"1% Pmd",null,null,null,null,-24.83,null,null,null,0,0,-24.83,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-18.2,null,null,null,0,0,-18.2,{"$error":"#DIV/0!"}]
[null,null,139,"AWGN",0,"1% Pmd",null,null,null,null,-18.66,null,null,null,0,0,-18.66,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-11.39,null,null,null,0,0,-11.39,{"$error":"#DIV/0!"}]
[null,"C2",571,"AWGN",0,"1% Pmd",null,null,null,null,-20.52,null,null,null,0,0,-20.52,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-14.04,null,null,null,0,0,-14.04,{"$error":"#DIV/0!"}]
[null,null,139,"AWGN",0,"1% Pmd",null,null,null,null,-14.31,null,null,null,0,0,-14.31,{"$error":"#DIV/0!"}]
[null,null,null,"TDLA10-650","7100Hz","1% Pmd",null,null,null,null,-6.75,null,null,null,0,0,-6.75,{"$error":"#DIV/0!"}]