{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Parameters","PUSCH 1T2R"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #109",null,null,null,null,null,null,null,"R4-2320217"]
[null,"Chicago, USA, November 13 – November 17, 2023"]
[]
[null,"Source: Huawei, HiSilicon, Nokia, Nokia Shanghai Bell, Ericsson, Samsung, NTT Docomo, Xiaomi, ZTE"]
[null,"Title: Simulation summary for 256 QAM UL BS Demodulation"]
[null,"Agenda: 8.6.4.1"]
[null,"Document for: Information"]
[null,"Notes: Impairment results include impact or Tx EVM and Rx Phase Noise"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUSCH 1T2R","index":2,"n_rows":18,"n_cols":27,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,11,0,12],[0,0,1,6],[0,7,1,7],[0,8,1,8],[0,9,0,10],[2,0,17,0],[2,1,17,1],[2,2,9,2],[2,3,3,3],[4,3,5,3],[6,3,7,3],[8,3,9,3],[10,2,17,2],[10,3,11,3],[12,3,13,3],[14,3,15,3],[16,3,17,3],[0,13,0,14],[0,15,0,16],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,19,0,20],[0,17,0,18]]}
["  FR2-1 PUSCH 1T2R",null,null,null,null,null,null,"38.104 req","38.141 req","Ericsson",null,"Huawei",null,"Samsung",null,"NTT Docomo",null,"Xiaomi",null,"ZTE",null,"Nokia",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["CP-OFDM","Mapping Type B","PT-RS Enabled","60kHz, 50MHz","MCS20","TDLD30-35","DMRS 1+1",{"$f":"DerivingPerfReq(J3:W3)","v":19.899999999999999},{"$f":"IF(H3>-100,H3+0.6,H3)","v":20.5},17.09,19.79,16.8,19.399999999999999,null,null,null,null,16.352158227769849,null,16.8,null,16.48,20.37,{"$f":"MAX(J3,L3,N3,P3,V3,R3,T3)-MIN(J3,L3,N3,P3,V3,R3,T3)","v":0.73784177223015135},0.97000000000000242,{"$f":"AVERAGE(J3,L3,N3,P3,V3,R3,T3)","v":16.704431645553971},19.853333333333335]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",20.100000000000001,20.700000000000003,17.329999999999998,19.829999999999998,17.100000000000001,19.899999999999999,null,null,null,null,16.309107189735503,null,16.600000000000001,null,16.579999999999998,20.450000000000003,1.0208928102644954,0.62000000000000455,16.783821437947104,20.059999999999999]
[null,null,null,"120kHz, 50MHz","MCS20","TDLD30-35","DMRS 1+1",19.600000000000001,20.200000000000003,17.12,19.86,16.2,18.7,null,null,null,null,16.370426024175991,null,17.100000000000001,null,16.52,20.360000000000003,0.92000000000000171,1.6600000000000037,16.662085204835201,19.64]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",20,20.6,17.55,20.05,16.600000000000001,19.3,null,null,null,null,16.50807720323672,null,16.899999999999999,null,16.87,20.75,1.0419227967632807,1.4499999999999993,16.885615440647349,20.033333333333335]
[null,null,null,"120kHz, 100MHz","MCS20","TDLD30-35","DMRS 1+1",19.7,20.3,17.22,19.829999999999998,16.100000000000001,18.8,null,null,null,null,16.061215440745041,null,17,null,16.59,20.490000000000002,1.1587845592549577,1.6900000000000013,16.594243088149007,19.706666666666667]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",19.899999999999999,20.5,17.48,19.98,16.399999999999999,19.2,null,null,null,null,15.942025922610036,null,16.8,null,16.760000000000002,20.66,1.5379740773899648,1.4600000000000009,16.676405184522004,19.946666666666669]
[null,null,null,"120kHz, 200MHz","MCS20","TDLD30-35","DMRS 1+1",19.8,20.400000000000002,17.21,19.79,16.2,19,null,null,null,null,16.021860939084362,null,17,null,16.579999999999998,20.51,1.1881390609156384,1.5100000000000016,16.602372187816872,19.766666666666666]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",20,20.6,17.489999999999998,19.989999999999998,16.399999999999999,19.399999999999999,null,null,null,null,15.882985256331157,null,16.899999999999999,null,16.72,20.71,1.6070147436688416,1.3100000000000023,16.67859705126623,20.033333333333335]
[null,null,"PT-RS Disabled","60kHz, 50MHz","MCS20","TDLD30-35","DMRS 1+1",{"$f":"DerivingPerfReq(J11:W11)","v":19.2},{"$f":"IF(H11>-100,H11+0.6,H11)","v":19.8},16.45,19.36,16.2,18.7,null,null,null,null,15.520011384045983,null,15.9,null,15.73,19.66,{"$f":"MAX(J11,L11,N11,P11,V11,R11,T11)-MIN(J11,L11,N11,P11,V11,R11,T11)","v":0.9299886159540165},{"$f":"MAX(K11,M11,O11,Q11,W11,S11,U11)-MIN(K11,M11,O11,Q11,W11,S11,U11)","v":0.96000000000000085},{"$f":"AVERAGE(J11,L11,N11,P11,V11,R11,T11)","v":15.960002276809197},{"$f":"AVERAGE(K11,M11,O11,Q11,W11,S11,U11)","v":19.239999999999998}]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",19.600000000000001,20.200000000000003,16.68,19.329999999999998,16.510000000000002,19.2,null,null,null,null,15.546186668038782,null,15.6,null,15.88,20.260000000000002,{"$f":"MAX(J12,L12,N12,P12,V12,R12,T12)-MIN(J12,L12,N12,P12,V12,R12,T12)","v":1.1338133319612176},1.0600000000000023,{"$f":"AVERAGE(J12,L12,N12,P12,V12,R12,T12)","v":16.043237333607756},19.596666666666668]
[null,null,null,"120kHz, 50MHz","MCS20","TDLD30-35","DMRS 1+1",18.899999999999999,19.5,16.5,19.18,15.5,18,null,null,null,null,15.275906016191573,null,16.2,null,15.67,19.490000000000002,1.2240939838084266,1.490000000000002,15.829181203238315,18.89]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",{"$f":"DerivingPerfReq(J14:W14)","v":19.5},20.100000000000001,16.84,19.829999999999998,15.89,18.5,null,null,null,null,15.575039487686277,null,15.9,null,16.010000000000002,20.150000000000002,1.2649605123137224,1.6500000000000021,16.043007897537258,19.493333333333336]
[null,null,null,"120kHz, 100MHz","MCS20","TDLD30-35","DMRS 1+1",19,19.600000000000001,16.579999999999998,19.14,15.5,18.100000000000001,null,null,null,null,15.275906016191573,null,16.3,null,15.8,19.760000000000002,1.3040939838084249,1.6600000000000001,15.891181203238313,19]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",19.5,20.100000000000001,16.78,19.75,15.8,18.399999999999999,null,null,null,null,15.206397178342998,null,16,null,15.99,20.220000000000002,1.573602821657003,1.8200000000000038,15.955279435668597,19.456666666666667]
[null,null,null,"120kHz, 200MHz","MCS20","TDLD30-35","DMRS 1+1",19.2,19.8,16.579999999999998,19.559999999999999,15.5,18.2,null,null,null,null,15.319862512648045,null,16.3,null,15.82,19.89,1.2601374873519529,1.6900000000000013,15.903972502529609,19.216666666666665]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",19.600000000000001,20.200000000000003,16.79,19.75,15.78,18.600000000000001,null,null,null,null,15.261807968328419,null,15.9,null,16.010000000000002,20.53,1.5281920316715798,1.9299999999999997,15.948361593665684,19.626666666666669]