{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Cover","Parameters","PRACH FR1 1T2R","PRACH FR2-1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #110bis",null,null,null,null,null,null,null,"R4-2404388"]
[null,"Changsha, China, April 15-19, 2024"]
[]
[null,"Source: China Telecom"]
[null,"Title: Summary of simulation results for Rel-18 NR coverage enhancements BS demodulation requirements"]
[null,"Agenda: 6.17.2"]
[]
[null,"Reference: R4-2402866 WF on NR_cov_enh2_demod, China Telecom"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PRACH FR1 1T2R","index":2,"n_rows":14,"n_cols":24,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,20,0,21],[0,22,0,23],[0,0,1,1],[0,2,1,2],[0,3,1,3],[0,8,0,9],[0,10,0,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,6,0,7],[10,0,13,0],[10,1,11,1],[12,1,13,1],[0,4,1,4],[0,5,1,5],[6,0,9,0],[6,1,7,1],[8,1,9,1],[2,0,5,0],[2,1,3,1],[4,1,5,1]]}
[" PRACH FR1 1T2R",null,"Propagation condition","Frequency offset (Hz)","38.104 req","38.141 req","Ericsson (R4-2405551)",null,"Huawei (R4-2405124)",null,"ZTE (R4-2405201)",null,"Samsung (R4- 2405862)",null,"Nokia",null,"Company 6",null,"Company 7",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format A2","15kHz","AWGN",0,{"$f":"DerivingPerfReq(G3:T3)","v":-100},{"$f":"IF(E3>-100,E3+0.3,E3)","v":-100},-17.399999999999999,null,-19.100000000000001,null,-18.5,null,-16.850000000000001,null,null,null,null,null,null,null,{"$f":"MAX(G3,I3,K3,M3,O3,Q3,S3)-MIN(G3,I3,K3,M3,O3,Q3,S3)","v":2.25},{"$f":"MAX(H3,J3,L3,N3,P3,R3,T3)-MIN(H3,J3,L3,N3,P3,R3,T3)","v":0},{"$f":"AVERAGE(G3,I3,K3,M3,O3,Q3,S3)","v":-17.962499999999999},{"$f":"AVERAGE(H3,J3,L3,N3,P3,R3,T3)","v":{"$error":"#DIV/0!"}}]
[null,null,"TDLC300-100 Low",400,-100,{"$f":"IF(E4>-100,E4+0.6,E4)","v":-100},-11.3,null,-11.6,null,-11.1,null,-10.54,null,null,null,null,null,null,null,1.0600000000000005,0,-11.135,{"$error":"#DIV/0!"}]
[null,"30kHz","AWGN",0,-100,{"$f":"IF(E5>-100,E5+0.3,E5)","v":-100},-17.5,null,-19.2,null,-18.5,null,-16.78,null,null,null,null,null,null,null,2.4199999999999982,0,-17.995000000000001,{"$error":"#DIV/0!"}]
[null,null,"TDLC300-100 Low",400,-100,{"$f":"IF(E6>-100,E6+0.6,E6)","v":-100},-11.4,null,-11.7,null,-12.9,null,-12.11,null,null,null,null,null,null,null,1.5,0,-12.0275,{"$error":"#DIV/0!"}]
["Format B4","15kHz","AWGN",0,-100,{"$f":"IF(E7>-100,E7+0.3,E7)","v":-100},null,null,-20.100000000000001,null,-21.7,null,-21.62,null,null,null,null,null,null,null,1.5999999999999979,0,-21.14,{"$error":"#DIV/0!"}]
[null,null,"TDLC300-100 Low",400,-100,{"$f":"IF(E8>-100,E8+0.6,E8)","v":-100},-15.7,null,-14.8,null,-13,null,-15.32,null,null,null,null,null,null,null,2.6999999999999993,0,-14.705,{"$error":"#DIV/0!"}]
[null,"30kHz","AWGN",0,-100,{"$f":"IF(E9>-100,E9+0.3,E9)","v":-100},null,null,-20.6,null,-21.7,null,-21.43,null,null,null,null,null,null,null,1.0999999999999979,0,-21.243333333333332,{"$error":"#DIV/0!"}]
[null,null,"TDLC300-100 Low",400,-100,{"$f":"IF(E10>-100,E10+0.6,E10)","v":-100},-16.2,null,-15.2,null,-17.100000000000001,null,-16.579999999999998,null,null,null,null,null,null,null,1.9000000000000021,0,-16.27,{"$error":"#DIV/0!"}]
["Format C2","15kHz","AWGN",0,-100,{"$f":"IF(E11>-100,E11+0.3,E11)","v":-100},null,null,-19.100000000000001,null,-18.600000000000001,null,-16.8,null,null,null,null,null,null,null,2.3000000000000007,0,-18.166666666666668,{"$error":"#DIV/0!"}]
[null,null,"TDLC300-100 Low",400,-100,{"$f":"IF(E12>-100,E12+0.6,E12)","v":-100},-11.6,null,-11.3,null,-11.2,null,-10.67,null,null,null,null,null,null,null,0.92999999999999972,0,-11.192499999999999,{"$error":"#DIV/0!"}]
[null,"30kHz","AWGN",0,-100,{"$f":"IF(E13>-100,E13+0.3,E13)","v":-100},null,null,-19.3,null,-18.600000000000001,null,-16.690000000000001,null,null,null,null,null,null,null,2.6099999999999994,0,-18.196666666666669,{"$error":"#DIV/0!"}]
[null,null,"TDLC300-100 Low",400,-100,{"$f":"IF(E14>-100,E14+0.6,E14)","v":-100},-11.3,null,-11.8,null,-12.7,null,-12.3,null,null,null,null,null,null,null,1.3999999999999986,0,-12.024999999999999,{"$error":"#DIV/0!"}]

{"sheet":"PRACH FR2-1","index":3,"n_rows":14,"n_cols":24,"rows_kept":14,"cut":false,"hidden":false,"merged":[[2,0,5,0],[2,1,3,1],[4,1,5,1],[10,0,13,0],[10,1,11,1],[12,1,13,1],[6,0,9,0],[6,1,7,1],[8,1,9,1],[0,0,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,0,7],[0,20,0,21],[0,22,0,23],[0,8,0,9],[0,10,0,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19]]}
[" PRACH FR2-1 1T2R",null,"Propagation condition","Frequency offset (Hz)","38.104 req","38.141 req","Nokia (R4-2400251)",null,"Ericsson (R4-2405551)",null,"Huawei (R4-2405124)",null,"ZTE (R4-2405201)",null,"Samsung (R4- 2405862)",null,"Company 6",null,"Company 7",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format A2","60kHz","AWGN",0,{"$f":"DerivingPerfReq(G3:T3)","v":-100},{"$f":"IF(E3>-100,E3+0.3,E3)","v":-100},-18.7,null,-17.899999999999999,null,-18.899999999999999,null,-17,null,-16.649999999999999,null,null,null,null,null,{"$f":"MAX(G3,I3,K3,M3,O3,Q3,S3)-MIN(G3,I3,K3,M3,O3,Q3,S3)","v":2.25},{"$f":"MAX(H3,J3,L3,N3,P3,R3,T3)-MIN(H3,J3,L3,N3,P3,R3,T3)","v":0},{"$f":"AVERAGE(G3,I3,K3,M3,O3,Q3,S3)","v":-17.830000000000002},{"$f":"AVERAGE(H3,J3,L3,N3,P3,R3,T3)","v":{"$error":"#DIV/0!"}}]
[null,null,"TDLA30-300 Low",4000,-100,{"$f":"IF(E4>-100,E4+0.6,E4)","v":-100},-11.1,null,-10.3,null,-9.9,null,-10.5,null,-10.88,null,null,null,null,null,1.1999999999999993,0,-10.536,{"$error":"#DIV/0!"}]
[null,"120kHz","AWGN",0,-100,{"$f":"IF(E5>-100,E5+0.3,E5)","v":-100},-18.8,null,-17.7,null,-18.8,null,-18.600000000000001,null,-16.7,null,null,null,null,null,2.1000000000000014,0,-18.12,{"$error":"#DIV/0!"}]
[null,null,"TDLA30-300 Low",4000,-100,{"$f":"IF(E6>-100,E6+0.6,E6)","v":-100},-12.1,null,-10.6,null,-11.4,null,-11.3,null,-11.81,null,null,null,null,null,1.5,0,-11.442000000000002,{"$error":"#DIV/0!"}]
["Format B4","60kHz","AWGN",0,-100,{"$f":"IF(E7>-100,E7+0.3,E7)","v":-100},-23.5,null,-22.2,null,-20,null,-21.7,null,-20.9,null,null,null,null,null,3.5,0,-21.660000000000004,{"$error":"#DIV/0!"}]
[null,null,"TDLA30-300 Low",4000,-100,{"$f":"IF(E8>-100,E8+0.6,E8)","v":-100},-4.8,null,null,null,-12.9,null,-11.1,null,-13.76,null,null,null,null,null,8.9600000000000009,0,-10.639999999999999,{"$error":"#DIV/0!"}]
[null,"120kHz","AWGN",0,-100,{"$f":"IF(E9>-100,E9+0.3,E9)","v":-100},-23.5,null,-22.2,null,-19.7,null,-21.7,null,-20.9,null,null,null,null,null,3.8000000000000007,0,-21.6,{"$error":"#DIV/0!"}]
[null,null,"TDLA30-300 Low",4000,-100,{"$f":"IF(E10>-100,E10+0.6,E10)","v":-100},-14.8,null,-12.8,null,-14.7,null,-13.8,null,-15.45,null,null,null,null,null,2.6499999999999986,0,-14.309999999999999,{"$error":"#DIV/0!"}]
["Format C2","60kHz","AWGN",0,-100,{"$f":"IF(E11>-100,E11+0.3,E11)","v":-100},-18.7,null,-17.8,null,-19.100000000000001,null,-17,null,-16.64,null,null,null,null,null,2.4600000000000009,0,-17.847999999999999,{"$error":"#DIV/0!"}]
[null,null,"TDLA30-300 Low",4000,-100,{"$f":"IF(E12>-100,E12+0.6,E12)","v":-100},-11.4,null,-10.6,null,-10.1,null,-10.6,null,-10.92,null,null,null,null,null,1.3000000000000007,0,-10.724,{"$error":"#DIV/0!"}]
[null,"120kHz","AWGN",0,-100,{"$f":"IF(E13>-100,E13+0.3,E13)","v":-100},-18.8,null,-17.7,null,-18.899999999999999,null,-18.600000000000001,null,-16.61,null,null,null,null,null,2.2899999999999991,0,-18.122,{"$error":"#DIV/0!"}]
[null,null,"TDLA30-300 Low",4000,-100,{"$f":"IF(E14>-100,E14+0.6,E14)","v":-100},-12.3,null,-10.9,null,-11.2,null,-11.3,null,-11.69,null,null,null,null,null,1.4000000000000004,0,-11.478,{"$error":"#DIV/0!"}]