**3GPP TSG-RAN WG4 Meeting #** **94-e-Bis R4-2005319**

**Electronic Meeting, 20 – 30 Apr., 2020**

**Agenda item:** 6.5.3.2

**Source:** Huawei, HiSilicon

**Title:** TP to TS 38.174 on random access requirement for IAB-MT

**Document for:** Approval

# Introduction

In RAN4#93 meeting, it was agreed reuse the random access requirements in TS 38.133 to IAB MT. The text proposal on random access requirement for IAB MT to TS 37.174 [1] is presented in this paper.

# Text proposal

Text proposal to TS 37.174

**<START OF TP>**

12.1.1.2 Random access

The requirements in clause 6.2.2 in TS 38.133 V16.3.0 [TBD] apply for IAB-MT.

*Editor’s note: The CR can be modified later to align the accuracy requirements for absolute power applied to the first preamble and the relative power applied to the additional preamble with RF’s conclusion.*

**<END OF TP>**

# Reference

 [1] TS 37.174