**3GPP TSG-RAN WG4 Meeting #96-e R4-2011757**

Electronic Meeting, August 17th – 28th, 2020

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v11.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **TS38.101-3** | **CR** | **0306** | **rev** | **1** | **Current version:** | **15.10.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR for missing IMD MSD in 38.101-3 for DC\_1A-41A\_n78A, DC\_7A-28A\_n78A | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Qualcomm Incorporated | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_newRAT-Core | | | | |  | | ***Date:*** | | 2020-08-24 |
|  |  | | | |  | | |  | |  |
| ***Category:*** | **F** |  | | | | | | ***Release:*** | | Rel-15 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Missing IMD MSD for various interband ENDC band combinations | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | IMD MSD must be added to the following interband ENDC band combinations:   1. DC\_1A-41A\_n78A is missing IMD4 MSD = 8.7dB for victim B1 like DC\_1A-7A\_n78A. 2. DC\_7A-28A\_n78A needs IMD2 MSD = 28.8dB for victim B28 like DC\_7A\_n28A-n78A. IMD2 MSD needs to increase from 8.3dB to 28.8dB. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | UE cannot meet REFSENS for interband ENDC combinations | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 7.3B.2.3.5.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | |  | | | |
| ***Other specs*** | |  | **X** | Other core specifications | | |  | | | |
| ***affected:*** | | **x** |  | Test specifications | | | 38.521-1 | | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | |  | | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |

< start of changes >

###### 7.3B.2.3.5.2 MSD test points for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 involving three bands

Table 7.3B.2.3.5.2-0: MSD test points for Pcell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA/NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_66A\_(n)71AA | 66 | 1750 | 5 | 25 | 2150 | 5 | IMD4 |
| n71 | 678 | 10 | 10 (RBstart =0) | 632 | N/A | N/A |

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_1A-3A\_n28A | 1 | 1975 | 5 | 25 | 2165 | N/A | N/A |
| n28 | 710.5 | 5 | 25 | 765.5 | N/A | N/A |
| 3 | 1723.5 | 5 | 25 | 1818.5 | 4.0 | IMD5 |
| DC\_1A-3A\_n28A | 3 | 1780 | 5 | 25 | 1875 | N/A | N/A |
| n28 | 710.5 | 5 | 25 | 765.5 | N/A | N/A |
| 1 | 1949 | 5 | 25 | 2139 | 11.0 | IMD4 |
| DC\_1A-7A\_n28A | 1 | 1935 | 5 | 25 | 2125 | N/A | N/A |
| n28 | 718 | 5 | 25 | 773 | N/A | N/A |
| 7 | 2533 | 10 | 50 | 2653 | 30.0 | IMD2 |
| DC\_1A-3A\_n77A | 1 | 1950 | 5 | 25 | 2140 | N/A | N/A |
| 3 | 1712.5 | 5 | 25 | 1807.5 | 31.5 | IMD2 |
| n77 | 3757.5 | 10 | 50 | 3757.5 | N/A | N/A |
| 1 | 1950 | 5 | 25 | 2140 | N/A | N/A |
| 3 | 1775 | 5 | 25 | 1870 | 8.5 | IMD4 |
| n77 | 3980 | 10 | 50 | 3980 | N/A | N/A |
| 1 | 1950 | 5 | 25 | 2140 | 31.0 | IMD2 |
| 3 | 1775 | 5 | 25 | 1870 | N/A | N/A |
| n77 | 3915 | 10 | 50 | 3915 | N/A | N/A |
| DC\_1A-3A\_n78A  DC\_1A-3C\_n78A | 1 | 1950 | 5 | 25 | 2140 | N/A | N/A |
| 3 | 1712.5 | 5 | 25 | 1807.5 | 31.2 | IMD2 |
| n78 | 3757.5 | 10 | 50 | 3757.5 | N/A | N/A |
| 1 | 1935 | 5 | 25 | 2125 | 2.8 | IMD5 |
| 3 | 1775 | 5 | 25 | 1870 | N/A | N/A |
| n78 | 3725 | 10 | 50 | 3725 | N/A | N/A |
| DC\_1A-5A\_n78A | 1 | 1932 | 5 | 25 | 2122 | 18.1 | IMD3 |
| 5 | 829 | 5 | 25 | 874 | N/A | N/A |
| n78 | 3780 | 10 | 50 | 3780 | N/A | N/A |
| 1 | 1975 | 5 | 25 | 2165 | N/A | N/A |
| 5 | 840 | 5 | 25 | 885 | 3.1 | IMD5 |
| n78 | 3405 | 10 | 50 | 3405 | N/A | N/A |
| DC\_1A-7A\_n78A | 1 | 1977.5 | 5 | 25 | 2167.5 | N/A | N/A |
| 7 | 2507.5 | 5 | 25 | 2627.5 | 9.1 | IMD4 |
| n78 | 3305 | 10 | 50 | 3305 | N/A | N/A |
| 1 | 1950 | 5 | 25 | 2140 | 8.7 | IMD4 |
| 7 | 2510 | 10 | 50 | 2630 | N/A | N/A |
| n78 | 3580 | 10 | 50 | 3580 | N/A | N/A |
| DC\_1A-3A\_n79A | 1 | 1950 | 5 | 25 | 2140 | 3.6 | IMD5 |
| 3 | 1750 | 5 | 25 | 1845 | N/A | N/A |
| n79 | 4860 | 40 | 216 | 4860 | N/A | N/A |
| DC\_1A-18A\_n77A | 1 | 1930 | 5 | 25 | 2120 | 16.4 | IMD3 |
| 18 | 825 | 5 | 25 | 870 | N/A | N/A |
| n77 | 3770 | 10 | 50 | 3770 | N/A | N/A |
| DC\_1A-18A\_n78A | 1 | 1930 | 5 | 25 | 2120 | 16.4 | IMD3 |
| 18 | 819 | 5 | 25 | 864 | N/A | N/A |
| n78 | 3758 | 10 | 50 | 3758 | N/A | N/A |
| DC\_1A-18A\_n79A | 1 | 1935 | 5 | 25 | 2125 | N/A | N/A |
| 18 | 822.5 | 5 | 25 | 867.5 | 18.3 | IMD3 |
| n79 | 4737.5 | 40 | 216 | 4737.5 | N/A | N/A |
| 1 | 1930 | 5 | 25 | 2120 | N/A | N/A |
| 18 | 820 | 5 | 25 | 865 | 8.9 | IMD4 |
| n79 | 4925 | 40 | 216 | 4925 | N/A | N/A |
| 1 | 1935 | 5 | 25 | 2125 | 8.1 | IMD4 |
| 18 | 822.5 | 5 | 25 | 867.5 | N/A | N/A |
| n79 | 4592.5 | 40 | 216 | 4592.5 | N/A | N/A |
| DC\_1A-19A\_n77A  DC\_1A-19A\_n78A | 1 | 1940 | 5 | 25 | 2130 | 17.8 | IMD3 |
| 19 | 832.5 | 5 | 25 | 877.5 | N/A | N/A |
| n77, n78 | 3795 | 10 | 50 | 3795 | N/A | N/A |
| DC\_1A-19A\_n79A | 1 | 1950 | 5 | 25 | 2140 | N/A | N/A |
| 19 | 837.5 | 5 | 25 | 882.5 | 18.3 | IMD3 |
| n79 | 4782.5 | 40 | 216 | 4782.5 | N/A | N/A |
| 1 | 1950 | 5 | 25 | 2140 | 8.1 | IMD4 |
| 19 | 837.5 | 5 | 25 | 882.5 | N/A | N/A |
| n79 | 4652.5 | 40 | 216 | 4652.5 | N/A | N/A |
| DC\_1A-20A\_n78A | 1 | 1930 | 5 | 25 | 2120 | 20.3 | IMD3 |
| 20 | 835 | 5 | 25 | 794 | N/A | N/A |
| n78 | 3790 | 10 | 50 | 3790 | N/A | N/A |
| DC\_1A-20A\_n78A | 1 | 1950 | 5 | 25 | 2140 | N/A | N/A |
| 20 | 851 | 5 | 25 | 810 | 3.0 | IMD5 |
| n78 | 3330 | 10 | 50 | 3330 | N/A | N/A |
| DC\_1A-21A\_n77A  DC\_1A-21A\_n78A | 1 | 1964.6 | 5 | 25 | 2154.6 | 30.6 | IMD2 |
| 21 | 1450.4 | 5 | 25 | 1498.4 | N/A | N/A |
| n77, n78 | 3605 | 10 | 50 | 3605 | N/A | N/A |
| 1 | 1950 | 5 | 25 | 2140 | N/A | N/A |
| 21 | 1452 | 5 | 25 | 1500 | 2.9 | IMD5 |
| n77, n78 | 3675 | 10 | 50 | 3675 | N/A | N/A |
| DC\_1A-28A\_n77A | 1 | 1960 | 5 | 25 | 2150 | 15.8 | IMD3 |
| 28 | 740 | 5 | 25 | 795 | N/A | N/A |
| n77 | 3630 | 10 | 50 | 3630 | N/A | N/A |
| DC\_1A-28A\_n77A | 1 | 1960 | 5 | 25 | 2150 | N/A | N/A |
| 28 | 725 | 5 | 25 | 780 | 4.3 | IMD5 |
| n77 | 3330 | 10 | 50 | 3330 | N/A | N/A |
| DC\_1A-28A\_n78A | 1 | 1960 | 5 | 25 | 2150 | 15.7 | IMD3 |
| 28 | 740 | 5 | 25 | 795 | N/A | N/A |
| n78 | 3630 | 10 | 50 | 3630 | N/A | N/A |
| DC\_1A-28A\_n78A | 1 | 1970 | 5 | 25 | 2160 | N/A | N/A |
| 28 | 739 | 5 | 25 | 794 | 4.2 | IMD5 |
| n78 | 3352 | 10 | 50 | 3352 | N/A | N/A |
| DC\_1A\_n28A-n78A | 1 | 1950 | 5 | 25 | 2140 | N/A | N/A |
| n28 | 733 | 5 | 25 | 788 | N/A | N/A |
| n78 | 3416 | 10 | 50 | 3416 | 15.7 | IMD3 |
| 1 | 1950 | 5 | 25 | 2140 | N/A | N/A |
| n78 | 3320 | 10 | 50 | 3320 | N/A | N/A |
| n28 | 735 | 5 | 25 | 790 | 3.3 | IMD5 |
| DC\_1A-28A\_n79A | 1 | 1930 | 5 | 25 | 2120 | N/A | N/A |
| 28 | 733 | 5 | 25 | 788 | 15.2 | IMD3 |
| n79 | 4648 | 40 | 216 | 4648 | N/A | N/A |
| 1 | 1925 | 5 | 25 | 2115 | N/A | N/A |
| 28 | 740 | 5 | 25 | 795 | 10.0 | IMD4 |
| n79 | 4980 | 40 | 216 | 4980 | N/A | N/A |
| 1 | 1977.5 | 5 | 25 | 2167.5 | 1.2 | IMD4 |
| 28 | 745.5 | 5 | 25 | 800.5 | N/A | N/A |
| n79 | 4420 | 40 | 216 | 4420 | N/A | N/A |
| 1 | 1935 | 5 | 25 | 2125 | 4.5 | IMD5 |
| 28 | 718 | 5 | 25 | 773 | N/A | N/A |
| n79 | 4807 | 40 | 216 | 4807 | N/A | N/A |
| DC\_1A-41A\_n77A | 1 | 1970 | 5 | 25 | 2160 | N/A | N/A |
| n77 | 3400 | 10 | 50 | 3400 | N/A |
| 41 | 2510 | 5 | 25 | 2510 | 11.0 | IMD4 |
| 1 | 1930 | 5 | 25 | 2120 | N/A | N/A |
| n77 | 4150 | 10 | 50 | 4150 | N/A |
| 41 | 2510 | 5 | 25 | 2510 | 3.6 | IMD5 |
| DC\_1A-41A\_n78A | 1 | 1975 | 5 | 25 | 2165 | N/A | N/A |
| 41 |  | 5 | 25 | 2515 | 12 | IMD4 |
| n78 | 3410 | 10 | 50 | 3410 | N/A | N/A |
| DC\_1A-41A\_n78A | 1 | 1955 | 5 | 25 | 2145 | 8.7 | IMD4 |
| 41 | 2507.5 | 10 | 50 | 2507.5 | N/A | N/A |
| n78 | 3580 | 10 | 50 | 3580 | N/A | N/A |
| DC\_1A-41A\_n79A | 1 | 1970 | 5 | 25 | 2160 | N/A | N/A |
| n79 | 4500 | 40 | 216 | 4500 | N/A |
| 41 | 2530 | 5 | 25 | 2530 | 29.4 | IMD2 |
| DC\_1A-42A\_n79A | 1 | 1977.5 | 5 | 25 | 2167.5 | N/A | N/A |
| n79 | 4420 | 40 | 216 | 4420 | N/A | N/A |
| 42 | 3490 | 5 | 25 | 3490 | 4.8 | IMD5 |
| 42 | 3402.5 | 5 | 25 | 3402.5 | N/A | N/A |
| n79 | 4640 | 40 | 216 | 4640 | N/A | N/A |
| 1 | 1975 | 5 | 25 | 2165 | 15.5 | IMD3 |
| 42 | 3450 | 5 | 25 | 3450 | N/A | N/A |
| n79 | 4520 | 40 | 216 | 4520 | N/A | N/A |
| 1 | 1950 | 5 | 25 | 2140 | 9.3 | IMD4 |
| DC\_1A\_n78A-n79A | 1 | 1950 | 5 | 25 | 2140 | N/A | N/A |
| n78 | 3410 | 10 | 50 | 3410 | N/A | N/A |
| n79 | 4870 | 40 | 216 | 4870 | 15.9 | IMD3 |
| 1 | 1950 | 5 | 25 | 2140 | N/A | N/A |
| n79 | 4670 | 40 | 216 | 4670 | N/A | N/A |
| n78 | 3490 | 10 | 50 | 3490 | 4.6 | IMD5 |
| DC\_3A-7A\_n28A | 3 | 1712.5 | 5 | 25 | 1807.5 | N/A | N/A |
| n28 | 743 | 5 | 25 | 798 | N/A | N/A |
| 7 | 2562 | 10 | 50 | 2682 | 16.9 | IMD3 |
| 7 | 2543 | 10 | 50 | 2663 | N/A | N/A |
| n28 | 710.5 | 5 | 25 | 765.5 | N/A | N/A |
| 3 | 1737.5 | 5 | 25 | 1832.5 | 26.0 | IMD2 |
| DC\_3A-7A\_n78A  DC\_3C-7A\_n78A DC\_3C-7C\_n78A | 3 | 1725 | 5 | 25 | 1820 | 17.6 | IMD3 |
| 7 | 2565 | 5 | 25 | 2685 | N/A | N/A |
| n78 | 3310 | 10 | 50 | 3310 | N/A | N/A |
| 3 | 1725 | 5 | 25 | 1820 | 8.6 | IMD4 |
| 7 | 2565 | 5 | 25 | 2685 | N/A | N/A |
| n78 | 3475 | 10 | 50 | 3475 | N/A | N/A |
| DC\_3A-8A\_n78A | 8 | 910 | 5 | 25 | 955 | N/A | N/A |
| n78 | 3640 | 10 | 50 | 3640 | N/A | N/A |
| 3 | 1725 | 5 | 25 | 1820 | 16.5 | IMD3 |
| DC\_3A-19A\_n79A | 3 | 1775 | 5 | 25 | 1870 | N/A | N/A |
| 19 | 840 | 5 | 25 | 885 | 18.5 | IMD3 |
| n79 | 4435 | 40 | 216 | 4435 | N/A | N/A |
| 3 | 1782.5 | 5 | 25 | 1877.5 | 0.2 | IMD4 |
| 19 | 842.5 | 5 | 25 | 887.5 | N/A | N/A |
| n79 | 4420 | 40 | 216 | 4420 | N/A | N/A |
| DC\_3A-20A\_n28A | 20 | 852 | 5 | 25 | 811 | N/A | N/A |
| n28 | 738 | 5 | 25 | 793 | N/A | N/A |
| 3 | 1723 | 5 | 25 | 1818 | 9.4 | IMD4 |
| DC\_3A-20A\_n78A  DC\_3C-20A\_n78A | 3 | 1725 | 5 | 25 | 1820 | 17.3 | IMD3 |
| 20 | 845 | 5 | 25 | 804 | N/A | N/A |
| n78 | 3510 | 10 | 50 | 3510 | N/A | N/A |
| DC\_3A-21A\_n77A  DC\_3A-21A\_n78A | 3 | 1767.5 | 5 | 25 | 1862.5 | N/A | N/A |
| 21 | 1459.5 | 5 | 25 | 1507.5 | 8.8 | IMD4 |
| n77, n78 | 3795 | 10 | 50 | 3795 | N/A | N/A |
| DC\_3A-21A\_n77A | 3 | 1771.6 | 5 | 25 | 1866.6 | 3.4 | IMD5 |
| 21 | 1450.4 | 5 | 25 | 1498.4 | N/A | N/A |
| n77 | 3935 | 10 | 50 | 3935 | N/A | N/A |
| DC\_3A-21A\_n79A | 3 | 1774.2 | 5 | 25 | 1869.2 | 17.8 | IMD3 |
| 21 | 1450.4 | 5 | 25 | 1498.4 | N/A | N/A |
| n79 | 4770 | 40 | 216 | 4770 | N/A | N/A |
| DC\_3A-28A\_n77A | 3 | 1712.5 | 5 | 25 | 1807.5 | N/A | N/A |
| 28 | 715 | 5 | 25 | 770 | 15.3 | IMD3 |
| n77 | 4195 | 10 | 50 | 4195 | N/A | N/A |
| 3 | 1755 | 5 | 25 | 1850 | 17.0 | IMD3 |
| 28 | 735 | 5 | 25 | 790 | N/A | N/A |
| n77 | 3320 | 10 | 50 | 3320 | N/A | N/A |
| DC\_3A-28A\_n78A | 3 | 1775 | 5 | 25 | 1870 | 17.3 | IMD3 |
| 28 | 740 | 5 | 25 | 760 | N/A | N/A |
| n78 | 3350 | 10 | 25 | 3350 | N/A | N/A |
| DC\_3A-28A\_n79A | 3 | 1770 | 5 | 25 | 1865 | N/A | N/A |
| 28 | 725 | 5 | 25 | 780 | 10.3 | IMD4 |
| n79 | 4530 | 40 | 216 | 4530 | N/A | N/A |
| 3 | 1775 | 5 | 25 | 1870 | 5.7 | IMD5 |
| 28 | 725 | 5 | 25 | 780 | N/A | N/A |
| n79 | 4770 | 40 | 216 | 4770 | N/A | N/A |
| DC\_3A\_n28A-n78A | 3 | 1750 | 5 | 25 | 1845 | N/A | N/A |
| n28 | 743 | 5 | 25 | 798 | N/A | N/A |
| n78 | 3764 | 10 | 50 | 3764 | 4.5 | IMD5 |
| DC\_3A-41A\_n78A | 41 | 2620 | 5 | 25 | 2620 | N/A | N/A |
| n78 | 3400 | 10 | 52 | 3400 | N/A | N/A |
| 3 | 1745 | 5 | 25 | 1840 | 16.4 | IMD3 |
| DC\_3A\_n78A-n79A | 3 | 1770 | 5 | 25 | 1865 | N/A | N/A |
| n78 | 3340 | 10 | 50 | 3340 | N/A | N/A |
| n79 | 4910 | 40 | 216 | 4910 | 16.3 | IMD3 |
| 3 | 1770 | 5 | 25 | 1865 | N/A | N/A |
| n79 | 4510 | 40 | 216 | 4510 | N/A | N/A |
| n78 | 3710 | 10 | 50 | 3710 | 4.2 | IMD5 |
| DC\_3A-SUL\_n78A-n82A | 3 | 1775 | 5 | 25 | 1870 | 4 | IMD4 |
| n82 | 840 | 5 | 25 |  | N/A | N/A |
| DC\_3A-21A\_n79A | 3 | 1774.2 | 5 | 25 | 1869.2 | 17.8 | IMD3 |
| 21 | 1450.4 | 5 | 25 | 1498.4 | N/A | N/A |
| n79 | 4770 | 40 | 216 | 4770 | N/A | N/A |
| DC\_5A-7A\_n78A | 5 | 844 | 5 | 25 | 889 | N/A | N/A |
| 7 | 2525 | 5 | 25 | 2645 | 30.1 | IMD2 |
| n78 | 3489 | 10 | 50 | 3489 | N/A | N/A |
| 5 | 834 | 5 | 25 | 879 | 30.2 | IMD2 |
| 7 | 2550 | 5 | 25 | 2670 | N/A | N/A |
| n78 | 3429 | 10 | 50 | 3429 | N/A | N/A |
| 5 | 830 | 5 | 25 | 875 | 3.3 | IMD5 |
| 7 | 2525 | 5 | 25 | 2645 | N/A | N/A |
| n78 | 3350 | 10 | 50 | 3350 | N/A | N/A |
| DC\_5A\_41A\_n78A | 5 | 860 | 5 | 25 | 885 | 30.2 | IMD2 |
| 41 | 2615 | 5 | 25 | 2615 | N/A | N/A |
| n78 | 3500 | 10 | 50 | 3500 | N/A | N/A |
| 5 | 856.5 | 5 | 25 | 881.5 | 3.1 | IMD5 |
| 41 | 2620.5 | 5 | 25 | 2620.5 | N/A | N/A |
| n78 | 3490 | 10 | 50 | 3490 | N/A | N/A |
| DC\_7A-20A\_n28A | 20 | 852 | 5 | 25 | 811 | N/A | N/A |
| n28 | 738 | 5 | 25 | 793 | N/A | N/A |
| 7 | 2550 | 10 | 50 | 2670 | 5.9 | IMD5 |
| DC\_7A-20A\_n78A | 7 | 2560 | 5 | 25 | 2680 | N/A | N/A |
| 20 | 851 | 5 | 25 | 810 | 30.5 | IMD2 |
| n78 | 3370 | 10 | 50 | 3370 | N/A | N/A |
| DC\_7A-20A\_n78A | 7 | 2560 | 5 | 25 | 2680 | N/A | N/A |
| 20 | 851 | 5 | 25 | 810 | 3.0 | IMD5 |
| n78 | 3435 | 10 | 50 | 3435 | N/A | N/A |
| DC\_7A-20A\_n78A | 7 | 2555 | 5 | 25 | 2675 | 30.8 | IMD2 |
| 20 | 845 | 5 | 25 | 804 | N/A | N/A |
| n78 | 3520 | 10 | 50 | 3520 | N/A | N/A |
| DC\_7A-28A\_n78A | 7 | 2567.5 | 5 | 25 | 2687.5 | N/A | N/A |
| 28 | 727.5 | 5 | 25 | 782.5 | 28.8 | IMD2 |
| n78 | 3350 | 10 | 50 | 3350 | N/A | N/A |
| 7 | 2567.5 | 5 | 25 | 2687.5 | N/A | N/A |
| 28 | 727.5 | 5 | 25 | 782.5 | 3.0 | IMD5 |
| n78 | 3460 | 10 | 50 | 3460 | N/A | N/A |
| 7 | 2530 | 5 | 25 | 2650 | 30.5 | IMD2 |
| 28 | 740 | 5 | 25 | 795 | N/A | N/A |
| n78 | 3390 | 10 | 50 | 3390 | N/A | N/A |
| DC\_7A\_n28A-n78A | 7 | 2565 | 5 | 25 | 2685 | N/A | N/A |
| n28 | 745 | 5 | 25 | 800 | N/A | N/A |
| n78 | 3310 | 10 | 50 | 3310 | 29.7 | IMD2 |
| 7 | 2565 | 5 | 25 | 2685 | N/A | N/A |
| n78 | 3365 | 10 | 50 | 3365 | N/A | N/A |
| n28 | 745 | 5 | 25 | 800 | 28.8 | IMD2 |
| DC\_7A-46A\_n78A6 | 7 | N/A | N/A | N/A | N/A | N/A | N/A |
| 46 | N/A | N/A | N/A | N/A | N/A | IMD2, IMD5 |
| n78 | N/A | N/A | N/A | N/A | N/A | N/A |
| DC\_18A-28A\_n77A | 18 | 820 | 5 | 25 | 865 | N/A | N/A |
| 28 | 723 | 5 | 25 | 778 | 4.4 | IMD5 |
| n77 | 4058 | 10 | 50 | 4058 | N/A | N/A |
| DC\_18A-28A\_n77A | 18 | 820 | 5 | 25 | 865 | 3.9 | IMD5 |
| 28 | 723 | 5 | 25 | 778 | N/A | N/A |
| n77 | 3757 | 10 | 50 | 3757 | N/A | N/A |
| DC\_18A-28A\_n78A | 18 | 819 | 5 | 25 | 864 | 3.8 | IMD5 |
| 28 | 723 | 5 | 25 | 778 | N/A | N/A |
| n78 | 3756 | 10 | 50 | 3756 | N/A | N/A |
| DC\_19A-21A\_n77A  DC\_19A-21A\_n78A | 19 | 837.5 | 5 | 25 | 882.5 | 18.7 | IMD3 |
| 21 | 1450.4 | 5 | 25 | 1498.4 | N/A | N/A |
| n77, n78 | 3783.3 | 10 | 50 | 3783.3 | N/A | N/A |
| DC\_19A-21A\_n77A | 19 | 837.5 | 5 | 25 | 882.5 | N/A | N/A |
| 21 | 1454.5 | 5 | 25 | 1502.5 | 9.0 | IMD4 |
| n77 | 4015 | 10 | 50 | 4015 | N/A | N/A |
| DC\_19A-21A\_n79A | 19 | 837.5 | 5 | 25 | 882.2 | N/A | N/A |
| 21 | 1452 | 5 | 25 | 1500 | 3.8 | IMD5 |
| n79 | 4850 | 40 | 216 | 4850 | N/A | N/A |
| DC\_21A-28A\_n77A | 21 | 1452 | 5 | 25 | 1500 | N/A | N/A |
| 28 | 730.5 | 5 | 25 | 785.5 | 16.9 | IMD3 |
| n77 | 3689.5 | 10 | 50 | 3689.5 | N/A | N/A |
| 21 | 1450.5 | 5 | 25 | 1498.5 | 9.9 | IMD4 |
| 28 | 730.5 | 5 | 25 | 785.5 | N/A | N/A |
| n77 | 3690 | 10 | 50 | 3690 | N/A | N/A |
| DC\_21A-28A\_n79A | 21 | 1450 | 5 | 25 | 1498 | 5.2 | IMD5 |
| 28 | 730.5 | 5 | 25 | 785.5 | N/A | N/A |
| n79 | 4420 | 40 | 216 | 4420 | N/A | N/A |
| DC\_28A-42A\_79A | 28 | 730 | 5 | 25 | 785 | N/A | N/A |
| 42 | 3420 | 5 | 25 | 3420 | 15.3 | IMD3 |
| n79 | 4880 | 40 | 216 | 4880 | N/A | N/A |
| 28 | 745 | 5 | 25 | 800 | 16.2 | IMD2 |
| 42 | 3597.5 | 5 | 25 | 3597.5 | N/A | N/A |
| n79 | 4420 | 40 | 216 | 4420 | N/A | N/A |
| DC\_19A\_n78A-n79A | 19 | 835 | 5 | 25 | 880 | N/A | N/A |
| n78 | 3680 | 10 | 50 | 3680 | N/A | N/A |
| n79 | 4515 | 40 | 216 | 4515 | 29.3 | IMD2 |
| 19 | 835 | 5 | 25 | 880 | N/A | N/A |
| n79 | 4550 | 40 | 216 | 4550 | N/A | N/A |
| n78 | 3715 | 10 | 50 | 3715 | 28.8 | IMD2 |
| DC\_20A\_n28A-n78A, DC\_20A\_SUL\_n78A-n83A | 20 | 857 | 5 | 25 | 816 | N/A | N/A |
| n28, n83 | 743 | 5 | 25 | 798 | N/A | N/A |
| n78 | 3314 | 10 | 50 | 3314 | 8.7 | IMD4 |
| 20 | 837 | 5 | 25 | 796 | N/A | N/A |
| n78 | 3310 | 10 | 50 | 3310 | N/A | N/A |
| n28 | 744 | 5 | 25 | 799 | 9.4 | IMD4 |
| DC\_21A\_n78A-n79A | 21 | 1453 | 5 | 25 | 1501 | N/A | N/A |
| n78 | 3420 | 10 | 50 | 3420 | N/A | N/A |
| n79 | 4873 | 40 | 216 | 4873 | 30.1 | IMD2 |
| 21 | 1453 | 5 | 25 | 1501 | N/A | N/A |
| n79 | 4940 | 40 | 216 | 4940 | N/A | N/A |
| n78 | 3487 | 10 | 50 | 3487 | 29.8 | IMD2 |

< end of changes >