{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["Introduction","NR bands","5G NR CADC Configurations","V2X bands","V2X Configurations","Revision History","Assignment template"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":62,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Introduction","index":0,"n_rows":104,"n_cols":8,"rows_kept":104,"cut":false,"hidden":false,"merged":[[82,3,85,7],[94,1,94,7],[95,4,95,5],[96,1,96,2],[97,1,97,7],[98,1,98,7],[87,1,87,7],[88,4,88,5],[89,1,89,2],[90,1,90,7],[91,1,91,7],[61,1,61,7],[66,1,66,7],[67,1,67,7],[76,1,76,7],[81,1,81,7],[45,1,45,7],[49,1,49,7],[50,1,50,7],[55,1,55,7],[56,1,56,7],[22,1,22,7],[30,1,30,7],[35,1,35,7],[40,1,40,7],[41,1,41,7],[17,1,17,7],[18,1,18,7],[19,4,19,5],[20,1,20,2],[21,1,21,7],[7,4,7,5],[8,1,8,2],[9,1,9,7],[10,1,10,7],[13,1,13,7],[0,6,0,7],[2,1,2,7],[3,1,3,7],[4,3,4,7],[6,1,6,7]]}
[null,"3GPP RAN WG5 status of 5G NR bands and V2X bands, and CA, NR-DC, NR SUL, NE-DC, EN-DC and V2X configurations",null,null,null,null,{"$f":"\"PRD21 \"&INDIRECT(\"'Revision History'!\"&\"C2\")","v":"PRD21 v1.5.0"}]
[]
[null,"The purpose of this document is to provide RAN5 status for NR bands, NR band CBW extensions, V2X bands and 5G NR CADC configurations (NR CA, NR-DC, NR SUL, NE-DC, EN-DC and V2X) covered by RAN5 work items. The document also indicates the Work Item code(s) to be used when submitting CRs for NR bands, NR band CBW extensions, V2X bands, and 5G NR CADC configurations depending on the target power class.\n\nThe worksheets \"NR bands\" and \"5G NR CADC Configurations\" include lists showing the current status for RAN5 NR bands, NR band CBW extensions and 5G NR CADC configurations for power class 3 (PC3) and applicable additional power classes (e.g. PC1.5 and PC2). The worksheet “5G NR CADC configurations” refers to the configurations specific to NR CA, NR-DC, NR SUL, NE-DC and EN-DC. The list shows for each NR band, NR band CBW extensions and 5G NR CADC configuration the declared interested operator and the company that have been assigned taking responsibility for adding necessary details to 3GPP RAN5 UE conformance test specifications for PC3. Interested operator for other power classes than PC3 is tracked within the specific work plan of the power class.  The list also shows the Work Item code (s) to be used when submitting CRs for the different NR bands and 5G NR CADC configurations for the different applicable power classes. The status is updated after each RAN5 meeting. \n\nThe NR bands and 5G NR CADC configurations worksheets provides tools to select one or more NR bands/5G NR CADC configurations for the purpose to request assignment as interested operator and/or responsible company of NR bands, NR band CBW extensions and 5G NR CADC configuration(s).\n\nThe worksheets \"V2X bands\" and \"V2X Configurations\" include lists showing the current status for RAN5 5G NR V2X bands and 5G NR V2X configurations.\n\nFor guideline how to use the NR bands and V2X bands, and 5G NR CADC and V2X configurations worksheets see the PRD21 word document."]
[null,"Overall status of RAN5 NR band, NR band CBW extensions and 5G NR CADC configurations"]
[null,"Selected Release Scope","All Releases"]
[]
[null,{"$f":"\"Status of NR Bands and CBW extensions for \"&$C$5&\" in RAN5 scope\"","v":"Status of NR Bands and CBW extensions for All Releases in RAN5 scope"}]
[null,"TS and Source Table","Type of NR band / CBW","Number of \nNR bands / CBW items","Number of completed \nNR bands / CBW items",null,"Number of assigned and ongoing \nNR bands / CBW items\n(not yet completed)","Number of pending \nNR bands / CBW items\n(not assigned)"]
[null,"Overall (All TSs and source tables for the selected release scope):",null,{"$f":"SUM($D$12:$D$16)","v":132},{"$f":"SUM($E$12:$E$16)","v":83},{"$f":"IFERROR(E9/D9,\"-\")","v":0.62878787878787878},{"$f":"SUM($G$12:$G$16)","v":35},{"$f":"D9-E9-G9","v":14}]
[null,"NR Bands"]
[null,"NR FR1 Bands and CBW extensions"]
[null,"38.101-1:Table 5.3.5-1","NR FR1 bands",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=$B12),--(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B12)))","v":75},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B12),--(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B12)))","v":59},{"$f":"IFERROR(E12/D12,\"-\")","v":0.78666666666666663},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Interested Deployer\n(Note 2)]])<>\"\"),--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B12),--(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Interested Deployer\n(Note 2)]])<>\"\"),--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B12)))","v":7},{"$f":"D12-E12-G12","v":9}]
[null,"38.101-1:Table 5.3.5-1 CBW","NR FR1 CBW extension items (adding one or more CBWs to a NR band)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=$B13),--(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B13)))","v":40},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B13),--(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B13)))","v":23},0.57499999999999996,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Interested Deployer\n(Note 2)]])<>\"\"),--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B13),--(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Interested Deployer\n(Note 2)]])<>\"\"),--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B13)))","v":13},4]
[null,"NR FR2 Bands and CBW extensions"]
[null,"38.101-2:Table 5.3.5-1","NR FR2 bands",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=$B15),--(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B15)))","v":17},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B15),--(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B15)))","v":1},{"$f":"IFERROR(E15/D15,\"-\")","v":5.8823529411764705E-2},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Interested Deployer\n(Note 2)]])<>\"\"),--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B15),--(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Interested Deployer\n(Note 2)]])<>\"\"),--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B15)))","v":15},{"$f":"D15-E15-G15","v":1}]
[null,"38.101-2:Table 5.3.5-1 CBW","NR FR2 CBW extension items (adding one or more CBWs to a NR band)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=$B16),--(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B16)))","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B16),--(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B16)))","v":0},"-",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Interested Deployer\n(Note 2)]])<>\"\"),--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B16),--(NRbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(NRbandsTblID[[#All],[Interested Deployer\n(Note 2)]])<>\"\"),--(TRIM(NRbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(NRbandsTblID[[#All],[TS and Source Table]]=Introduction!$B16)))","v":0},0]
[]
[null,{"$f":"\"Status NR CA, NR-DC, NR SUL, NE-DC and EN-DC configurations for \"&$C$5&\" in RAN5 scope\"","v":"Status NR CA, NR-DC, NR SUL, NE-DC and EN-DC configurations for All Releases in RAN5 scope"}]
[null," Each DL-UL-configuration-combination is counted as one configuration, i.e. a DL configuration having N valid UL configurations is counted as N configurations."]
[null,"TS and Source Table","Type of configuration","Number of configurations","Number of completed configurations",null,"Number of assigned and ongoing configurations\n(not yet completed)","Number of pending configurations\n(not assigned)"]
[null,"Overall (All TSs and source tables for the selected release scope):",null,{"$f":"SUM($D$24:$D$81)","v":62308},{"$f":"SUM($E$24:$E$81)","v":871},{"$f":"IFERROR(E21/D21,\"-\")","v":1.3978943313860178E-2},{"$f":"SUM($G$24:$G$81)","v":8800},{"$f":"D21-E21-G21","v":52637}]
[null,"NR CA"]
[null,"NR CA configurations within FR1"]
[null,"38.101-1:Table 5.5A.1-1","NR CA configurations for intra-band contiguous CA",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B24),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B24)))","v":72},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B24),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B24)))","v":14},{"$f":"IFERROR(E24/D24,\"-\")","v":0.19444444444444445},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B24),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B24)))","v":7},{"$f":"D24-E24-G24","v":51}]
[null,"38.101-1:Table 5.5A.2-1","NR CA configurations for intra-band non-contiguous CA",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B25),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B25)))","v":62},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B25),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B25)))","v":4},6.4516129032258063E-2,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B25),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B25)))","v":7},51]
[null,"38.101-1:Table 5.5A.2-2","NR CA configurations for mixed intra-band contiguous and non-contiguous CA",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B26),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B26)))","v":12},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B26),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B26)))","v":0},0,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B26),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B26)))","v":3},9]
[null,"38.101-1:Table 5.5A.3.1-1a-n","NR CA configurations for inter-band CA (two bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[Type of configuration]]=\"NR CA FR1 inter-band (2 bands)\"),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[Type of configuration]]=\"NR CA FR1 inter-band (2 bands)\")))","v":1705},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[Type of configuration]]=\"NR CA FR1 inter-band (2 bands)\"),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[Type of configuration]]=\"NR CA FR1 inter-band (2 bands)\")))","v":134},7.859237536656892E-2,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[Type of configuration]]=\"NR CA FR1 inter-band (2 bands)\"),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[Type of configuration]]=\"NR CA FR1 inter-band (2 bands)\")))","v":266},1305]
[null,"38.101-1:Table 5.5A.3.2-1","NR CA configurations for inter-band CA (three bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B28),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B28)))","v":2668},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B28),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B28)))","v":81},3.0359820089955022E-2,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B28),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B28)))","v":224},2363]
[null,"38.101-1:Table 5.5A.3.3-1","NR CA configurations for inter-band CA (four bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B29),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B29)))","v":1509},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B29),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B29)))","v":0},{"$f":"IFERROR(E29/D29,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B29),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B29)))","v":56},{"$f":"D29-E29-G29","v":1453}]
[null,"38.101-1:Table 5.5A.3.4-1","NR CA configurations for inter-band CA (five bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B30),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B30)))","v":90},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B30),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B30)))","v":0},0,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B30),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B30)))","v":1},89]
[null,"NR CA configurations within FR2"]
[null,"38.101-2:Table 5.5A.1-1","NR CA configurations for intra-band contiguous CA",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B32),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B32)))","v":312},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B32),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B32)))","v":0},{"$f":"IFERROR(E32/D32,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B32),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B32)))","v":50},{"$f":"D32-E32-G32","v":262}]
[null,"38.101-2:Table 5.5A.2-1","NR CA configurations for intra-band non-contiguous CA",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B33),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B33)))","v":60},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B33),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B33)))","v":0},0,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B33),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B33)))","v":4},56]
[null,"38.101-2:Table 5.5A.2-2","NR CA configurations for intra-band non-contiguous CA",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B34),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B34)))","v":390},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B34),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B34)))","v":0},0,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B34),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B34)))","v":4},386]
[null,"38.101-2:Table 5.5A.3-1","NR CA configurations for inter-band CA",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B35),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B35)))","v":169},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B35),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B35)))","v":0},0,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B35),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B35)))","v":1},168]
[null,"NR CA configurations including FR1 with FR2"]
[null,"38.101-3:Table 5.5A.1-1a-o","Inter-band CA configurations between FR1 and FR2 (two bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B37),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B37)))","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B37),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B37)))","v":0},{"$f":"IFERROR(E37/D37,\"-\")","v":"-"},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B37),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B37)))","v":0},{"$f":"D37-E37-G37","v":0}]
[null,"38.101-3:Table 5.5A.1-2","Inter-band CA configurations between FR1 and FR2 (three bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B38),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B38)))","v":5016},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B38),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B38)))","v":0},{"$f":"IFERROR(E38/D38,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B38),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B38)))","v":192},{"$f":"D38-E38-G38","v":4824}]
[null,"38.101-3:Table 5.5A.1-3","Inter-band CA configurations between FR1 and FR2 (four bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B39),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B39)))","v":1171},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B39),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B39)))","v":0},{"$f":"IFERROR(E39/D39,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B39),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B39)))","v":0},{"$f":"D39-E39-G39","v":1171}]
[null,"38.101-3:Table 5.5A.1-4","Inter-band CA configurations between FR1 and FR2 (five bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B40),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B40)))","v":152},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B40),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B40)))","v":0},{"$f":"IFERROR(E40/D40,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B40),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B40)))","v":0},{"$f":"D40-E40-G40","v":152}]
[null,"NR-DC"]
[null,"NR-DC configurations within FR1"]
[null,"38.101-1:Table 5.5B.1-1","Inter-band NR DC configurations (two bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B43),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B43)))","v":140},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B43),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B43)))","v":1},7.1428571428571426E-3,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B43),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B43)))","v":14},125]
[null,"38.101-1:Table 5.5B.1-2","Inter-band NR DC configurations (three bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B44),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B44)))","v":87},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B44),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B44)))","v":0},{"$f":"IFERROR(E44/D44,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B44),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B44)))","v":0},{"$f":"D44-E44-G44","v":87}]
[null,"38.101-1:Table 5.5B.1-3","Inter-band NR DC configurations (four bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B45),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B45)))","v":42},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B45),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B45)))","v":0},{"$f":"IFERROR(E45/D45,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B45),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B45)))","v":0},{"$f":"D45-E45-G45","v":42}]
[null,"NR-DC configurations including FR1 and FR2"]
[null,"38.101-3:Table 5.5B.7-1","Inter-band NR-DC configurations between FR1 and FR2 (two bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B47),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B47)))","v":2039},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B47),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B47)))","v":6},{"$f":"IFERROR(E47/D47,\"-\")","v":2.9426189308484553E-3},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B47),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B47)))","v":260},{"$f":"D47-E47-G47","v":1773}]
[null,"38.101-3:Table 5.5B.7-2","Inter-band NR-DC configurations between FR1 and FR2 (three bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B48),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B48)))","v":3314},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B48),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B48)))","v":0},{"$f":"IFERROR(E48/D48,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B48),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B48)))","v":253},{"$f":"D48-E48-G48","v":3061}]
[null,"38.101-3:Table 5.5B.7-3","Inter-band NR-DC configurations between FR1 and FR2 (four bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B49),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B49)))","v":654},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B49),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B49)))","v":0},{"$f":"IFERROR(E49/D49,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B49),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B49)))","v":0},{"$f":"D49-E49-G49","v":654}]
[null,"NR SUL"]
[null,"NR SUL configurations within FR1"]
[null,"38.101-1:Table 5.5C-1","SUL band combination",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B52),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B52)))","v":33},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B52),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B52)))","v":2},6.0606060606060608E-2,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B52),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B52)))","v":6},25]
[null,"38.101-1:Table 5.5C-2","SUL band combination with intra-band non-contiguous CA",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B53),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B53)))","v":5},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B53),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B53)))","v":0},0,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B53),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B53)))","v":3},2]
[null,"38.101-1:Table 5.5C-3","SUL band combination with intra-band contiguous CA",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B54),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B54)))","v":17},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B54),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B54)))","v":4},0.23529411764705882,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B54),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B54)))","v":0},13]
[null,"38.101-1:Table 5.5C-4","SUL band combination with inter-band CA",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B55),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B55)))","v":26},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B55),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B55)))","v":5},0.19230769230769232,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B55),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B55)))","v":0},21]
[null,"NE-DC"]
[null,"NE-DC configurations within FR1"]
[null,"38.101-3:Table 5.5B.4a.1-1","Inter-band NE-DC configurations within FR1 (two bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B58),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B58)))","v":42},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B58),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B58)))","v":0},{"$f":"IFERROR(E58/D58,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B58),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B58)))","v":0},{"$f":"D58-E58-G58","v":42}]
[null,"38.101-3:Table 5.5B.4a.2-1","Inter-band NE-DC configurations within FR1 (three bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B59),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B59)))","v":42},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B59),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B59)))","v":0},{"$f":"IFERROR(E59/D59,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B59),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B59)))","v":0},{"$f":"D59-E59-G59","v":42}]
[null,"38.101-3:Table 5.5B.4a.3-1","Inter-band NE-DC configurations within FR1 (four bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B60),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B60)))","v":33},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B60),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B60)))","v":0},{"$f":"IFERROR(E60/D60,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B60),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B60)))","v":0},{"$f":"D60-E60-G60","v":33}]
[null,"38.101-3:Table 5.5B.4a.4-1","Inter-band NE-DC configurations within FR1 (five bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B61),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B61)))","v":8},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B61),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B61)))","v":0},{"$f":"IFERROR(E61/D61,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B61),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B61)))","v":0},{"$f":"D61-E61-G61","v":8}]
[null,"NE-DC configurations within FR2"]
[null,"38.101-3:Table 5.5B.5a.1-1","Inter-band NE-DC configurations including FR2 (two bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B63),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B63)))","v":177},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B63),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B63)))","v":0},{"$f":"IFERROR(E63/D63,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B63),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B63)))","v":0},{"$f":"D63-E63-G63","v":177}]
[null,"38.101-3:Table 5.5B.5a.2-1","Inter-band NE-DC configurations including FR2 (three bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B64),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B64)))","v":329},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B64),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B64)))","v":0},{"$f":"IFERROR(E64/D64,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B64),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B64)))","v":0},{"$f":"D64-E64-G64","v":329}]
[null,"38.101-3:Table 5.5B.5a.3-1","Inter-band NE-DC configurations including FR2 (four bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B65),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B65)))","v":280},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B65),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B65)))","v":0},{"$f":"IFERROR(E65/D65,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B65),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B65)))","v":0},{"$f":"D65-E65-G65","v":280}]
[null,"38.101-3:Table 5.5B.5a.4-1","Inter-band NE-DC configurations including FR2 (five bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B66),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B66)))","v":64},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B66),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B66)))","v":0},{"$f":"IFERROR(E66/D66,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B66),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B66)))","v":0},{"$f":"D66-E66-G66","v":64}]
[null,"EN-DC"]
[null,"EN-DC configurations within FR1"]
[null,"38.101-3:Table 5.3B.1.2-1","EN-DC configurations for intra-band contiguous EN-DC",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B69),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B69)))","v":32},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B69),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B69)))","v":1},{"$f":"IFERROR(E69/D69,\"-\")","v":3.125E-2},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B69),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B69)))","v":8},{"$f":"D69-E69-G69","v":23}]
[null,"38.101-3:Table 5.3B.1.3-1","EN-DC configurations for intra-band non-contiguous EN-DC",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B70),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B70)))","v":23},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B70),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B70)))","v":2},8.6956521739130432E-2,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B70),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B70)))","v":2},19]
[null,"38.101-3:Table 5.3B.1.3-2","EN-DC configurations and bandwidth combination sets defined for intra-band EN-DC mixed intra-band contiguous and non-contiguous EN-DC",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B71),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B71)))","v":2},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B71),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B71)))","v":0},{"$f":"IFERROR(E71/D71,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B71),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B71)))","v":0},{"$f":"D71-E71-G71","v":2}]
[null,"38.101-3:Table 5.5B.4.1-1","Inter-band EN-DC configurations within FR1 (two bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B72),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B72)))","v":606},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B72),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B72)))","v":113},0.18646864686468648,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B72),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B72)))","v":85},408]
[null,"38.101-3:Table 5.5B.4.2-1","Inter-band EN-DC configurations within FR1 (three bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B73),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B73)))","v":3107},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B73),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B73)))","v":187},6.0186675249436758E-2,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B73),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B73)))","v":520},2400]
[null,"38.101-3:Table 5.5B.4.3-1","Inter-band EN-DC configurations within FR1 (four bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B74),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B74)))","v":4529},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B74),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B74)))","v":174},3.8419077058953414E-2,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B74),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B74)))","v":737},3618]
[null,"38.101-3:Table 5.5B.4.4-1","Inter-band EN-DC configurations within FR1 (five bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B75),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B75)))","v":2138},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B75),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B75)))","v":68},3.1805425631431246E-2,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B75),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B75)))","v":258},1812]
[null,"38.101-3:Table 5.5B.4.5-1","Inter-band EN-DC configurations within FR1 (six bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B76),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B76)))","v":252},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B76),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B76)))","v":8},3.1746031746031744E-2,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B76),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B76)))","v":0},244]
[null,"EN-DC configurations within FR2"]
[null,"38.101-3:Table 5.5B.5.1-1","Inter-band EN-DC configurations including FR2 (two bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B78),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B78)))","v":5048},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B78),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B78)))","v":11},2.1790808240887481E-3,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B78),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B78)))","v":523},4514]
[null,"38.101-3:Table 5.5B.5.2-1","Inter-band EN-DC configurations including FR2 (three bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B79),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B79)))","v":10660},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B79),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B79)))","v":34},3.1894934333958724E-3,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B79),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B79)))","v":2426},8200]
[null,"38.101-3:Table 5.5B.5.3-1","Inter-band EN-DC configurations including FR2 (four bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B80),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B80)))","v":10718},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B80),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B80)))","v":18},1.6794178018286995E-3,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B80),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B80)))","v":2340},8360]
[null,"38.101-3:Table 5.5B.5.4-1","Inter-band EN-DC configurations including FR2 (five bands)",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B81),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B81)))","v":4473},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B81),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Completion Reference]])<>\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B81)))","v":4},8.94254415381176E-4,{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B81),--(ConfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(ConfigTblID[[#All],[Interested Deployer(Note 2)]])<>\"\"),--(TRIM(ConfigTblID[[#All],[Completion Reference]])=\"\"),--(ConfigTblID[[#All],[TS and Source Table]]=Introduction!$B81)))","v":550},3919]
[null,"EN-DC configurations including FR1 and FR2"]
[null,"38.101-3:Table 5.5B.6.2-1","Inter-band EN-DC configurations including FR1 and FR2 (three bands)","Inter-band EN-DC with NR FR1+FR2 is not testable"]
[null,"38.101-3:Table 5.5B.6.3-1","Inter-band EN-DC configurations including FR1 and FR2 (four bands)"]
[null,"38.101-3:Table 5.5B.6.4-1","Inter-band EN-DC configurations including FR1 and FR2 (five bands)"]
[null,"38.101-3:Table 5.5B.6.5-1","Inter-band EN-DC configurations including FR1 and FR2 (six bands)"]
[]
[null,{"$f":"\"Status of V2X Bands and CBW extensions for \"&$C$5&\" in RAN5 scope for Power Class 3\"","v":"Status of V2X Bands and CBW extensions for All Releases in RAN5 scope for Power Class 3"}]
[null,"TS and Source Table","Type of configuration","Number of \nV2X bands","Number of completed \nV2X bands",null,"Number of assigned and ongoing \nV2X bands\n(not yet completed)","Number of pending \nV2X bands\n(not assigned)"]
[null,"Overall (All TSs and source tables for the selected release scope):",null,{"$f":"SUM($D$93)","v":6},{"$f":"IFERROR(SUM($E$93),\"-\")","v":0},{"$f":"IFERROR(E90/D90,\"-\")","v":0},{"$f":"IFERROR(SUM($G$93),\"-\")","v":0},{"$f":"IFERROR(D90-E90-G90,\"-\")","v":6}]
[null,"NR Bands"]
[null,"NR FR1 Bands and CBW extensions"]
[null,"38.101-1:Table 5.2E.1-1","V2X operating bands in FR1",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XbandsTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(V2XbandsTblID[[#All],[TS and Source Table]]=$B93),--(V2XbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XbandsTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(V2XbandsTblID[[#All],[TS and Source Table]]=Introduction!$B93)))","v":6},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(V2XbandsTblID[[#All],[TS and Source Table]]=Introduction!$B93),--(V2XbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(V2XbandsTblID[[#All],[TS and Source Table]]=Introduction!$B93)))","v":0},{"$f":"IFERROR(E93/D93,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XbandsTblID[[#All],[Interested Deployer]])<>\"\"),--(TRIM(V2XbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(V2XbandsTblID[[#All],[TS and Source Table]]=Introduction!$B93),--(V2XbandsTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XbandsTblID[[#All],[Interested Deployer]])<>\"\"),--(TRIM(V2XbandsTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(V2XbandsTblID[[#All],[TS and Source Table]]=Introduction!$B93)))","v":0},{"$f":"D93-E93-G93","v":6}]
[]
[null,{"$f":"\"Status of V2X configurations for \"&$C$5&\" in RAN5 scope for Power Class 3\"","v":"Status of V2X configurations for All Releases in RAN5 scope for Power Class 3"}]
[null,"TS and Source Table","Type of configuration","Number of \nV2X Configurations","Number of completed \nV2X Configurations",null,"Number of assigned and ongoing \nV2X Configurations\n(not yet completed)","Number of pending \nV2X Configurations\n(not assigned)"]
[null,"Overall (All TSs and source tables for the selected release scope):",null,{"$f":"IFERROR(SUM($D$100:$D$104),\"-\")","v":30},{"$f":"IFERROR(SUM($E$100:$E$104),\"-\")","v":0},{"$f":"IFERROR(E97/D97,\"-\")","v":0},{"$f":"SUM(G100:G104)","v":0},{"$f":"IFERROR(D97-E97-G97,\"-\")","v":30}]
[null,"V2X configurations"]
[null,"FR1 V2X Configurations"]
[null,"38.101-1:Table 5.3E.2-2","Intra-band con-current operation configurations",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=$B100),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B100)))","v":2},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B100),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B100)))","v":0},{"$f":"IFERROR(E100/D100,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Interested Deployer]])<>\"\"),--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B100),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Interested Deployer]])<>\"\"),--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B100)))","v":0},{"$f":"D100-E100-G100","v":2}]
[null,"38.101-1:Table 5.3E.2-1","Intra-band contiguous V2X configurations",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=$B101),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B101)))","v":9},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B101),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B101)))","v":0},{"$f":"IFERROR(E101/D101,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Interested Deployer]])<>\"\"),--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B101),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Interested Deployer]])<>\"\"),--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B101)))","v":0},{"$f":"D101-E101-G101","v":9}]
[null,"38.101-3:Table 5.5E.2-1","Intra-band contiguous V2X configurations",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=$B102),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B102)))","v":1},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B102),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B102)))","v":0},{"$f":"IFERROR(E102/D102,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Interested Deployer]])<>\"\"),--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B102),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Interested Deployer]])<>\"\"),--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B102)))","v":0},{"$f":"D102-E102-G102","v":1}]
[null,"38.101-3:Table 5.5E.3-1","Intra-band non-contiguous V2X configurations",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=$B103),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B103)))","v":1},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B103),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B103)))","v":0},{"$f":"IFERROR(E103/D103,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Interested Deployer]])<>\"\"),--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B103),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Interested Deployer]])<>\"\"),--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B103)))","v":0},{"$f":"D103-E103-G103","v":1}]
[null,"38.101-3:Table 5.5E.4.1-1","Inter-band V2X configurations",{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=$B104),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B104)))","v":17},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B104),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])<>\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B104)))","v":0},{"$f":"IFERROR(E104/D104,\"-\")","v":0},{"$f":"IF($C$5<>\"All Releases\",SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Interested Deployer]])<>\"\"),--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B104),--(V2XconfigTblID[[#All],[Release introduced in TS 38.101-x]]=$C$5)),SUMPRODUCT(--(TRIM(V2XconfigTblID[[#All],[Interested Deployer]])<>\"\"),--(TRIM(V2XconfigTblID[[#All],[RAN5 Completion Reference\n(Note 1)]])=\"\"),--(V2XconfigTblID[[#All],[TS and Source Table]]=Introduction!$B104)))","v":0},{"$f":"D104-E104-G104","v":17}]

{"sheet":"NR bands","index":1,"n_rows":141,"n_cols":17,"rows_kept":141,"cut":false,"hidden":false,"merged":[[6,2,6,10],[7,2,7,10],[0,0,2,0],[3,11,4,12],[0,2,0,10],[1,2,1,10],[3,2,3,10],[4,2,4,10],[5,2,5,10]]}
[{"$f":"COUNTA(NRbandsTblID[Marked config])&\" band items marked\"","v":"0 band items marked"},null,"3GPP RAN WG5 status for NR bands and CBW extensions",null,null,null,null,null,null,null,null,null,null,{"$f":"PRD21version","v":"PRD21 v1.5.0"}]
[null,null,"Based on:  TS 38.101-1 v17.8.0, TS 38.101-2 v17.8.0 (Dec 2022)"]
[]
[null,null,"Completed: Green row indicates that the 5G NR band / NR band CBW Extension item is complete in the RAN5 test specifications. Available for testing."]
[null,null,"Ongoing: Yellow row indicates that the 5G NR band / NR band CBW Extension item is ongoing and assigned to at least one \"Interested Deployer\" and at least one \"Responsible Company assignment\". CRs can be submitted to RAN5 test specifications."]
[null,null,"Ongoing: White row with black text indicates that the 5G NR band / NR band CBW Extension item is ongoing but pending assignment to a \"Responsible Company\". No CRs shall be submitted to the RAN5 specifications unless the company volunteers to be assigned as \"Responsible Company\"."]
[null,null,"Pending: White row with red text indicates that the 5G NR band / NR band CBW Extension item is pending assignment to an \"Interested Deployer\". No CRs shall be submitted to the RAN5 specifications."]
[null,null,"Note 1: Power classes beyond PC3 applies to all CBWs of the NR band and are indicated by a \"PCx\" suffix in the NR band column and in the power class column, where x is the power class e.g. \"PC2\" for power class 2.\nNote 2: The interested deployer column can be an interested mobile network operator (MNO) or any other interested deployers as defined in PRD21, clause 3.1. For the case the type of deployer is not an MNO the type of deployer is described in the comments column."]
["Marked config","Release introduced in TS 38.101-x","Type of band","TS and Source Table","NR band / NR band CBW Extension\n(Note 1)","CBWs \nSCS[kHz]:[MHz]+...+[MHz]\n(Note 1)","Status","Power Class (Note 1)","RAN5 Completion Meeting\n(Note 1)","RAN5 Completion Reference\n(Note 1)","Interested Deployer\n(Note 2)","Responsible Company (contact)","Assignment\n[RAN5 meeting]","Applicable RAN5 WI code(s)  for CRs","Band Sort Key","Comments","Introduced in PRD version"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n1","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:10+15+20","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Huawei (Yuxin Hao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n001 "},null,"v1.0.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n1 CBW (25,50)","SCS15:+25+50\nSCS30:+25+50\nSCS60:+25+50","Completed","PC3","RAN5#89","R5-216629","China Unicom","China Unicom (Yu Shi)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n001 CBW z25,50z "},null,"v1.0.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n1 CBW (30,40)","SCS15:+30+40\nSCS30:+30+40\nSCS60:+30+40","Completed","PC3","RAN5#89","R5-216629","China Unicom","China Unicom (Yu Shi)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n001 CBW z30,40z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n1 CBW (45)","SCS15:+45\nSCS30:+45\nSCS60:+45","Completed","PC3","RAN5#97","R5-226871","Legacy","Huawei (Yuxin Hao)","RAN5#93-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n001 CBW z45z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1","n1 PC2",null,"Completed","PC2","RAN5#97","R5-227635","China Unicom","China Unicom (Yu Shi), MediaTek","RAN#96e","TEI17_Test, NR_PC2_UE_FDD-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n001 PC002 "},null,"v1.2.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n2","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:10+15+20","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Bureau Veritas (Amy Tao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n002 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW"," n2 CBW (25,30,40)","SCS15:+25+30+40\nSCS30:+25+30+40\nSCS60:+25+30+40","Completed","PC3"," RAN5#95-e","R5-222357","Legacy","Ericsson (Leif Mattisson)","<RAN5#93-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n002 CBW z25,30,40z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n2 CBW (35)","SCS15:+35\nSCS30:+35\nSCS60:+35","Ongoing","PC3","","","T-Mobile USA","T-Mobile USA (Scott Probasco)",null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n002 CBW z35z "},null,"v1.0.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n3","SCS15:5+10+15+20+25+30\nSCS30:10+15+20+25+30\nSCS60:10+15+20+25+30","Completed","PC3","<=RAN5#93-e","R5-216625","China Telecom","China Telecom (Jing Zhao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n003 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n3 CBW (35,45)","SCS15:+35+45\nSCS30:+35+45\nSCS60:+35+45","Completed","PC3","RAN5#98","R5-230665","China Unicom","China Unicom (Huifang Sun)","RAN5#96-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n003 CBW z35,45z "},null,"v1.0.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n3 CBW (40)","SCS15:+40\nSCS30:+40\nSCS60:+40","Completed","PC3","RAN5#91","R5-216629","China Telecom","China Telecom (Jing Zhao)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n003 CBW z40z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n3 CBWs (50)","SCS15:+50\nSCS30:+50\nSCS60:+50","Completed","PC3","RAN5#97","R5-227115","China Unicom","China Unicom (Yu Shi)","<RAN5#93-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n003 CBWs z50z "},null,"v1.0.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n3 PC2",null,"Completed","PC2","RAN5#97","R5-227636","China Unicom","China Unicom (Yu Shi), MediaTek","RAN#96e","TEI17_Test, NR_PC2_UE_FDD-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n003 PC002 "},null,"v1.2.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n5","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:-","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Bureau Veritas (Amy Tao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n005 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n5 CBW (25)","SCS15:+25\nSCS30:+25\nSCS60:+25","Completed","PC3"," RAN5#95-e","R5-222358","Legacy","Ericsson (Leif Mattisson)","<RAN5#93-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n005 CBW z25z "},null,"v1.0.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n7","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:10+15+20","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Huawei (Yuxin Hao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n007 "},null,"v1.0.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n7 CBW (25,30,40,50)","SCS15:+25+30+40+50\nSCS30:+25+30+40+50\nSCS60:+25+30+40+50","Ongoing","PC3","","","Orange","Orange (Hajer Khanfir)","RAN5#94-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n007 CBW z25,30,40,50z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n7 CBW (35)","SCS15:+35\nSCS30:+35\nSCS60:+35","Ongoing (CBW)","PC3","","","-",null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n007 CBW z35z "},null,"v1.0.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n8","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:-","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Huawei (Yuxin Hao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n008 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n8 CBW (35)","SCS15:+35\nSCS30:+35\nSCS60:-","Completed","PC3","RAN5#98","R5-230665",null,"China Unicom (Huifang Sun)","RAN5#96-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n008 CBW z35z "},null,"v1.0.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n12","SCS15:5+10+15\nSCS30:10+15\nSCS60:-","Completed","PC3","<=RAN5#93-e","R5-216625","U.S. Cellular","Ericsson (Leif Mattisson)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n012 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1","n13","SCS15:5+10\nSCS30:10\nSCS60:-","Pending","PC3","","",null,null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n013 "},null,"v1.0.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1","n14","SCS15:5+10\nSCS30:10\nSCS60:-","Completed","PC3","RAN5#90","R5-216629","AT&T","AT&T (Ron Borsato)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n014 "},"n14 CBWs 5 and 10 MHz are also used for V2X operation (see \"V2X bands\" worksheet for V2X status)","v1.0.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1","n18","SCS15:5+10\nSCS30:10\nSCS60:-","Ongoing","PC3",null,null,"KDDI","KDDI (Taiki Matsuyoshi)","RAN5#94-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n018 "},null,"v1.0.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n20","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:-","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Huawei (Yuxin Hao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n020 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1","n24","SCS15:5+10\nSCS30:10\nSCS60:10","Completed","PC3","RAN5#93-e","R5-217494","Ligado Networks","Ligado Networks (Ojas Choksi)","<RAN5#93-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n024 "},null,"v1.0.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n25","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:10+15+20","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Huawei (Yuxin Hao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n025 "},null,"v1.0.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n25 CBW (25,30,40)","SCS15:+25+30+40\nSCS30:+25+30+40\nSCS60:+25+30+40","Completed","PC3"," RAN5#94-e","R5-220443","T-Mobile USA","T-Mobile (Scott Prather),Ericsson (Leif Mattisson),Rhode&Schwarz (Edwin Menzel)","RAN5#94-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n025 CBW z25,30,40z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n25 CBW (35,45)","SCS15:+35+45\nSCS30:+35+45\nSCS60:+35+45","Ongoing","PC3","","","T-Mobile USA","T-Mobile USA (Scott Probasco)",null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n025 CBW z35,45z "},null,"v1.0.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1","n26","SCS15:5+10+15+20\nSCS30:10+15\nSCS60:-","Completed","PC3","RAN5#89","R5-216629","Dish Network","DISH Network (Jussi Kuusisto)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n026 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1","n26 CBW (25,30)","TBD (Not yet in 38.101-1)","Pending","PC3",null,null,null,null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n026 CBW z25,30z "},null,"v1.1.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n28","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:-","Completed","PC3","<=RAN5#93-e","R5-216625","Orange","Orange (Hajer Khanfir)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n028 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1","n28 CBW (25)","TBD (Not yet in 38.101-1)","Pending","PC3",null,null,null,null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n028 CBW z25z "},null,"v1.1.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n28 CBW (30)","SCS15:+30\nSCS30:+30\nSCS60:-","Completed","PC3","RAN5#88","R5-216629","CMCC, CBN","CMCC (Danni Song)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n028 CBW z30z "},null,"v1.0.0"]
[null,"Rel-16","SDL FR1","38.101-1:Table 5.3.5-1","n29","SCS15:5+10\nSCS30:10\nSCS60:-","Completed","PC3","RAN5#87","R5-216629","Dish Network","DISH Network (Jussi Kuusisto)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n029 "},null,"v1.0.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1","n30","SCS15:5+10\nSCS30:10\nSCS60:-","Ongoing","PC3","","","AT&T","AT&T (Ron Borsato)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n030 "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n34","SCS15:5+10+15\nSCS30:10+15\nSCS60:10+15","Completed","PC3","<=RAN5#93-e","R5-216625","CMCC","CMCC (Danni Song)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n034 "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n34 PC2",null,"Completed","PC2","RAN5#95-e","R5-223502","CMCC","CMCC (Danni Song)","<RAN5#93-e","NR_UE_PC2_n34-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n034 PC002 "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n38","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:10+15+20","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Ericsson (Leif Mattisson)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n038 "},"n38 CBWs 10, 20, and 30 MHz are also used for V2X operation (see \"V2X bands\" worksheet for V2X status)","v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1 CBW","n38 CBW (25,30)","SCS15:+25+30\nSCS30:+25+30\nSCS60:+25+30","Completed","PC3"," RAN5#94-e","R5-220443","Anritsu","Anritsu (Setsu Masafumi)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n038 CBW z25,30z "},null,"v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1 CBW","n38 CBW (40)","SCS15:+40\nSCS30:+40\nSCS60:+40","Completed","PC3","RAN5#89","R5-216629","Legacy","Huawei (Yuxin Hao)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n038 CBW z40z "},"n38 CBW=40 MHz is also used for V2X operation (see \"V2X bands\" worksheet for V2X status)","v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n39","SCS15:5+10+15+20+25+30+40\nSCS30:10+15+20+25+30+40\nSCS60:10+15+20+25+30+40","Completed","PC3","<=RAN5#93-e","R5-216625","CMCC","CMCC (Danni Song)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n039 "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n39 PC2",null,"Completed","PC2","<=RAN5#93-e","R5-216625","CMCC","CMCC (Danni Song)","<RAN5#93-e","NR_UE_PC2_n39-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n039 PC002 "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n40","SCS15:5+10+15+20+25+30+40+50\nSCS30:10+15+20+25+30+40+50+60+80\nSCS60:10+15+20+25+30+40+50+60+80","Completed","PC3","<=RAN5#93-e","R5-216625","CMCC","CMCC (Danni Song)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n040 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n40 CBW (70)","SCS15:-\nSCS30:+70\nSCS60:+70","Ongoing (CBW)","PC3","","","-",null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n040 CBW z70z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n40 CBW (90,100)","SCS15:-\nSCS30:+90+100\nSCS60:+90+100","Ongoing (CBW)","PC3","","","-",null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n040 CBW z90,100z "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n41","SCS15:10+15+20+40+50\nSCS30:10+15+20+40+50+60+80+90+100\nSCS60:10+15+20+40+50+60+80+90+100","Completed","PC3","<=RAN5#88-e","R5-216625","T-Mobile USA","T-mobil (Scott Probasco)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n041 "},null,"v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1 CBW","n41 CBW (30)","SCS15:+30\nSCS30:+30\nSCS60:+30","Completed","PC3","RAN5#89","R5-216629","Softbank","Ericsson (Leif Mattisson)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n041 CBW z30z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1","n41 CBW (5)","TBD (Not yet in 38.101-1)","Pending","PC3",null,null,null,null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n041 CBW z5z "},null,"v1.1.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n41 CBW (70)","SCS15:-\nSCS30:+70\nSCS60:+70","Completed","PC3"," RAN5#96-e","R5-224021","Legacy","Ericsson (Leif Mattisson)","<RAN5#93-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n041 CBW z70z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n41 CBW(25,35,45)","TBD (Not yet in 38.101-1)","Pending","PC3","","",null,null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n041 CBWz25,35,45z "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n41 PC1.5",null,"Completed","PC1.5","RAN5#97","R5-227633","CMCC, T-Mobile USA","CMCC, T-mobil (Danni Song,Scott Probasco)","<RAN5#93-e","TEI16_Test, LTE_NR_B41_Bn41_PC29dBm-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n041 PC001.005 "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n41 PC2","SCS15:10+15+20+40+50\nSCS30:10+15+20+40+50+60+80+90+100\nSCS60:10+15+20+40+50+60+80+90+100","Completed","PC2","PC2: RAN5#88","R5-203332","T-Mobile USA","T-mobil (Scott Probasco)","<RAN5#93-e","TEI16_Test, ENDC_UE_PC2_TDD_TDD-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n041 PC002 "},null,"v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1","n46","SCS15:10+20+40\nSCS30:10+20+40+60+80\nSCS60:10+20+40+60+80","Ongoing","PC3","","","Charter Communications ",null,"RAN5#97","NR_unlic-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n046 "},null,"v1.1.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n46 CBW (100)","TBD (Not yet in 38.101-1)","Pending","PC3","","",null,null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n046 CBW z100z "},null,"v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1","n48","SCS15:5+10+15+20+40+50\nSCS30:10+15+20+40+50+60+80+90+100\nSCS60:10+15+20+40+50+60+80+90+100","Completed","PC3","RAN5#88","R5-216629","Legacy","Ericsson (Leif Mattisson)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n048 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n48 CBW (30)","SCS15:+30\nSCS30:+30\nSCS60:+30","Completed","PC3"," RAN5#96-e","R5-224022","Legacy","Ericsson (Leif Mattisson)","<RAN5#93-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n048 CBW z30z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n48 CBW (70)","SCS15:-\nSCS30:+70\nSCS60:+70","Completed","PC3","RAN5#96-e","R5-224022","Legacy","Ericsson (Leif Mattisson)","<RAN5#93-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n048 CBW z70z "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n50","SCS15:5+10+15+20+40+50\nSCS30:10+15+20+40+50+60+80\nSCS60:10+15+20+40+50+60+80","Completed","PC3","RAN5#97","R5-226274","Legacy","CAICT (Yufeng Zhang)",null,"TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n050 "},null,"v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1 CBW","n50 CBW (30)","SCS15:+30\nSCS30:+30\nSCS60:+30","Pending","PC3","","",null,null,null,"NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n050 CBW z30z "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n51","SCS15:5\nSCS30:-\nSCS60:-","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Ericsson (Leif Mattisson)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n051 "},null,"v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1","n53","SCS15:5+10\nSCS30:10\nSCS60:10","Completed","PC3","RAN5#90","R5-216629","Globalstar","Nokia (Tuomo Saynajakangas)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n053 "},null,"v1.0.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1","n65","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:10+15+20","Completed","PC3","RAN5#87","R5-216629","Dish Network","DISH Network (Jussi Kuusisto)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n065 "},null,"v1.0.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n65 CBW (50)","SCS15:+50\nSCS30:+50\nSCS60:+50","Ongoing (CBW)","PC3","","","-",null,null,"NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n065 CBW z50z "},null,"v1.0.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n66","SCS15:5+10+15+20+40\nSCS30:10+15+20+40\nSCS60:10+15+20+40","Completed","PC3","<=RAN5#93-e","R5-216625","Dish Network","DISH Network (Jussi Kuusisto)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n066 "},null,"v1.0.0"]
[null,"Rel-16","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n66 CBW (25,30)","SCS15:+25+30\nSCS30:+25+30\nSCS60:+25+30\n+asymmetric BCS1","Completed","PC3","RAN5#87","R5-216629","Legacy","Huawei (Yuxin Hao)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n066 CBW z25,30z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n66 CBW (35,45)","SCS15:+35+45\nSCS30:+35+45\nSCS60:+35+45","Ongoing","PC3","","","T-Mobile USA","T-Mobile USA (Scott Probasco)","<RAN5#93-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n066 CBW z35,45z "},null,"v1.0.0"]
[null,"Rel-17","SDL FR1","38.101-1:Table 5.3.5-1","n67","SCS15:5+10+15+20\nSCS30:10+15+20","Pending","PC3",null,null,null,null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n067 "},null,"v1.3.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n70","SCS15:5+10+15+20+25\nSCS30:10+15+20+25\nSCS60:10+15+20+25","Completed","PC3","<=RAN5#93-e","R5-216625","Dish Network","DISH Network (Jussi Kuusisto)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n070 "},null,"v1.0.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n71","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:-","Completed","PC3","<=RAN5#93-e","R5-216625","Dish Network","DISH Network (Jussi Kuusisto)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n071 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n71 CBW (25,30)","SCS15:+25+30\nSCS30:+25+30\nSCS60:-","Ongoing (CBW)","PC3","","","-",null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n071 CBW z25,30z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n71 CBW (35)","SCS15:+35\nSCS30:+35\nSCS60:-","Ongoing (CBW)","PC3","","","-",null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n071 CBW z35z "},null,"v1.0.0"]
[null,"Rel-15","FDD FR1","38.101-1:Table 5.3.5-1","n74","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:10+15+20","Completed","PC3","<=RAN5#93-e","R5-216625","NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n074 "},null,"v1.0.0"]
[null,"Rel-15","SDL FR1","38.101-1:Table 5.3.5-1","n75","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:10+15+20","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Ericsson (Leif Mattisson)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n075 "},null,"v1.0.0"]
[null,"Rel-16","SDL FR1","38.101-1:Table 5.3.5-1 CBW","n75 CBW (25,30,40,50)","SCS15:+25+30+40+50\nSCS30:+25+30+40+50\nSCS60:+25+30+40+50","Ongoing (CBW)","PC3","","","-",null,null,"NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n075 CBW z25,30,40,50z "},null,"v1.0.0"]
[null,"Rel-15","SDL FR1","38.101-1:Table 5.3.5-1","n76","SCS15:5\nSCS30:-\nSCS60:-","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Ericsson (Leif Mattisson)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n076 "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n77","SCS15:10+15+20+40+50\nSCS30:10+15+20+40+50+60+80+90+100\nSCS60:10+15+20+40+50+60+80+90+100","Completed","PC3","<=RAN5#88-e","R5-216625","Legacy","Ericsson (Leif Mattisson)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n077 "},null,"v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1 CBW","n77 CBW (25,30,70)","SCS15:+25+30\nSCS30:+25+30+70\nSCS60:+25+30+70","Completed","PC3","RAN5#95-e","R5-223500","China Unicom","China Unicom (Yu Shi)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n077 CBW z25,30,70z "},null,"v1.0.0"]
[null,"Rel-17","TDD FR1","38.101-1:Table 5.3.5-1","n77 PC1.5",null,"Completed","PC1.5","RAN5#97","R5-227637","Verizon","Verizon,Nokia (Jinwen Ma, Tuomo Saynajakangas)","<RAN5#93-e","TEI17_test, HPUE_PC1_5_n77_n78-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n077 PC001.005 "},null,"v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1","n77 PC2",null,"Completed","PC2","RAN5#88","R5-203332","CMCC","CMCC (Danni Song)","<RAN5#93-e","TEI_16Test, ENDC_UE_PC2_TDD_TDD-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n077 PC002 "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n78","SCS15:10+15+20+40+50\nSCS30:10+15+20+40+50+60+80+90+100\nSCS60:10+15+20+40+50+60+80+90+100","Completed","PC3","<=RAN5#88-e","R5-216625","CMCC","CMCC (Danni Song)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n078 "},null,"v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1 CBW","n78 CBW (25,30,70)","SCS15:+25+30\nSCS30:+25+30+70\nSCS60:+25+30+70","Completed","PC3","RAN5#95-e","R5-223500","China Unicom","China Unicom (Yu Shi)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n078 CBW z25,30,70z "},null,"v1.0.0"]
[null,"Rel-17","TDD FR1","38.101-1:Table 5.3.5-1","n78 PC1.5",null,"Completed","PC1.5","RAN5#97","R5-227638","Verizon","Verizon,Nokia (Jinwen Ma, Tuomo Saynajakangas)","<RAN5#93-e","TEI17_test, HPUE_PC1_5_n77_n78-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n078 PC001.005 "},null,"v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1","n78 PC2",null,"Completed","PC2","RAN5#88","R5-203332","CMCC","CMCC (Danni Song)","<RAN5#93-e","TEI_16Test, ENDC_UE_PC2_TDD_TDD-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n078 PC002 "},null,"v1.0.0"]
[null,"Rel-15","TDD FR1","38.101-1:Table 5.3.5-1","n79","SCS15:40+50\nSCS30:40+50+60+80+100\nSCS60:40+50+60+80+100","Completed","PC3","<=RAN5#88-e","R5-216625","CMCC","CMCC (Danni Song)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n079 "},"n79 CBW 40 MHz is also used for V2X operation (see \"V2X bands\" worksheet for V2X status)","v1.0.0"]
[null,"Rel-17","TDD FR1","38.101-1:Table 5.3.5-1 CBW","n79 CBW (10,20)","SCS15:+10+20\nSCS30:+10+20\nSCS60:+10+20","Completed","PC3","RAN5#97","R5-226867","-","Huawei (Yuxin Hao)","RAN5#97","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n079 CBW z10,20z "},"n79 CBWs 10 and 20 MHz are also used for V2X operation (see \"V2X bands\" worksheet for V2X status)","v1.0.0"]
[null,"Rel-17","TDD FR1","38.101-1:Table 5.3.5-1 CBW","n79 CBW (30,70, 90)","SCS15:+30\nSCS30:+30+70+90\nSCS60:+30+70+90","Ongoing (CBW)","PC3","","","-",null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n079 CBW z30,70, 90z "},"n79 CBW 30 MHz is also used for V2X operation (see \"V2X bands\" worksheet for V2X status)","v1.0.0"]
[null,"Rel-17","TDD FR1","38.101-1:Table 5.3.5-1","n79 PC1.5",null,"Completed","PC1.5","RAN5#97","R5-227634","CMCC","CMCC (Danni Song)","<RAN5#93-e","TEI17_Test, NR_UE_PC1_5_n79-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n079 PC001.005 "},null,"v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1","n79 PC2",null,"Completed","PC2","RAN5#88","R5-203332","CMCC","CMCC (Danni Song)","<RAN5#93-e","TEI_16Test, ENDC_UE_PC2_TDD_TDD-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n079 PC002 "},null,"v1.0.0"]
[null,"Rel-15","SUL FR1","38.101-1:Table 5.3.5-1","n80","SCS15:5+10+15+20+25+30\nSCS30:10+15+20+25+30\nSCS60:10+15+20+25+30","Completed","PC3","<RAN5#94-e","R5-217496","China Telecom","Chinatelecom (Jing Zhao)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n080 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n80 CBW (40)","SCS15:+40\nSCS30:+40\nSCS60:+40","Ongoing (CBW)","PC3","","","-",null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n080 CBW z40z "},null,"v1.0.0"]
[null,"Rel-15","SUL FR1","38.101-1:Table 5.3.5-1","n81","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:-","Ongoing","PC3","","","Legacy","Huawei (Yuxin Hao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n081 "},null,"v1.0.0"]
[null,"Rel-15","SUL FR1","38.101-1:Table 5.3.5-1","n82","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:-","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Huawei (Yuxin Hao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n082 "},null,"v1.0.0"]
[null,"Rel-15","SUL FR1","38.101-1:Table 5.3.5-1","n83","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:-","Completed","PC3","<RAN5#94-e","R5-217496","CMCC, CBN","Huawei (Chunying Gu)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n083 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1","n83 CBW (25)","TBD (Not yet in 38.101-1)","Ongoing (CBW)","PC3",null,null,"-",null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n083 CBW z25z "},null,"v1.1.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n83 CBW (30)","SCS15:+30\nSCS30:+30\nSCS60:-","Completed","PC3","<RAN5#93-e","R5-217494","Legacy","Huawei (Yuxin Hao)","<RAN5#93-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n083 CBW z30z "},null,"v1.0.0"]
[null,"Rel-15","SUL FR1","38.101-1:Table 5.3.5-1","n84","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:10+15+20","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Huawei (Yuxin Hao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n084 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n84 CBW (25,30,40,50)","SCS15:+25+30+40+50\nSCS30:+25+30+40+50\nSCS60:+25+30+40+50","Completed","PC3","<RAN5#93-e","R5-217494","Legacy","Huawei (Yuxin Hao)","<RAN5#93-e","NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n084 CBW z25,30,40,50z "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1","n85","SCS15:5+10+15\nSCS30:10+15","Pending","PC3",null,null,null,null,null,"NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n085 "},null,"v1.3.0"]
[null,"Rel-15","SUL FR1","38.101-1:Table 5.3.5-1","n86","SCS15:5+10+15+20+40\nSCS30:10+15+20+40\nSCS60:10+15+20+40","Completed","PC3","RAN5#97","R5-226275","Legacy","CAICT (Yufeng Zhang)",null,"TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n086 "},null,"v1.0.0"]
[null,"Rel-16","SUL FR1","38.101-1:Table 5.3.5-1","n89","SCS15:5+10+15+20\nSCS30:10+15+20\nSCS60:-","Pending","PC3","","",null,null,null,"NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n089 "},null,"v1.0.0"]
[null,"Rel-16","NR FR1","38.101-1:Table 5.3.5-1","n90","SCS15:10+15+20+30+40+50\nSCS30:10+15+20+30+40+50+60+80+90+100\nSCS60:10+15+20+30+40+50+60+80+90+100","Pending","PC3","","",null,null,null,"FFS",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n090 "},"Currently not in scope of PRD21 but included for completeness (RAN4 WI; NR_n41_LTE_41_coex-Core not yet covered by any  RAN5 WI)","v1.2.0"]
[null,"Rel-16","NR FR1","38.101-1:Table 5.3.5-1","n91","SCS15:5+10","Completed","PC3","RAN5#97","R5-225951","Orange","Nokia (Tuomo Saynajakangas)","RAN5#96-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n091 "},null,"v1.2.0"]
[null,"Rel-16","NR FR1","38.101-1:Table 5.3.5-1","n92","SCS15:5+10+15+10\nSCS30:10+15+20","Completed","PC3","RAN5#97","R5-225951","Orange","Nokia (Tuomo Saynajakangas)","RAN5#96-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n092 "},null,"v1.2.0"]
[null,"Rel-16","NR FR1","38.101-1:Table 5.3.5-1","n93","SCS15:5+10","Completed","PC3","RAN5#97","R5-225951","Orange","Nokia (Tuomo Saynajakangas)","RAN5#96-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n093 "},null,"v1.2.0"]
[null,"Rel-16","NR FR1","38.101-1:Table 5.3.5-1","n94","SCS15:5+10+15+10\nSCS30:10+15+20","Completed","PC3","RAN5#97","R5-225951","Orange","Nokia (Tuomo Saynajakangas)","RAN5#96-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n094 "},null,"v1.2.0"]
[null,"Rel-16","SUL FR1","38.101-1:Table 5.3.5-1","n95","SCS15:5+10+15\nSCS30:10+15\nSCS60:10+15","Completed","PC3","RAN5#87","R5-216629","CMCC","CMCC (Danni Song)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n095 "},null,"v1.0.0"]
[null,"Rel-16","TDD FR1","38.101-1:Table 5.3.5-1","n96","SCS15:20+40\nSCS30:20+40+60+80\nSCS60:20+40+60+80","Ongoing","PC3","","","Charter Communications ",null,"RAN5#97","NR_unlic-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n096 "},null,"v1.1.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1 CBW","n96 CBW (100)\n","TBD (Not yet in 38.101-1)","Pending","PC3","","",null,null,null,"TEI17_Test, NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n096 CBW z100z\n "},null,"v1.0.0"]
[null,"Rel-17","SUL FR1","38.101-1:Table 5.3.5-1","n97","SCS15:5+10+15+20+25+30+40+50\nSCS30:10+15+20+25+30+40+50+60+70+80+90+100\nSCS60:10+15+20+25+30+40+50+60+70+80+90+100","Completed","PC3","RAN5#94-e","R5-221138","Legacy","Huawei (Yuxin Hao)","<RAN5#94-e","TEI17_Test, NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n097 "},null,"v1.0.0"]
[null,"Rel-17","SUL FR1","38.101-1:Table 5.3.5-1","n98","SCS15:5+10+15+20+25+30+40\nSCS30:10+15+20+25+30+40\nSCS60:10+15+20+25+30+40","Pending","PC3","","",null,null,null,"TEI17_Test, NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n098 "},null,"v1.0.0"]
[null,"Rel-17","SUL FR1","38.101-1:Table 5.3.5-1","n99","SCS15:5+10\nSCS30:10\nSCS60:10","Completed","PC3","RAN5#93-e","R5-217494","Ligado Networks","Ligado Networks (Ojas Choksi)","<RAN5#93-e","TEI17_Test, NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n099 "},null,"v1.0.0"]
[null,"Rel-17","FDD FR1","38.101-1:Table 5.3.5-1","n100 (railway band))","SCS 15: 5","Completed","PC3","RAN5#98","R5-230064","UIC","Nokia (Tuomo Säynäjäkangas)","RAN5#97","TEI17_Test, NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n100 zrailway bandz) "},"UIC (International Union of Railways) is interested deployer of the band.","v1.1.0"]
[null,"Rel-17","TDD FR1","38.101-1:Table 5.3.5-1","n101 (railway band))","SCS15:5+10\nSCS30:10","Completed","PC3","RAN5#98","R5-230064","UIC","Nokia (Tuomo Säynäjäkangas)","RAN5#97","TEI17_Test, NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n101 zrailway bandz) "},"UIC (International Union of Railways) is interested deployer of the band.","v1.1.0"]
[null,"Rel-17","TDD FR1","38.101-1:Table 5.3.5-1","n104","SCS15:5+10\nSCS30:10","Pending","PC3",null,null,"Orange",null,"RAN5#98","TEI17_Test, NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n104 "},null,"v1.3.0"]
[null,"Rel-17","TDD FR2","38.101-2:Table 5.3.5-1","n255",null,"Ongoing","PC3","","","CMCC","CMCC (Danni Song)","RAN5#98","NR_NTN_solutions_plus_CT-UEConTest,\nLTE_NBIOT_eMTC_NTN_plus_EPS-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n255 "},null,"v1.4.0"]
[null,"Rel-17","TDD FR2","38.101-2:Table 5.3.5-1","n255 PC5",null,"Ongoing","PC5","","","CMCC","CMCC (Danni Song)","RAN5#98","NR_NTN_solutions_plus_CT-UEConTest,\nLTE_NBIOT_eMTC_NTN_plus_EPS-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n255 PC005 "},null,"v1.4.0"]
[null,"Rel-17","TDD FR2","38.101-2:Table 5.3.5-1","n256",null,"Ongoing","PC3","","","CMCC","CMCC (Danni Song)","RAN5#98","NR_NTN_solutions_plus_CT-UEConTest,\nLTE_NBIOT_eMTC_NTN_plus_EPS-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n256 "},null,"v1.4.0"]
[null,"Rel-17","TDD FR2","38.101-2:Table 5.3.5-1","n256 PC5",null,"Ongoing","PC5","","","CMCC","CMCC (Danni Song)","RAN5#98","NR_NTN_solutions_plus_CT-UEConTest,\nLTE_NBIOT_eMTC_NTN_plus_EPS-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n256 PC005 "},null,"v1.4.0"]
[null,"Rel-15","TDD FR2","38.101-2:Table 5.3.5-1","n257","SCS60:50+100+200\nSCS120:50+100+200+400","Completed","PC3","<=RAN5#93-e","R5-216625","NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n257 "},null,"v1.0.0"]
[null,"Rel-17","TDD FR2","38.101-2:Table 5.3.5-1","n257 PC6",null,"Ongoing","PC6","","","China Unicom",null,"RAN5#98","NR_HST_FR2-UEConTest\t",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n257 PC006 "},null,"v1.3.0"]
[null,"Rel-17","TDD FR2","38.101-2:Table 5.3.5-1","n257 PC7",null,"Ongoing","PC7","","","China Unicom","China Unicom (Yu Shi)","RAN5#98","NR_redcap_plus_ARCH-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n257 PC007 "},null,"v1.4.0"]
[null,"Rel-15","TDD FR2","38.101-2:Table 5.3.5-1","n258","SCS60:50+100+200\nSCS120:50+100+200+400","Ongoing","PC3","","","U.S. Cellular","Ericsson (Niclas Weiler)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n258 "},null,"v1.0.0"]
[null,"Rel-17","TDD FR2","38.101-2:Table 5.3.5-1","n258 PC6",null,"Ongoing","PC6","","","China Unicom","Samsung (Sunlin Zhu)","RAN5#97","NR_HST_FR2-UEConTest\t",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n258 PC006 "},null,"v1.3.0"]
[null,"Rel-17","TDD FR2","38.101-2:Table 5.3.5-1","n258 PC7",null,"Ongoing","PC7","","","China Unicom","China Unicom (Yu Shi)","RAN5#98","NR_redcap_plus_ARCH-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n258 PC007 "},null,"v1.4.0"]
[null,"Rel-16","TDD FR2","38.101-2:Table 5.3.5-1","n259","SCS60:50+100+200\nSCS120:50+100+200+400","Ongoing","PC3","","","NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#93-e","NR_bands_BW_R16-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n259 "},null,"v1.0.0"]
[null,"Rel-17","TDD FR2","38.101-2:Table 5.3.5-1","n259 PC2",null,"Pending","PC2","","",null,null,null,"NR_RF_FR2_req_enh2-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n259 PC002 "},null,"v1.3.0"]
[null,"Rel-15","TDD FR2","38.101-2:Table 5.3.5-1","n260","SCS60:50+100+200\nSCS120:50+100+200+400","Ongoing","PC3","","","Legacy","Bureau Veritas (Amy Tao)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n260 "},null,"v1.0.0"]
[null,"Rel-15","TDD FR2","38.101-2:Table 5.3.5-1","n261","SCS60:50+100+200\nSCS120:50+100+200+400","Ongoing","PC3","","","Legacy","Ericsson (Niclas Weiler)","<RAN5#93-e","TEI15_Test, 5GS_NR_LTE-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n261 "},null,"v1.0.0"]
[null,"Rel-17","TDD FR2","38.101-2:Table 5.3.5-1","n261 PC6",null,"Ongoing","PC6","","","Veri<on",null,"RAN5#98","NR_HST_FR2-UEConTest\t",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n261 PC006 "},null,"v1.3.0"]
[null,"Rel-17","TDD FR2","38.101-2:Table 5.3.5-1","n261 PC7",null,"Ongoing","PC7","","","China Unicom","China Unicom (Yu Shi)","RAN5#98","NR_redcap_plus_ARCH-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n261 PC007 "},null,"v1.4.0"]
[null,"Rel-17","TDD FR2","38.101-2:Table 5.3.5-1","n262","SCS60:50+100+200\nSCS120:50+100+200+400","Ongoing","PC3","","","Legacy","Apple (Ashwin Mohan)","<RAN5#93-e","TEI17_Test, NR_lic_bands_BW_R17-UEConTest",{"$f":"SortKey(NRbandsTblID[[#This Row],[NR band / NR band CBW Extension\n(Note 1)]])","v":" n262 "},null,"v1.0.0"]

{"sheet":"5G NR CADC Configurations","index":2,"n_rows":82441,"n_cols":18,"rows_kept":4500,"cut":true,"hidden":false,"merged":[[6,2,6,10],[7,2,7,10],[0,0,2,0],[3,0,7,0],[0,13,7,13],[3,11,6,12],[0,2,0,10],[1,2,1,10],[3,2,3,10],[4,2,4,10],[5,2,5,10]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
[{"$f":"COUNTA(ConfigTblID[Marked config])&\" configs marked\"","v":"0 configs marked"},null,"3GPP RAN WG5 status NR CA, NR-DC, NE-DC and EN-DC configurations",null,null,null,null,null,null,null,null,null,null,{"$f":"PRD21version","v":"PRD21 v1.5.0"}]
[null,null,"Based on:  TS 38.101-1 v17.8.0, TS 38.101-2 v17.8.0 and TS 38.101-3 v17.8.0 (Dec 2022)"]
[]
[null,null,"Completed: Green row indicates that the 5G NR CADC configuration is complete in the RAN5 test specifications. Available for testing."]
[null,null,"Ongoing: Yellow row indicates that the 5G NR CADC configuration is assigned to at least one \"Interested Deployer\" or is a fallback to an ongoing configuration, and at least one \"Responsible Company\". CRs can be submitted to RAN5 test specifications."]
[null,null,"Ongoing: White row with black text indicates that the 5G NR CADC configuration is ongoing but not yet assigned to any \"Responsible Company\". No CRs shall be submitted to the RAN5 specifications unless the company volunteers to be assigned as \"Responsible Company\"."]
[null,null,"Pending: White row with red text indicates that the 5G NR CADC configuration is is pending assignment to \"Interested Deployer\" for PC3. No CRs shall be submitted to the RAN5 specifications."]
[null,null,"Note 1: Power classes beyond PC3 are indicated by a \"PCx\" suffix in the \"UL configuration\" and \"Power class\" columns, where x is the power class e.g. \"PC2\" for power class 2. Power classes beyond PC3 are only indicated for the items without any \"BCS\" suffix but applies to all bandwidth combination sets of the UL configuration defined for the PC3 case.\nNote 2: The interested deployer column can be an interested mobile network operator (MNO) or any other interested deployers as defined in PRD21, clause 3.1. For the case the type of deployer is not an MNO the type of deployer is described in the comments column."]
["Marked config","Release introduced in TS 38.101-x","Type of configuration","TS and Source Table","Configuration","Uplink\nconfiguration\n(Note 1)","Status","Power Class (Note 1)","RAN5 Completion Meeting","Completion Reference","Interested Deployer(Note 2)","Responsible Company (contact)","Assignment\n[RAN5 meeting]","Applicable RAN5 WI code(s)  for CRs","DL Sort Key","UL Sort Key","Comments","Introduced in PRD version"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n3A","-","Ongoing","PC3",null,null,"Telefonica","Huawei (Chunying Gu)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n3A","CA_n1A-n3A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n3A BCS1","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n3A BCS1","CA_n1A-n3A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A BCS1 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n5A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n5A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n5A","CA_n1A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A ","CA_n001A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n5A","CA_n3A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A ","CA_n003A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7A","CA_n1A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A ","CA_n001A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7A","CA_n3A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A ","CA_n003A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7A","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A ","CA_n003A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7A","CA_n5A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A ","CA_n005A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A_n078A ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7A-n78A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A_n078A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7A-n78A","CA_n1A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A_n078A ","CA_n001A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7A-n78A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A_n078A ","CA_n001A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A_n078A ","CA_n001A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7A-n78A","CA_n3A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A_n078A ","CA_n003A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7A-n78A","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A_n078A ","CA_n003A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7A-n78A","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A_n078A ","CA_n003A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7A-n78A","CA_n5A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A_n078A ","CA_n005A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7A-n78A","CA_n5A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A_n078A ","CA_n005A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7A-n78A","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007A_n078A ","CA_n007A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7B","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7B","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7B","CA_n1A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B ","CA_n001A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7B","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7B","CA_n3A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B ","CA_n003A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7B","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B ","CA_n003A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7B","CA_n5A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B ","CA_n005A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n7B","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B ","CA_n007B ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7B-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B_n078A ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7B-n78A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B_n078A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7B-n78A","CA_n1A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B_n078A ","CA_n001A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7B-n78A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B_n078A ","CA_n001A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7B-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B_n078A ","CA_n001A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7B-n78A","CA_n3A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B_n078A ","CA_n003A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7B-n78A","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B_n078A ","CA_n003A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7B-n78A","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B_n078A ","CA_n003A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7B-n78A","CA_n5A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B_n078A ","CA_n005A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7B-n78A","CA_n5A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B_n078A ","CA_n005A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7B-n78A","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B_n078A ","CA_n007A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n5A-n7B-n78A","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n007B_n078A ","CA_n007B ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n78A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n078A ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n78A","CA_n1A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n078A ","CA_n001A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n78A","CA_n3A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n078A ","CA_n003A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n78A","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n078A ","CA_n003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n5A-n78A","CA_n5A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n005A_n078A ","CA_n005A_n078A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7A","-","Ongoing","PC3",null,null,"Orange",null,"RAN5#97","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n007A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7A BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A BCS1 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7A BCS1","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A BCS1 ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7A BCS1","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A BCS1 ","CA_n003A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7A BCS2","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A BCS2 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7A BCS2","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A BCS2 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7A BCS2","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A BCS2 ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7A BCS2","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A BCS2 ","CA_n003A_n007A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n28A","-","Ongoing","PC3",null,null,"Orange",null,"RAN5#97","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n007A_n028A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n28A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n28A BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A BCS1 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n28A BCS1","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A BCS1 ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n28A BCS1","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A BCS1 ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n28A BCS1","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A BCS1 ","CA_n003A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n28A BCS1","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A BCS1 ","CA_n003A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n28A BCS1","CA_n7A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A BCS1 ","CA_n007A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78A","-","Ongoing","PC3",null,null,"Orange","Nokia (Tuomo Saynajakangas)","RAN5#97,RAN5#98","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078A BCS1 ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78A BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078A BCS1 ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78A BCS1","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078A BCS1 ","CA_n001A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78A BCS1","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078A BCS1 ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78A BCS1","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078A BCS1 ","CA_n001A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78A BCS1","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078A BCS1 ","CA_n003A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78A BCS1","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078A BCS1 ","CA_n003A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78A BCS1","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078A BCS1 ","CA_n003A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78A BCS1","CA_n7A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078A BCS1 ","CA_n007A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78A BCS1","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078A BCS1 ","CA_n007A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78A BCS1","CA_n28A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078A BCS1 ","CA_n028A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078z2Az ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78(2A)","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078z2Az ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78(2A)","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078z2Az ","CA_n001A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78(2A)","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078z2Az ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78(2A)","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078z2Az ","CA_n001A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78(2A)","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078z2Az ","CA_n003A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78(2A)","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078z2Az ","CA_n003A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78(2A)","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078z2Az ","CA_n003A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78(2A)","CA_n7A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078z2Az ","CA_n007A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78(2A)","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078z2Az ","CA_n007A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7A-n28A-n78(2A)","CA_n28A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n028A_n078z2Az ","CA_n028A_n078A ",null,"v1.1.0"]
[null,"Rel-16","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A","-","Ongoing","PC3",null,null,"Orange",null,"RAN5#97","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n007A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS1 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS1","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS1 ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS1","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS1 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS1","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS1 ","CA_n003A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS1","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS1 ","CA_n003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS1","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS1 ","CA_n007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS2","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS2 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS2","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS2 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS2","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS2 ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS2","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS2 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS2","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS2 ","CA_n003A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS2","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS2 ","CA_n003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78A BCS2","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078A BCS2 ","CA_n007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78(2A)","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078z2Az ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78(2A)","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078z2Az ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78(2A)","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078z2Az ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78(2A)","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078z2Az ","CA_n003A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78(2A)","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078z2Az ","CA_n003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7A-n78(2A)","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007A_n078z2Az ","CA_n007A_n078A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7B","-","Ongoing","PC3",null,null,"Orange",null,"RAN5#97","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n007B ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7B BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7B BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B BCS1 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7B BCS1","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B BCS1 ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7B BCS1","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B BCS1 ","CA_n003A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n7B BCS1","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B BCS1 ","CA_n007B ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n28A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n007B_n028A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n28A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A BCS1 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n28A BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A BCS1 ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n28A BCS1","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A BCS1 ","CA_n001A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n28A BCS1","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A BCS1 ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n28A BCS1","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A BCS1 ","CA_n003A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n28A BCS1","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A BCS1 ","CA_n003A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n28A BCS1","CA_n7A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A BCS1 ","CA_n007A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n28A BCS1","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A BCS1 ","CA_n007B ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7B-n28A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A_n078A ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7B-n28A-n78A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A_n078A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7B-n28A-n78A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A_n078A ","CA_n001A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7B-n28A-n78A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A_n078A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7B-n28A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A_n078A ","CA_n001A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7B-n28A-n78A","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A_n078A ","CA_n003A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7B-n28A-n78A","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A_n078A ","CA_n003A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7B-n28A-n78A","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A_n078A ","CA_n003A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7B-n28A-n78A","CA_n7A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A_n078A ","CA_n007A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7B-n28A-n78A","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A_n078A ","CA_n007A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7B-n28A-n78A","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A_n078A ","CA_n007B ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n1A-n3A-n7B-n28A-n78A","CA_n28A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n028A_n078A ","CA_n028A_n078A ",null,"v1.1.0"]
[null,"Rel-16","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n78A","-","Ongoing","PC3",null,null,"Orange",null,"RAN5#97","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n007B_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n78A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n078A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n78A BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n078A BCS1 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n78A BCS1","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n078A BCS1 ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n78A BCS1","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n078A BCS1 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n78A BCS1","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n078A BCS1 ","CA_n003A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n78A BCS1","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n078A BCS1 ","CA_n003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n78A BCS1","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n078A BCS1 ","CA_n007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n7B-n78A BCS1","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n007B_n078A BCS1 ","CA_n007B ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n8A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n008A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n8A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77A-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077A_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77A-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077A_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77A-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077A_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77A-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077A_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n8A-n77(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77(2A)-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077z2Az_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77(2A)-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077z2Az_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77(2A)-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077z2Az_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77(2A)-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077z2Az_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77(2A)-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077z2Az_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77(2A)-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077z2Az_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77(2A)-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077z2Az_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n1A-n3A-n8A-n77(2A)-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n077z2Az_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n8A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n008A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n8A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n8A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n8A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n8A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n8A-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n8A-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n8A-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n8A-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n008A_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n18A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n18A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n18A","CA_n1A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A ","CA_n001A_n018A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n18A","CA_n3A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A ","CA_n003A_n018A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n28A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n028A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n28A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n028A ","CA_n001A_n003A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n28A","CA_n1A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n028A ","CA_n001A_n018A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n28A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n028A ","CA_n001A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n28A","CA_n3A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n028A ","CA_n003A_n018A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n28A","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n028A ","CA_n003A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n41A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n041A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n41A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n041A ","CA_n001A_n003A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n41A","CA_n1A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n041A ","CA_n001A_n018A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n41A","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n041A ","CA_n001A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n41A","CA_n3A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n041A ","CA_n003A_n018A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n41A","CA_n3A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n041A ","CA_n003A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n41A","CA_n18A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n041A ","CA_n018A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n077A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n77A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n077A ","CA_n001A_n003A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n77A","CA_n1A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n077A ","CA_n001A_n018A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n77A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n077A ","CA_n001A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n77A","CA_n3A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n077A ","CA_n003A_n018A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n77A","CA_n3A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n077A ","CA_n003A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n18A-n77A","CA_n18A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n018A_n077A ","CA_n018A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n20A","-","Ongoing","PC3",null,null,"Orange",null,"RAN5#97","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n020A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n20A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n020A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n20A","CA_n1A-n20A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n020A ","CA_n001A_n020A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n20A","CA_n3A-n20A","Ongoing","PC3",null,null,"Orange",null,"RAN5#97","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n020A ","CA_n003A_n020A ",null,"v1.1.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n28A","-","Ongoing","PC3",null,null,"Orange",null,"RAN5#97","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n028A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n28A BCS1","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A BCS1 ","_ ","Fallback to CA_n1A-n3A-n28A-n78A BCS1 with UL CA_n28A-n78A","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n28A BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A BCS1 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n28A BCS1","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A BCS1 ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n28A BCS1","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A BCS1 ","CA_n003A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n28A BCS2","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A BCS2 ","_ ","Fallback to CA_n1A-n3A-n28A-n78A BCS2 with UL CA_n28A-n78A","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n28A BCS2","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A BCS2 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n28A BCS2","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A BCS2 ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n28A BCS2","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A BCS2 ","CA_n003A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n41A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n041A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n41A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n041A ","CA_n001A_n003A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n41A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n041A ","CA_n001A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n41A","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n041A ","CA_n001A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n41A","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n041A ","CA_n003A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n41A","CA_n3A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n041A ","CA_n003A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n41A","CA_n28A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n041A ","CA_n028A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A ","CA_n003A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A","CA_n3A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A ","CA_n003A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A ","CA_n028A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A BCS1 ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A BCS1 ","CA_n001A_n003A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A BCS1","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A BCS1 ","CA_n001A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A BCS1","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A BCS1 ","CA_n001A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A BCS1","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A BCS1 ","CA_n003A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A BCS1","CA_n3A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A BCS1 ","CA_n003A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n77A BCS1","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n077A BCS1 ","CA_n028A_n077A ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A","-","Ongoing","PC3",null,null,"Orange","Nokia (Tuomo Saynajakangas)","RAN5#97,RAN5#98","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n028A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS1","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS1 ","_ ","Fallback to CA_n1A-n3A-n28A-n78A BCS1 with UL CA_n28A-n78A","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS1 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS1","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS1 ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS1","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS1 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS1","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS1 ","CA_n003A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS1","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS1 ","CA_n003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS1","CA_n28A-n78A","Ongoing","PC3",null,null,"Orange",null,"RAN5#97","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS1 ","CA_n028A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS2","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS2 ","_ ","Fallback to CA_n1A-n3A-n28A-n78A BCS2 with UL CA_n28A-n78A","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS2","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS2 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS2","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS2 ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS2","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS2 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS2","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS2 ","CA_n003A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS2","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS2 ","CA_n003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78A BCS2","CA_n28A-n78A","Ongoing","PC3",null,null,"Orange",null,"RAN5#97","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078A BCS2 ","CA_n028A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078z2Az ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78(2A)","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078z2Az ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78(2A)","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078z2Az ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78(2A)","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078z2Az ","CA_n001A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78(2A)","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078z2Az ","CA_n003A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78(2A)","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078z2Az ","CA_n003A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n78(2A)","CA_n28A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n078z2Az ","CA_n028A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n079A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n79A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n079A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n79A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n079A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n79A","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n079A ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n79A","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n079A ","CA_n003A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n79A","CA_n3A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n079A ","CA_n003A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n28A-n79A","CA_n28A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n079A ","CA_n028A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257A ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257A","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257A ","CA_n003A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257A","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257A ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257A","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257A ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257G ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257G","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257G ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257G","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257G ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257G ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257G ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257G","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257G ","CA_n003A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257G","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257G ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257G","CA_n3A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257G ","CA_n003A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257G","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257G ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257G","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257G ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","CA_n003A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","CA_n3A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","CA_n003A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","CA_n3A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","CA_n003A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257H","CA_n28A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257H ","CA_n028A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n001A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n003A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n3A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n003A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n3A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n003A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n3A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n003A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n28A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n028A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n28A-n257I","CA_n28A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n028A_n257I ","CA_n028A_n257I ",null,"v1.1.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n41A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n041A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n41A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n041A ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n41A","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n041A ","CA_n001A_n041A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n41A","CA_n3A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n041A ","CA_n003A_n041A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n41A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n041A_n077A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n41A-n77A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n041A_n077A ","CA_n001A_n003A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n41A-n77A","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n041A_n077A ","CA_n001A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n41A-n77A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n041A_n077A ","CA_n001A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n41A-n77A","CA_n3A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n041A_n077A ","CA_n003A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n41A-n77A","CA_n3A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n041A_n077A ","CA_n003A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n41A-n77A","CA_n41A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n041A_n077A ","CA_n041A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n41A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n041A_n257A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n41A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n041A_n257G ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n41A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n041A_n257H ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n41A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n041A_n257I ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n67A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n067A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n67A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n067A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n77A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n77A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n77A","CA_n3A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A ","CA_n003A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n77A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n77A BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A BCS1 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n77A BCS1","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A BCS1 ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n77A BCS1","CA_n3A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A BCS1 ","CA_n003A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n77A-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n079A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n77A-n79A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n079A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n77A-n79A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n079A ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n77A-n79A","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n079A ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n77A-n79A","CA_n3A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n079A ","CA_n003A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n77A-n79A","CA_n3A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n079A ","CA_n003A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n3A-n77A-n79A","CA_n77A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n079A ","CA_n077A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77A-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77A-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77A-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77A-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077A_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n77(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n77(2A)","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077z2Az ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n77(2A)","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077z2Az ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n77(2A)","CA_n3A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077z2Az ","CA_n003A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77(2A)-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077z2Az_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77(2A)-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077z2Az_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77(2A)-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077z2Az_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77(2A)-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077z2Az_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77(2A)-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077z2Az_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77(2A)-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077z2Az_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77(2A)-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077z2Az_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n77(2A)-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n077z2Az_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A","-","Ongoing","PC3",null,null,"Orange,China Telecom","China Telecom (Jingzhou Wu)","RAN5#97","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n078A ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A","CA_n1A-n78A","Ongoing","PC3",null,null,"China Telecom","China Telecom (Jingzhou Wu)","RAN5#97","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A","CA_n3A-n78A","Ongoing","PC3",null,null,"China Telecom","China Telecom (Jingzhou Wu)","RAN5#97","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003A_n078A ","CA_n003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A BCS1","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078A BCS1 ","_ ","Fallback to CA_n1A-n3A-n28A-n78A BCS1 with UL CA_n28A-n78A","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078A BCS1 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A BCS1","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078A BCS1 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A BCS1","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078A BCS1 ","CA_n003A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A BCS1","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078A BCS1 ","CA_n003A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A BCS2","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078A BCS2 ","_ ","Fallback to CA_n1A-n3A-n28A-n78A BCS2 with UL CA_n28A-n78A","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A BCS2","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078A BCS2 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A BCS2","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078A BCS2 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A BCS2","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078A BCS2 ","CA_n003A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78A BCS2","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078A BCS2 ","CA_n003A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78(2A)","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078z2Az ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78(2A)","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078z2Az ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n78(2A)","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n078z2Az ","CA_n003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n79A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n79A","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3A-n79A","CA_n3A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A ","CA_n003A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257A","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257A ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257A ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257A","CA_n3A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257A ","CA_n003A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257A","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257A ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257A","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257A ","CA_n079A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257G ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257G","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257G ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257G","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257G ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257G ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257G ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257G","CA_n3A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257G ","CA_n003A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257G","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257G ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257G","CA_n3A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257G ","CA_n003A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257G","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257G ","CA_n079A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257G","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257G ","CA_n079A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","CA_n3A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","CA_n003A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","CA_n3A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","CA_n003A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","CA_n3A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","CA_n003A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","CA_n079A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","CA_n079A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257H","CA_n79A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257H ","CA_n079A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n001A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n3A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n003A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n3A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n003A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n3A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n003A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n3A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n003A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n079A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n079A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n79A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n079A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n3A-n79A-n257I","CA_n79A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n079A_n257I ","CA_n079A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257A","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257A ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257A ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257A","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257A ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257G","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257G ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257G ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257G ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257G","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257G ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257G","CA_n3A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257G ","CA_n003A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257H","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257H ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257H ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257H ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257H ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257H","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257H ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257H","CA_n3A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257H ","CA_n003A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257H","CA_n3A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257H ","CA_n003A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257I","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257I ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257I ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257I ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257I ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257I ","CA_n001A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257I","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257I ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257I","CA_n3A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257I ","CA_n003A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257I","CA_n3A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257I ","CA_n003A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257I","CA_n3A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257I ","CA_n003A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n3A-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003A_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n3B","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003B ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3B-n7A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003B_n007A ","_ ",null,"v1.4.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n3(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n3(2A)","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n003z2Az ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n3(2A) BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003z2Az BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n3(2A) BCS1","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003z2Az BCS1 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n3(2A) BCS2","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003z2Az BCS2 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n3(2A) BCS2","CA_n1A-n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003z2Az BCS2 ","CA_n001A_n003A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n3(2A)-n7A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n003z2Az_n007A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n5A","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A ","_ ","Fallback to CA_n1(2A)-n5A with UL -","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n5A","CA_n1A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A ","CA_n001A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n7A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n7A","CA_n1A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007A ","CA_n001A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n7A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007A ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n7A","CA_n5A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007A ","CA_n005A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7A-n78A","CA_n1A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007A_n078A ","CA_n001A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7A-n78A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007A_n078A ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007A_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7A-n78A","CA_n5A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007A_n078A ","CA_n005A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7A-n78A","CA_n5A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007A_n078A ","CA_n005A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n7B","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n7B","CA_n1A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B ","CA_n001A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n7B","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n7B","CA_n5A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B ","CA_n005A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n7B","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B ","CA_n007B ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7B-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7B-n78A","CA_n1A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B_n078A ","CA_n001A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7B-n78A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B_n078A ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7B-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7B-n78A","CA_n5A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B_n078A ","CA_n005A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7B-n78A","CA_n5A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B_n078A ","CA_n005A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7B-n78A","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B_n078A ","CA_n007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n5A-n7B-n78A","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n007B_n078A ","CA_n007B ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n28A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n028A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n78A","CA_n1A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n078A ","CA_n001A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n5A-n78A","CA_n5A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n005A_n078A ","CA_n005A_n078A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n7A","-","Ongoing","PC3",null,null,"Orange",null,"RAN5#97","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n7A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n7A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n7A BCS1","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A BCS1 ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n8A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n8A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A ","CA_n001A_n007A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n8A","CA_n1A-n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A ","CA_n001A_n008A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n8A","CA_n7A-n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A ","CA_n007A_n008A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n40A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n040A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n40A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n040A ","CA_n001A_n007A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n40A","CA_n1A-n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n040A ","CA_n001A_n008A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n40A","CA_n1A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n040A ","CA_n001A_n040A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n40A","CA_n7A-n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n040A ","CA_n007A_n008A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n40A","CA_n7A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n040A ","CA_n007A_n040A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n40A","CA_n8A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n040A ","CA_n008A_n040A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n078A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n78A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n078A ","CA_n001A_n007A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n78A","CA_n1A-n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n078A ","CA_n001A_n008A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n078A ","CA_n001A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n78A","CA_n7A-n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n078A ","CA_n007A_n008A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n78A","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n078A ","CA_n007A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n8A-n78A","CA_n8A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n008A_n078A ","CA_n008A_n078A ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n28A","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A_n028A ","_ ","Fallback to CA_n1A-n3A-n7A-n28A with UL -","v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n28A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A_n028A ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n28A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A_n028A ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n28A","CA_n7A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A_n028A ","CA_n007A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78A","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078A ","_ ","Fallback to CA_n1A-n3A-n7A-n28A-n78A with UL -","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078A ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078A ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78A","CA_n7A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078A ","CA_n007A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78A","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078A ","CA_n007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78A","CA_n28A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078A ","CA_n028A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078z2Az ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78(2A)","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078z2Az ","CA_n001A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78(2A)","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078z2Az ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78(2A)","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078z2Az ","CA_n001A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78(2A)","CA_n7A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078z2Az ","CA_n007A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78(2A)","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078z2Az ","CA_n007A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n28A-n78(2A)","CA_n28A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n028A_n078z2Az ","CA_n028A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n40A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n040A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n40A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n040A ","CA_n001A_n007A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n40A","CA_n1A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n040A ","CA_n001A_n040A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n40A","CA_n7A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n040A ","CA_n007A_n040A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n40A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n040A_n078A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n40A-n78A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n040A_n078A ","CA_n001A_n007A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n40A-n78A","CA_n1A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n040A_n078A ","CA_n001A_n040A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n40A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n040A_n078A ","CA_n001A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n40A-n78A","CA_n7A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n040A_n078A ","CA_n007A_n040A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n40A-n78A","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n040A_n078A ","CA_n007A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7A-n40A-n78A","CA_n40A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n040A_n078A ","CA_n040A_n078A ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78A","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A_n078A ","_ ","Fallback to CA_n1A-n3A-n7A-n78A with UL -","v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A_n078A ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78A","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A_n078A ","CA_n007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n078A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78A BCS1","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n078A BCS1 ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78A BCS1","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n078A BCS1 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78A BCS1","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n078A BCS1 ","CA_n007A_n078A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A_n078z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78(2A)","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A_n078z2Az ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78(2A)","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A_n078z2Az ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78(2A)","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007A_n078z2Az ","CA_n007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78(2A) BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n078z2Az BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78(2A) BCS1","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n078z2Az BCS1 ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78(2A) BCS1","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n078z2Az BCS1 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n78(2A) BCS1","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n078z2Az BCS1 ","CA_n007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n079A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7A-n79C","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007A_n079C ","_ ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n7B","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n007B ","_ ","Fallback to CA_n1A-n3A-n7B with UL -","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n7B","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n7B","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B ","CA_n007B ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7B-n28A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7B-n28A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7B-n28A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7B-n28A","CA_n7A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A ","CA_n007A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7B-n28A","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A ","CA_n007B ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7B-n28A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A_n078A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7B-n28A-n78A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A_n078A ","CA_n001A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7B-n28A-n78A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A_n078A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7B-n28A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A_n078A ","CA_n001A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7B-n28A-n78A","CA_n7A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A_n078A ","CA_n007A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7B-n28A-n78A","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A_n078A ","CA_n007A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7B-n28A-n78A","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A_n078A ","CA_n007B ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n7B-n28A-n78A","CA_n28A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n028A_n078A ","CA_n028A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7B-n78A","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n078A ","_ ","Fallback to CA_n1A-n3A-n7B-n78A with UL -","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7B-n78A","CA_n1A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n078A ","CA_n001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7B-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7B-n78A","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n078A ","CA_n007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n7B-n78A","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n007B_n078A ","CA_n007B ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n8A","-","Completed","PC3","RAN5#98","R5-231217","China Unicom","China Unicom (Huifang Sun)","RAN5#95-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n008A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n8A","CA_n1A-n8A","Completed","PC3","RAN5#98","R5-231217","China Unicom","China Unicom (Huifang Sun)","RAN5#95-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n008A ","CA_n001A_n008A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n8A BCS1","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A BCS1 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n8A BCS1","CA_n1A-n8A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A BCS1 ","CA_n001A_n008A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n28A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n028A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n40A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n040A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n40A","CA_n1A-n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n040A ","CA_n001A_n008A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n40A","CA_n1A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n040A ","CA_n001A_n040A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n40A","CA_n8A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n040A ","CA_n008A_n040A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n8A-n40A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n040A_n078A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n8A-n40A-n78A","CA_n1A-n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n040A_n078A ","CA_n001A_n008A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n8A-n40A-n78A","CA_n1A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n040A_n078A ","CA_n001A_n040A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n8A-n40A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n040A_n078A ","CA_n001A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n8A-n40A-n78A","CA_n8A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n040A_n078A ","CA_n008A_n040A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n8A-n40A-n78A","CA_n8A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n040A_n078A ","CA_n008A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n8A-n40A-n78A","CA_n40A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n040A_n078A ","CA_n040A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77A-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077A_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77A-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077A_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77A-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077A_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77A-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077A_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n77(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77(2A)-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077z2Az_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77(2A)-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077z2Az_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77(2A)-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077z2Az_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77(2A)-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077z2Az_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77(2A)-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077z2Az_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77(2A)-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077z2Az_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77(2A)-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077z2Az_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n77(2A)-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n077z2Az_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n008A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n78A","CA_n1A-n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A ","CA_n001A_n008A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A ","CA_n001A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n78A","CA_n8A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A ","CA_n008A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n78A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n8A-n78A-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A_n079A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n78A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A_n257A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n78A-n257D","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A_n257D ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n78A-n257E","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A_n257E ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n78A-n257F","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A_n257F ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n78A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A_n257G ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n78A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A_n257H ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n78A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A_n257I ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n78A-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A_n257J ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n78A-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A_n257K ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n78A-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A_n257L ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n8A-n78A-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078A_n257M ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n78(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n8A-n78(2A)-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n078z2Az_n079A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n8A-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n079A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n8A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n8A-n257D","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n257D ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n8A-n257E","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n257E ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n8A-n257F","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n257F ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n8A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n8A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n8A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n8A-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n8A-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n8A-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n8A-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n008A_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n18A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n18A","CA_n1A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A ","CA_n001A_n018A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n28A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n28A","CA_n1A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A ","CA_n001A_n018A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n28A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n28A","CA_n18A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A ","CA_n018A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n41A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n041A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n41A","CA_n1A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n041A ","CA_n001A_n018A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n41A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n041A ","CA_n001A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n41A","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n041A ","CA_n001A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n41A","CA_n18A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n041A ","CA_n018A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n41A","CA_n18A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n041A ","CA_n018A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n41A","CA_n28A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n041A ","CA_n028A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n077A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n77A","CA_n1A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n077A ","CA_n001A_n018A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n77A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n077A ","CA_n001A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n77A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n077A ","CA_n001A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n77A","CA_n18A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n077A ","CA_n018A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n77A","CA_n18A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n077A ","CA_n018A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n28A-n77A","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n028A_n077A ","CA_n028A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n41A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n041A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n41A","CA_n1A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n041A ","CA_n001A_n018A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n41A","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n041A ","CA_n001A_n041A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n41A","CA_n18A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n041A ","CA_n018A_n041A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n41A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n041A_n077A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n41A-n77A","CA_n1A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n041A_n077A ","CA_n001A_n018A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n41A-n77A","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n041A_n077A ","CA_n001A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n41A-n77A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n041A_n077A ","CA_n001A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n41A-n77A","CA_n18A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n041A_n077A ","CA_n018A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n41A-n77A","CA_n18A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n041A_n077A ","CA_n018A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n18A-n41A-n77A","CA_n41A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n041A_n077A ","CA_n041A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n077A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n77A","CA_n1A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n077A ","CA_n001A_n018A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n77A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n077A ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n77A","CA_n18A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n077A ","CA_n018A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n77(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n077z2Az ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n77(2A)","CA_n1A-n18A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n077z2Az ","CA_n001A_n018A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n77(2A)","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n077z2Az ","CA_n001A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n18A-n77(2A)","CA_n18A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n018A_n077z2Az ","CA_n018A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n20A","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n020A ","_ ","Fallback to CA_n1A-n3A-n20A with UL -","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n20A","CA_n1A-n20A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n020A ","CA_n001A_n020A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n20A-n67A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n020A_n067A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n20A-n67A","CA_n1A-n20A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n020A_n067A ","CA_n001A_n020A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n20A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n020A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n28A","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n028A ","_ ","Fallback to CA_n1A-n3A-n28A with UL -","v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n28A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n028A ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n28A BCS1","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A BCS1 ","_ ","Fallback to CA_n1A-n3A-n28A-n78A BCS1 with UL CA_n28A-n78A","v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n28A BCS1","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A BCS1 ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n38A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n038A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n40A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40A-n78A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040A_n078A ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40A-n78A","CA_n1A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040A_n078A ","CA_n001A_n040A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040A_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40A-n78A","CA_n28A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040A_n078A ","CA_n028A_n040A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40A-n78A","CA_n28A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040A_n078A ","CA_n028A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40A-n78A","CA_n40A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040A_n078A ","CA_n040A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n40B","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040B ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40B-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040B_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40B-n78A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040B_n078A ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40B-n78A","CA_n1A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040B_n078A ","CA_n001A_n040A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40B-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040B_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40B-n78A","CA_n28A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040B_n078A ","CA_n028A_n040A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40B-n78A","CA_n28A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040B_n078A ","CA_n028A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n40B-n78A","CA_n40A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n040B_n078A ","CA_n040A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n41A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n41A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n41A","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A ","CA_n001A_n041A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n41A","CA_n28A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A ","CA_n028A_n041A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n41A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A_n077A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n41A-n77A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A_n077A ","CA_n001A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n41A-n77A","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A_n077A ","CA_n001A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n41A-n77A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A_n077A ","CA_n001A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n41A-n77A","CA_n28A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A_n077A ","CA_n028A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n41A-n77A","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A_n077A ","CA_n028A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n41A-n77A","CA_n41A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A_n077A ","CA_n041A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n41A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A_n257A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n41A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A_n257G ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n41A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A_n257H ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n41A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n041A_n257I ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n77A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n77A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n77A","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A ","CA_n028A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n77A-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n079A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n77A-n79A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n079A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n77A-n79A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n079A ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n77A-n79A","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n079A ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n77A-n79A","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n079A ","CA_n028A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n77A-n79A","CA_n28A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n079A ","CA_n028A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n1A-n28A-n77A-n79A","CA_n77A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n079A ","CA_n077A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257A ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257A ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257A","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257A ","CA_n028A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257A","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257A ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257A","CA_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257A ","CA_n077A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257G ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257G","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257G ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257G","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257G ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257G ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257G ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257G","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257G ","CA_n028A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257G","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257G ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257G","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257G ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257G","CA_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257G ","CA_n077A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257G","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257G ","CA_n077A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","CA_n028A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","CA_n28A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","CA_n028A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","CA_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","CA_n077A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","CA_n077A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257H","CA_n77A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257H ","CA_n077A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n001A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n028A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n28A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n028A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n28A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n028A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n077A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n077A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n77A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n077A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n77A-n257I","CA_n77A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077A_n257I ","CA_n077A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n77(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077z2Az ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n77(2A)","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077z2Az ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n77(2A)","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077z2Az ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n77(2A)","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077z2Az ","CA_n028A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n77(2A) BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077z2Az BCS1 ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n77(2A) BCS1","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077z2Az BCS1 ","CA_n001A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n77(2A) BCS1","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077z2Az BCS1 ","CA_n001A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n77(2A) BCS1","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n077z2Az BCS1 ","CA_n028A_n077A ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78A","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n028A_n078A ","_ ","Fallback to CA_n1A-n3A-n28A-n78A with UL -","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078A ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78A","CA_n28A-n78A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078A ","CA_n028A_n078A ","Fallback to CA_n1A-n3A-n28A-n78A BCS1 with UL CA_n28A-n78A","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78A BCS1","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078A BCS1 ","_ ","Fallback to CA_n1A-n3A-n28A-n78A BCS1 with UL CA_n28A-n78A","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78A BCS1","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078A BCS1 ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78A BCS1","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078A BCS1 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78A BCS1","CA_n28A-n78A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078A BCS1 ","CA_n028A_n078A ","Fallback to CA_n1A-n3A-n28A-n78A BCS1 with UL CA_n28A-n78A","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78A BCS2","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078A BCS2 ","_ ","Fallback to CA_n1A-n3A-n28A-n78A BCS2 with UL CA_n28A-n78A","v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78A BCS2","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078A BCS2 ","CA_n001A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78A BCS2","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078A BCS2 ","CA_n001A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78A BCS2","CA_n28A-n78A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078A BCS2 ","CA_n028A_n078A ","Fallback to CA_n1A-n3A-n28A-n78A BCS2 with UL CA_n28A-n78A","v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78(2A)","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078z2Az ","CA_n001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78(2A)","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078z2Az ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n78(2A)","CA_n28A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n078z2Az ","CA_n028A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n79A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n79A","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n28A-n79A","CA_n28A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A ","CA_n028A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257A","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257A ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257A ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257A","CA_n28A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257A ","CA_n028A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257A","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257A ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257A","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257A ","CA_n079A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257G ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257G","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257G ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257G","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257G ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257G ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257G ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257G","CA_n28A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257G ","CA_n028A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257G","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257G ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257G","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257G ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257G","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257G ","CA_n079A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257G","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257G ","CA_n079A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","CA_n28A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","CA_n028A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","CA_n28A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","CA_n028A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","CA_n079A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","CA_n079A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257H","CA_n79A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257H ","CA_n079A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n001A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n28A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n028A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n28A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n028A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n28A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n028A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n079A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n079A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n79A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n079A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n28A-n79A-n257I","CA_n79A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n079A_n257I ","CA_n079A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257A","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257A ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257A ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257A","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257A ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257G","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257G ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257G ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257G ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257G","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257G ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257G","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257G ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257G","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257G ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257H","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257H ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257H ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257H ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257H ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257H","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257H ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257H","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257H ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257H","CA_n28A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257H ","CA_n028A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257H","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257H ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257H","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257H ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","CA_n1A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","CA_n001A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","CA_n001A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","CA_n028A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","CA_n28A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","CA_n028A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","CA_n28A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","CA_n028A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n28A-n257I","CA_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n028A_n257I ","CA_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n38A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n038A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n38A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n038A_n078A ","_ ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n40A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n040A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n40A","CA_n1A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n040A ","CA_n001A_n040A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n040A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40A-n78A","CA_n1A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n078A ","CA_n001A_n040A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40A-n78A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40A-n78A","CA_n40A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n078A ","CA_n040A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40A-n78A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n078A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40A-n78A BCS1","CA_n1A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n078A BCS1 ","CA_n001A_n040A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40A-n78A BCS1","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n078A BCS1 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40A-n78A BCS1","CA_n40A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n078A BCS1 ","CA_n040A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40A-n78A BCS2","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n078A BCS2 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40A-n78A BCS2","CA_n1A-n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n078A BCS2 ","CA_n001A_n040A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40A-n78A BCS2","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n078A BCS2 ","CA_n001A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40A-n78A BCS2","CA_n40A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n078A BCS2 ","CA_n040A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n40A-n258A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n258A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n40A-n258D","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n258D ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n40A-n258E","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n258E ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n40A-n258F","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n258F ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n40A-n258G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n258G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n40A-n258H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n258H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n40A-n258I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n258I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n40A-n258J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n258J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n40A-n258K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n258K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n40A-n258L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n258L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n40A-n258M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040A_n258M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n40B","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040B ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n40B-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n040B_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n41A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n041A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n41A","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n041A ","CA_n001A_n041A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n41A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n41A BCS1","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A BCS1 ","CA_n001A_n041A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n41A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n41A-n77A","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n077A ","CA_n001A_n041A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n41A-n77A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n077A ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n41A-n77A","CA_n41A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n077A ","CA_n041A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n41A-n77A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n077A_n257A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n41A-n77A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n077A_n257G ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n41A-n77A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n077A_n257H ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n41A-n77A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n077A_n257I ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n41A-n77(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n077z2Az ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n41A-n77(2A)","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n077z2Az ","CA_n001A_n041A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n41A-n77(2A)","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n077z2Az ","CA_n001A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n41A-n77(2A)","CA_n41A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n077z2Az ","CA_n041A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257A","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257A ","CA_n001A_n041A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257A ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257A","CA_n41A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257A ","CA_n041A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257G","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257G ","CA_n001A_n041A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257G ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257G ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257G","CA_n41A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257G ","CA_n041A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257G","CA_n41A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257G ","CA_n041A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257G","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257G ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257H","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257H ","CA_n001A_n041A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257H ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257H ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257H ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257H","CA_n41A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257H ","CA_n041A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257H","CA_n41A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257H ","CA_n041A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257H","CA_n41A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257H ","CA_n041A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257H","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257H ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257H","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257H ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","CA_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","CA_n001A_n041A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","CA_n001A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","CA_n001A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","CA_n001A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","CA_n001A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","CA_n41A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","CA_n041A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","CA_n41A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","CA_n041A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","CA_n41A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","CA_n041A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","CA_n41A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","CA_n041A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n41A-n257I","CA_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n041A_n257I ","CA_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n67A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n067A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n74A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n074A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n74A","CA_n1A-n74A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n074A ","CA_n001A_n074A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n77A","-","Completed","PC3","<RAN5#94-e","R5-216445","China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n77A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n77A-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n77A-n79A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n77A-n79A","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n77A-n79A","CA_n77A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A ","CA_n077A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257A ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257A","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257A ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257A ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257A","CA_n77A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257A ","CA_n077A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257A","CA_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257A ","CA_n077A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257A","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257A ","CA_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257G","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257G ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257G","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257G ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257G ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257G ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257G","CA_n77A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257G ","CA_n077A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257G","CA_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257G ","CA_n077A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257G","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257G ","CA_n077A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257G","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257G ","CA_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257G","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257G ","CA_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257G","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257G ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n77A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n077A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n077A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n077A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n77A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n077A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n79A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n079A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257H","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257H ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n001A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n77A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n077A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n077A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n077A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n77A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n077A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n77A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n077A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n79A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n079A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n79A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n079A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n77A-n79A-n257I","CA_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n079A_n257I ","CA_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257A ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257A ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257A","CA_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257A ","CA_n077A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257G","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257G ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257G ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257G ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257G","CA_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257G ","CA_n077A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257G","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257G ","CA_n077A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257G","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257G ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257H","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257H ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257H ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257H ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257H ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257H","CA_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257H ","CA_n077A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257H","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257H ","CA_n077A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257H","CA_n77A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257H ","CA_n077A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257H","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257H ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257H","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257H ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","CA_n001A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","CA_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","CA_n077A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","CA_n077A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","CA_n77A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","CA_n077A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","CA_n77A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","CA_n077A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257I","CA_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257I ","CA_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77A-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077A_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n77(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n77(2A)","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az ","CA_n001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n77(2A)-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az_n079A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n77(2A)-n79A","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az_n079A ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n77(2A)-n79A","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az_n079A ","CA_n001A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n77(2A)-n79A","CA_n77A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az_n079A ","CA_n077A_n079A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77(2A)-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77(2A)-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77(2A)-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77(2A)-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77(2A)-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77(2A)-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77(2A)-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n77(2A)-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z2Az_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n77(3A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z3Az ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n77(3A)","CA_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n077z3Az ","CA_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78A","n78 PC2","Completed","PC2","RAN5#96-e","R5-224367","China Telecom","China Telecom",null,"TEI17_test, NR_SAR_PC2_interB_SUL_2BUL-UEConTest","CA_n001A_n078A "," n078 PC002 ",null,"v1.3.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78A","-","Completed","PC3","<RAN5#94-e","R5-216445","China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78A","CA_n1A-n78A","Completed","PC3","<RAN5#94-e","R5-216445","China Unicom","China Unicom (Yu Shi)","RAN5#96-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n078A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78A","CA_n1A-n78A PC2","Ongoing","PC2",null,null,"China Telecom",null,null,"NR_PC2_CA_R17_2BDL_2BUL-UEConTest","CA_n001A_n078A ","CA_n001A_n078A PC002 ",null,"v1.3.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78A BCS1","-","Completed","PC3","<RAN5#94-e","R5-217496","China Unicom","Huawei (Chunying Gu)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78A BCS1","CA_n1A-n78A","Completed","PC3","<RAN5#94-e","R5-217496","China Unicom","Huawei (Chunying Gu)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A BCS1 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78A BCS2","-","Completed","PC3","<RAN5#94-e","R5-217496","China Unicom","Huawei (Chunying Gu)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A BCS2 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78A BCS2","CA_n1A-n78A","Completed","PC3","<RAN5#94-e","R5-217496","China Unicom","Huawei (Chunying Gu)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A BCS2 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78A BCS3","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A BCS3 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78A BCS3","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A BCS3 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n78A-n79A","-","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n78A-n79A","CA_n1A-n78A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n78A-n79A","CA_n1A-n79A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n78A-n79A","CA_n78A-n79A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A ","CA_n078A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n78A-n79A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n78A-n79A BCS1","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A BCS1 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n78A-n79A BCS1","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A BCS1 ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n78A-n79A BCS1","CA_n78A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A BCS1 ","CA_n078A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257A","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257A ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257A ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257A","CA_n78A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257A ","CA_n078A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257A","CA_n78A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257A ","CA_n078A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257A","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257A ","CA_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257G","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257G ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257G","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257G ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257G ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257G ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257G","CA_n78A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257G ","CA_n078A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257G","CA_n78A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257G ","CA_n078A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257G","CA_n78A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257G ","CA_n078A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257G","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257G ","CA_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257G","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257G ","CA_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257G","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257G ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n78A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n078A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n78A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n078A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n78A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n078A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n78A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n078A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n79A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n079A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257H","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257H ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n001A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n78A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n078A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n78A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n078A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n78A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n078A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n78A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n078A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n78A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n078A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n79A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n079A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n79A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n079A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n1A-n78A-n79A-n257I","CA_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n079A_n257I ","CA_n257I ",null,"v1.0.0"]
[null,"Rel-17","SUL FR1 with inter-band CA","38.101-1:Table 5.5C-4","CA_n1A_SUL_n78A-n80A","SUL_n78A-n80A","Completed","PC3","<RAN5#94-e","R5-217496","China Telecom","Chinatelecom (Jing Zhao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n080A ","CA_n078A_n080A ",null,"v1.0.0"]
[null,"Rel-17","SUL FR1 with inter-band CA","38.101-1:Table 5.5C-4","CA_n1A_SUL_n78A-n84A","SUL_n78A-n84A","Completed","PC3","<RAN5#94-e","R5-217496","China Unicom","Huawei (Chunying Gu)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n084A ","CA_n078A_n084A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n078A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257A","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257A ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257A ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257A","CA_n78A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257A ","CA_n078A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257D","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257D ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257E","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257E ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257F","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257F ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257G","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257G ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257G ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257G ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257G","CA_n78A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257G ","CA_n078A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257G","CA_n78A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257G ","CA_n078A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257G","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257G ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257H","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257H ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257H ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257H ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257H ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257H","CA_n78A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257H ","CA_n078A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257H","CA_n78A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257H ","CA_n078A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257H","CA_n78A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257H ","CA_n078A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257H","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257H ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257H","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257H ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","CA_n1A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","CA_n001A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","CA_n78A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","CA_n078A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","CA_n78A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","CA_n078A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","CA_n78A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","CA_n078A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","CA_n78A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","CA_n078A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257I","CA_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257I ","CA_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n258A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n258A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n258D","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n258D ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n258E","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n258E ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n258F","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n258F ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n258G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n258G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n258H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n258H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n258I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n258I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n258J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n258J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n258K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n258K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n258L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n258L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n78A-n258M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078A_n258M ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78C","-","Completed","PC3","<RAN5#94-e","R5-216445","China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n078C ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78C","CA_n1A-n78A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n078C ","CA_n001A_n078A ","Fallback to CA_n1A-n78C BCS1 with UL CA_n1A-n78A","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78C","CA_n78C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078C ","CA_n078C ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78C BCS1","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078C BCS1 ","_ ","Fallback to CA_n1A-n78C BCS1 with UL CA_n1A-n78A","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78C BCS1","CA_n1A-n78A","Ongoing","PC3",null,null,"China Telecom",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078C BCS1 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78C BCS1","CA_n78C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078C BCS1 ","CA_n078C ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78C BCS2","-","Ongoing","PC3",null,null,"China Telecom",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078C BCS2 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78C BCS2","CA_n1A-n78A","Ongoing","PC3",null,null,"China Telecom",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078C BCS2 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78C BCS2","CA_n78C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078C BCS2 ","CA_n078C ",null,"v1.2.0"]
[null,"Rel-17","SUL FR1 with inter-band CA","38.101-1:Table 5.5C-4","CA_n1A_SUL_n78C-n84A","SUL_n78A-n84A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078C_n084A ","CA_n078A_n084A ",null,"v1.0.0"]
[null,"Rel-17","SUL FR1 with inter-band CA","38.101-1:Table 5.5C-4","CA_n1A_SUL_n78C-n84A","SUL_n78C-n84A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078C_n084A ","CA_n078C_n084A ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78(2A)","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n078z2Az ","_ ","Fallback to CA_n1A-n78(2A) BCS1 with UL -","v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78(2A)","CA_n1A-n78A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n078z2Az ","CA_n001A_n078A ","Fallback to CA_n1A-n78(2A) BCS1 with UL CA_n1A-n78A","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78(2A) BCS1","-","Completed","PC3","<RAN5#94-e","R5-217496","China Telecom","Chinatelecom (Jing Zhao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078z2Az BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78(2A) BCS1","CA_n1A-n78A","Completed","PC3","<RAN5#94-e","R5-217496","China Telecom","Chinatelecom (Jing Zhao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078z2Az BCS1 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78(2A) BCS2","-","Completed","PC3","RAN5#94-e","R5-221140","China Telecom","Chinatelecom (Jin Gao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078z2Az BCS2 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n78(2A) BCS2","CA_n1A-n78A","Completed","PC3","RAN5#94-e","R5-221140","China Telecom","Chinatelecom (Jin Gao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078z2Az BCS2 ","CA_n001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1A-n78(2A)-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n078z2Az_n079A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n79A","-","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n079A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n79A","CA_n1A-n79A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n079A ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257A","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257A ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257A ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257A","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257A ","CA_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257G","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257G ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257G ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257G ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257G","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257G ","CA_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257G","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257G ","CA_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257G","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257G ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257H","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257H ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257H ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257H ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257H ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257H","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257H ","CA_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257H","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257H ","CA_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257H","CA_n79A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257H ","CA_n079A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257H","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257H ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257H","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257H ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","CA_n001A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","CA_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","CA_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","CA_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","CA_n79A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","CA_n079A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","CA_n79A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","CA_n079A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n1A-n79A-n257I","CA_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n079A_n257I ","CA_n257I ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n79C","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n079C ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1A-n79C","CA_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n079C ","CA_n001A_n079A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257A","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001A_n257A ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257D","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257D ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257D","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257D ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257D","CA_n1A-n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257D ","CA_n001A_n257D ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257D","CA_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257D ","CA_n257D ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257E","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257E ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257F","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257F ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257G","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257G ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257G","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257G ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257G","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257G ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257H","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257H ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257H","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257H ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257H","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257H ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257H","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257H ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257H","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257H ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257I","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257I ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257I","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257I ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257I","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257I ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257I","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257I ","CA_n001A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257I","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257I ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257I","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257I ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257I","CA_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257I ","CA_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257J","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257J ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257J","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257J ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257J","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257J ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257J","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257J ","CA_n001A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257J","CA_n1A-n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257J ","CA_n001A_n257J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257J","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257J ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257J","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257J ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257J","CA_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257J ","CA_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257J","CA_n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257J ","CA_n257J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257K","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257K ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257K","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257K ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257K","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257K ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257K","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257K ","CA_n001A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257K","CA_n1A-n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257K ","CA_n001A_n257J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257K","CA_n1A-n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257K ","CA_n001A_n257K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257K","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257K ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257K","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257K ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257K","CA_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257K ","CA_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257K","CA_n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257K ","CA_n257J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257K","CA_n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257K ","CA_n257K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257L","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257L ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257L","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257L ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257L","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257L ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257L","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257L ","CA_n001A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257L","CA_n1A-n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257L ","CA_n001A_n257J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257L","CA_n1A-n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257L ","CA_n001A_n257K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257L","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257L ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257L","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257L ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257L","CA_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257L ","CA_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257L","CA_n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257L ","CA_n257J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257L","CA_n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257L ","CA_n257K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257M","CA_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257M ","CA_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257M","CA_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257M ","CA_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257M","CA_n1A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257M ","CA_n001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257M","CA_n1A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257M ","CA_n001A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257M","CA_n1A-n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257M ","CA_n001A_n257J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257M","CA_n1A-n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257M ","CA_n001A_n257K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257M","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257M ","CA_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257M","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257M ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257M","CA_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257M ","CA_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257M","CA_n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257M ","CA_n257J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n257M","CA_n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n257M ","CA_n257K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258A","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258A","CA_n1A-n258A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258A ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258A BCS1","CA_n1A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258A BCS1 ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258B","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258B ","_ ","Fallback to CA_n1A-n258D with UL -","v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258B","CA_n1A-n258A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258B ","CA_n001A_n258A ","Fallback to CA_n1A-n258D with UL CA_n1A-n258A","v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258C","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258C ","_ ","Fallback to CA_n1A-n258D with UL -","v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258C","CA_n1A-n258A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258C ","CA_n001A_n258A ","Fallback to CA_n1A-n258D with UL CA_n1A-n258A","v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258D","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258D ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258D","CA_n1A-n258A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258D ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258D BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258D BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258D BCS1","CA_n1A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258D BCS1 ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258E","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258E ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258E","CA_n1A-n258A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258E ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258E BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258E BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258E BCS1","CA_n1A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258E BCS1 ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258F","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258F ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258F","CA_n1A-n258A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258F ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258F BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258F BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258F BCS1","CA_n1A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258F BCS1 ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258G","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258G","CA_n1A-n258A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258G ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258G","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258G ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258G BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258G BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258G BCS1","CA_n1A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258G BCS1 ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258G BCS1","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258G BCS1 ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258H","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258H","CA_n1A-n258A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258H ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258H","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258H ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258H","CA_n1A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258H ","CA_n001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258H BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258H BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258H BCS1","CA_n1A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258H BCS1 ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258H BCS1","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258H BCS1 ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258H BCS1","CA_n1A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258H BCS1 ","CA_n001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258I","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258I","CA_n1A-n258A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258I ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258I","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258I ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258I","CA_n1A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258I ","CA_n001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258I","CA_n1A-n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258I ","CA_n001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258I BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258I BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258I BCS1","CA_n1A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258I BCS1 ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258I BCS1","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258I BCS1 ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258I BCS1","CA_n1A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258I BCS1 ","CA_n001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258I BCS1","CA_n1A-n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258I BCS1 ","CA_n001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258J","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258J","CA_n1A-n258A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258J ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258J","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258J ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258J","CA_n1A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258J ","CA_n001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258J","CA_n1A-n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258J ","CA_n001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258J BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258J BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258J BCS1","CA_n1A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258J BCS1 ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258J BCS1","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258J BCS1 ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258J BCS1","CA_n1A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258J BCS1 ","CA_n001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258J BCS1","CA_n1A-n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258J BCS1 ","CA_n001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258K","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258K","CA_n1A-n258A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258K ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258K","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258K ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258K","CA_n1A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258K ","CA_n001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258K","CA_n1A-n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258K ","CA_n001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258K BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258K BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258K BCS1","CA_n1A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258K BCS1 ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258K BCS1","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258K BCS1 ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258K BCS1","CA_n1A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258K BCS1 ","CA_n001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258K BCS1","CA_n1A-n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258K BCS1 ","CA_n001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258L","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258L","CA_n1A-n258A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258L ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258L","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258L ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258L","CA_n1A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258L ","CA_n001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258L","CA_n1A-n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258L ","CA_n001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258L BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258L BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258L BCS1","CA_n1A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258L BCS1 ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258L BCS1","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258L BCS1 ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258L BCS1","CA_n1A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258L BCS1 ","CA_n001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258L BCS1","CA_n1A-n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258L BCS1 ","CA_n001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258M","-","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258M","CA_n1A-n258A","Ongoing","PC3",null,null,"China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258M ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258M","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258M ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258M","CA_n1A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258M ","CA_n001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258M","CA_n1A-n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258M ","CA_n001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258M BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258M BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258M BCS1","CA_n1A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258M BCS1 ","CA_n001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258M BCS1","CA_n1A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258M BCS1 ","CA_n001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258M BCS1","CA_n1A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258M BCS1 ","CA_n001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1a","CA_n1A-n258M BCS1","CA_n1A-n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001A_n258M BCS1 ","CA_n001A_n258I ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 IB cont","38.101-1:Table 5.5A.1-1","CA_n1B","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001B ","_ ","Fallback to CA_n1B-n3A with UL -","v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1B-n3A","-","Ongoing","PC3",null,null,"China Telecom",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001B_n003A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1B-n3A","CA_n1A-n3A","Ongoing","PC3",null,null,"China Telecom",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n001B_n003A ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1B-n3A BCS1","-","Ongoing","PC3",null,null,"China Telecom",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001B_n003A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1B-n3A BCS1","CA_n1A-n3A","Ongoing","PC3",null,null,"China Telecom",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001B_n003A BCS1 ","CA_n001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 IB non-cont","38.101-1:Table 5.5A.2-1","CA_n1(2A)","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az ","_ ","Fallback to CA_n1(2A)-n3A with UL -","v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1(2A)-n3A","-","Completed","PC3","RAN5#94-e","R5-221140","China Telecom","Chinatelecom (Jin Gao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n003A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1(2A)-n3A-n7A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n003A_n007A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1(2A)-n3B","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n003B ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1(2A)-n3B-n7A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n003B_n007A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1(2A)-n3(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n003z2Az ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1(2A)-n3(2A)-n7A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n003z2Az_n007A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1(2A)-n5A","-","Completed","PC3","RAN5#94-e","R5-221140","China Telecom","Chinatelecom (Jin Gao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n005A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1(2A)-n7A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n007A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1(2A)-n7A-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n007A_n079A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n1(2A)-n7A-n79C","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n007A_n079C ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1(2A)-n8A","-","Completed","PC3","RAN5#94-e","R5-221140","China Telecom","Chinatelecom (Jin Gao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n008A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1(2A)-n28A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n028A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1(2A)-n38A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n038A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1(2A)-n78A","-","Completed","PC3","RAN5#94-e","R5-221140","China Telecom","Chinatelecom (Jin Gao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1(2A)-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n079A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1a","CA_n1(2A)-n79C","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n001z2Az_n079C ","_ ",null,"v1.1.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n5A","-","Ongoing","PC3",null,null,"AT&T,Verizon","Qualcomm Kevin Wang)","<RAN5#94-e,RAN5#96-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n002A_n005A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n5A","CA_n2A-n5A","Ongoing","PC3",null,null,"Verizon,AT&T","Qualcomm Kevin Wang)","<RAN5#94-e,RAN5#96-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n002A_n005A ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n30A","-","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n30A","CA_n2A-n5A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n30A","CA_n2A-n30A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A ","CA_n002A_n030A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n30A","CA_n5A-n30A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A ","CA_n005A_n030A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66A","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066A ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66A","CA_n2A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066A ","CA_n002A_n030A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66A","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066A ","CA_n002A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66A","CA_n5A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066A ","CA_n005A_n030A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66A","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066A ","CA_n005A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66A","CA_n30A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066A ","CA_n030A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066z2Az ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66(2A)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066z2Az ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66(2A)","CA_n2A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066z2Az ","CA_n002A_n030A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66(2A)","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066z2Az ","CA_n002A_n066A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66(2A)","CA_n5A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066z2Az ","CA_n005A_n030A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66(2A)","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066z2Az ","CA_n005A_n066A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n66(2A)","CA_n30A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n066z2Az ","CA_n030A_n066A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77A","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077A ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77A","CA_n2A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077A ","CA_n002A_n030A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77A","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077A ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77A","CA_n5A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077A ","CA_n005A_n030A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77A","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077A ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77A","CA_n30A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077A ","CA_n030A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077z2Az ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77(2A)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077z2Az ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77(2A)","CA_n2A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077z2Az ","CA_n002A_n030A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77(2A)","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077z2Az ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77(2A)","CA_n5A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077z2Az ","CA_n005A_n030A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77(2A)","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077z2Az ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n30A-n77(2A)","CA_n30A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n030A_n077z2Az ","CA_n030A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48A","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48A","CA_n2A-n5A","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#99","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A ","CA_n002A_n005A ",null,"v1.5.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48A","CA_n2A-n48A","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#99","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A ","CA_n002A_n048A ",null,"v1.5.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48A","CA_n5A-n48A","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#99","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A ","CA_n005A_n048A ",null,"v1.5.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n66A","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n66A BCS1","-","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A BCS1 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n66A BCS1","CA_n2A-n5A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A BCS1 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n66A BCS1","CA_n2A-n48A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A BCS1 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n66A BCS1","CA_n2A-n66A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A BCS1 ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n66A BCS1","CA_n5A-n48A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A BCS1 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n66A BCS1","CA_n5A-n66A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A BCS1 ","CA_n005A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n66A BCS1","CA_n48A-n66A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A BCS1 ","CA_n048A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077A ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77A","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077A ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77A","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077A ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77A","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077A ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77A","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077A ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77A","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077A ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77A","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077A ","CA_n005A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77A","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077A ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77A","CA_n48A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077A ","CA_n048A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77A","CA_n66A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077A ","CA_n066A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77C","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077C ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77C","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077C ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77C","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077C ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77C","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077C ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77C","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077C ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77C","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077C ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77C","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077C ","CA_n005A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77C","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077C ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77C","CA_n48A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077C ","CA_n048A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77C","CA_n66A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077C ","CA_n066A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48A-n66A-n77C","CA_n77C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n066A_n077C ","CA_n077C ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77A","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77A BCS1","-","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077A BCS1 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77A BCS1","CA_n2A-n5A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077A BCS1 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77A BCS1","CA_n2A-n48A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077A BCS1 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77A BCS1","CA_n2A-n77A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077A BCS1 ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77A BCS1","CA_n5A-n48A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077A BCS1 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77A BCS1","CA_n5A-n77A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077A BCS1 ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77C","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077C ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77C","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077C ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77C","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077C ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77C","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077C ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77C","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077C ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77C","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077C ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77C BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077C BCS1 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77C BCS1","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077C BCS1 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77C BCS1","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077C BCS1 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77C BCS1","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077C BCS1 ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77C BCS1","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077C BCS1 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48A-n77C BCS1","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048A_n077C BCS1 ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48B","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48B","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48B","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48B","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48B BCS1","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48B BCS1","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B BCS1 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48B BCS1","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B BCS1 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48B BCS1","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B BCS1 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48B BCS2","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B BCS2 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48B BCS2","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B BCS2 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48B BCS2","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B BCS2 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48B BCS2","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B BCS2 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS1 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS1","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS1 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS1","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS1 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS1","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS1 ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS1","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS1 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS1","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS1 ","CA_n005A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS1","CA_n48A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS1 ","CA_n048A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS2","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS2 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS2","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS2 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS2","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS2 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS2","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS2 ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS2","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS2 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS2","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS2 ","CA_n005A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS2","CA_n48A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS2 ","CA_n048A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS3","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS3 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS3","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS3 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS3","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS3 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS3","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS3 ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS3","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS3 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS3","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS3 ","CA_n005A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n66A BCS3","CA_n48A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A BCS3 ","CA_n048A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48B-n66A-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A_n077A ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48B-n66A-n77A","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A_n077A ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48B-n66A-n77A","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A_n077A ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48B-n66A-n77A","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A_n077A ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48B-n66A-n77A","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A_n077A ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48B-n66A-n77A","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A_n077A ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48B-n66A-n77A","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A_n077A ","CA_n005A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48B-n66A-n77A","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A_n077A ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48B-n66A-n77A","CA_n48A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A_n077A ","CA_n048A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48B-n66A-n77A","CA_n48B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A_n077A ","CA_n048B ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (5 bands)","38.101-1:Table 5.5A.3.4-1","CA_n2A-n5A-n48B-n66A-n77A","CA_n66A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n066A_n077A ","CA_n066A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS1 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS1","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS1 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS1","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS1 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS1","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS1 ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS1","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS1 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS1","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS1 ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS2","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS2 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS2","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS2 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS2","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS2 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS2","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS2 ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS2","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS2 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS2","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS2 ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS3","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS3 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS3","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS3 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS3","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS3 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS3","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS3 ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS3","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS3 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48B-n77A BCS3","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048B_n077A BCS3 ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(2A)","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(2A)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(2A)","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(2A)","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(2A) BCS1","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(2A) BCS1","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az BCS1 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(2A) BCS1","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az BCS1 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(2A) BCS1","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az BCS1 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS1 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS1","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS1 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS1","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS1 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS1","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS1 ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS1","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS1 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS1","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS1 ","CA_n005A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS1","CA_n48A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS1 ","CA_n048A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS2","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS2 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS2","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS2 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS2","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS2 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS2","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS2 ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS2","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS2 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS2","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS2 ","CA_n005A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n66A BCS2","CA_n48A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n066A BCS2 ","CA_n048A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A BCS1 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A BCS1","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A BCS1 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A BCS1","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A BCS1 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A BCS1","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A BCS1 ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A BCS1","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A BCS1 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A BCS1","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A BCS1 ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A BCS2","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A BCS2 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A BCS2","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A BCS2 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A BCS2","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A BCS2 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A BCS2","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A BCS2 ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A BCS2","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A BCS2 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(2A)-n77A BCS2","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048z2Az_n077A BCS2 ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(A-B)","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048zA_Bz ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(A-B)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048zA_Bz ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(A-B)","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048zA_Bz ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(A-B)","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048zA_Bz ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(A-B) BCS1","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048zA_Bz BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(A-B) BCS1","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048zA_Bz BCS1 ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(A-B) BCS1","CA_n2A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048zA_Bz BCS1 ","CA_n002A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n48(A-B) BCS1","CA_n5A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048zA_Bz BCS1 ","CA_n005A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n48(A-B)-n66A","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n048zA_Bz_n066A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n66A","-","Ongoing","PC3",null,null,"AT&T,Verizon,Rogers",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n66A","CA_n2A-n5A","Ongoing","PC3",null,null,"AT&T,Verizon,Rogers",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n66A","CA_n2A-n66A","Ongoing","PC3",null,null,"AT&T,Verizon,Rogers",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A ","CA_n002A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n66A","CA_n5A-n66A","Ongoing","PC3",null,null,"AT&T,Verizon,Rogers",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A ","CA_n005A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77A","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77A","CA_n2A-n5A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077A ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77A","CA_n2A-n66A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077A ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77A","CA_n2A-n77A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077A ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77A","CA_n5A-n66A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077A ","CA_n005A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77A","CA_n5A-n77A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077A ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77A","CA_n66A-n77A","Ongoing","PC3",null,null,"Verizon",null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077A ","CA_n066A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77C","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077C ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77C","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077C ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77C","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077C ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77C","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077C ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77C","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077C ","CA_n005A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77C","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077C ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77C","CA_n66A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077C ","CA_n066A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077z2Az ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77(2A)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077z2Az ","CA_n002A_n005A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77(2A)","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077z2Az ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77(2A)","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077z2Az ","CA_n002A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77(2A)","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077z2Az ","CA_n005A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77(2A)","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077z2Az ","CA_n005A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n5A-n66A-n77(2A)","CA_n66A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066A_n077z2Az ","CA_n066A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n66(2A)","-","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n66(2A)","CA_n2A-n5A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066z2Az ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n66(2A)","CA_n2A-n66A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066z2Az ","CA_n002A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n66(2A)","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066z2Az ","CA_n005A_n066A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n66(3A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066z3Az ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n66(3A)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066z3Az ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n66(3A)","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066z3Az ","CA_n002A_n066A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n66(3A)","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n066z3Az ","CA_n005A_n066A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77A","-","Completed","PC3","RAN5#98","R5-230291","AT&T,Verizon,Rogers","Verizon,Qualcomm (Jinwen Ma,Kevin Wang)","<RAN5#94-e,RAN5#98","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77A","CA_n2A-n5A","Completed","PC3","RAN5#98","R5-230291","AT&T,Verizon,Rogers","Verizon,Qualcomm (Jinwen Ma,Kevin Wang)","RAN5#94-e,RAN5#98","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077A ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77A","CA_n2A-n77A","Completed","PC3","RAN5#98","R5-230291","AT&T,Verizon,Rogers","Verizon,Qualcomm (Jinwen Ma,Kevin Wang)","RAN5#94-e,RAN5#98","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077A ","CA_n002A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77A","CA_n5A-n77A","Completed","PC3","RAN5#98","R5-230291","AT&T,Verizon,Rogers","Verizon,Qualcomm (Jinwen Ma,Kevin Wang)","RAN5#94-e,RAN5#98","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077A ","CA_n005A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77C","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077C ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77C","CA_n2A-n5A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077C ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77C","CA_n2A-n77A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077C ","CA_n002A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77C","CA_n5A-n77A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077C ","CA_n005A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77C BCS1","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077C BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77C BCS1","CA_n2A-n5A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077C BCS1 ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77C BCS1","CA_n2A-n77A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077C BCS1 ","CA_n002A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77C BCS1","CA_n5A-n77A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077C BCS1 ","CA_n005A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77(2A)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077z2Az ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77(2A)","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077z2Az ","CA_n002A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n5A-n77(2A)","CA_n5A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n077z2Az ","CA_n005A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260A","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260A ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260A","CA_n2A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260A ","CA_n002A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260A","CA_n5A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260A ","CA_n005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260G ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260G","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260G ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260G","CA_n2A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260G ","CA_n002A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260G","CA_n2A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260G ","CA_n002A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260G","CA_n5A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260G ","CA_n005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260G","CA_n5A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260G ","CA_n005A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260H","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260H ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260H","CA_n2A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260H ","CA_n002A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260H","CA_n2A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260H ","CA_n002A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260H","CA_n2A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260H ","CA_n002A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260H","CA_n5A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260H ","CA_n005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260H","CA_n5A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260H ","CA_n005A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260H","CA_n5A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260H ","CA_n005A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260I","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260I ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260I","CA_n2A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260I ","CA_n002A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260I","CA_n2A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260I ","CA_n002A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260I","CA_n2A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260I ","CA_n002A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260I","CA_n2A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260I ","CA_n002A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260I","CA_n5A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260I ","CA_n005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260I","CA_n5A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260I ","CA_n005A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260I","CA_n5A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260I ","CA_n005A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260I","CA_n5A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260I ","CA_n005A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260J ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260J","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260J ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260J","CA_n2A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260J ","CA_n002A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260J","CA_n2A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260J ","CA_n002A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260J","CA_n2A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260J ","CA_n002A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260J","CA_n2A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260J ","CA_n002A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260J","CA_n2A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260J ","CA_n002A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260J","CA_n5A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260J ","CA_n005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260J","CA_n5A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260J ","CA_n005A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260J","CA_n5A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260J ","CA_n005A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260J","CA_n5A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260J ","CA_n005A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260J","CA_n5A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260J ","CA_n005A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n2A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n002A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n2A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n002A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n2A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n002A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n2A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n002A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n2A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n002A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n2A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n002A_n260K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n5A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n5A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n005A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n5A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n005A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n5A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n005A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n5A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n005A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260K","CA_n5A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260K ","CA_n005A_n260K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n002A_005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n2A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n002A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n2A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n002A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n2A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n002A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n2A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n002A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n2A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n002A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n2A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n002A_n260K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n2A-n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n002A_n260L ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n5A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n5A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n005A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n5A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n005A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n5A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n005A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n5A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n005A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n5A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n005A_n260K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260L","CA_n5A-n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260L ","CA_n005A_n260L ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n2A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n002A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n2A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n002A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n2A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n002A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n2A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n002A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n2A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n002A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n2A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n002A_n260K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n2A-n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n002A_n260L ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n2A-n260M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n002A_n260M ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n5A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n5A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n005A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n5A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n005A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n5A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n005A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n5A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n005A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n5A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n005A_n260K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n5A-n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n005A_n260L ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n260M","CA_n5A-n260M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n260M ","CA_n005A_n260M ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261A","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261A ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261A","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261A ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261A","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261A ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261G ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261G","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261G ","CA_n002A_n005A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261G","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261G ","CA_n002A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261G","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261G ","CA_n002A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261G","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261G ","CA_n005A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261G","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261G ","CA_n005A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261H ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261H","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261H ","CA_n002A_n005A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261H","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261H ","CA_n002A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261H","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261H ","CA_n002A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261H","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261H ","CA_n002A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261H","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261H ","CA_n005A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261H","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261H ","CA_n005A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261H","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261H ","CA_n005A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261I ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261I","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261I ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261I","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261I ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261I","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261I ","CA_n002A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261I","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261I ","CA_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261I","CA_n2A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261I ","CA_n002A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261I","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261I ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261I","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261I ","CA_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261I","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261I ","CA_n005A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261I","CA_n5A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261I ","CA_n005A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261J ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261J","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261J ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261J","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261J ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261J","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261J ","CA_n002A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261J","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261J ","CA_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261J","CA_n2A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261J ","CA_n002A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261J","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261J ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261J","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261J ","CA_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261J","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261J ","CA_n005A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261J","CA_n5A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261J ","CA_n005A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261K ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261K","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261K ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261K","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261K ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261K","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261K ","CA_n002A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261K","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261K ","CA_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261K","CA_n2A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261K ","CA_n002A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261K","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261K ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261K","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261K ","CA_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261K","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261K ","CA_n005A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261K","CA_n5A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261K ","CA_n005A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261L ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261L","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261L ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261L","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261L ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261L","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261L ","CA_n002A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261L","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261L ","CA_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261L","CA_n2A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261L ","CA_n002A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261L","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261L ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261L","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261L ","CA_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261L","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261L ","CA_n005A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261L","CA_n5A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261L ","CA_n005A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261M ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261M","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261M ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261M","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261M ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261M","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261M ","CA_n002A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261M","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261M ","CA_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261M","CA_n2A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261M ","CA_n002A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261M","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261M ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261M","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261M ","CA_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261M","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261M ","CA_n005A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261M","CA_n5A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261M ","CA_n005A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-G)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Gz ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-G)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Gz ","CA_n002A_n005A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-G)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Gz ","CA_n002A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-G)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Gz ","CA_n002A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-G)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Gz ","CA_n005A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-G)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Gz ","CA_n005A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-H)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Hz ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-H)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Hz ","CA_n002A_n005A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-H)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Hz ","CA_n002A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-H)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Hz ","CA_n002A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-H)","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Hz ","CA_n002A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-H)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Hz ","CA_n005A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-H)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Hz ","CA_n005A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-H)","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Hz ","CA_n005A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-I)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Iz ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-I)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Iz ","CA_n002A_n005A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-I)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Iz ","CA_n002A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-I)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Iz ","CA_n002A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-I)","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Iz ","CA_n002A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-I)","CA_n2A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Iz ","CA_n002A_n261I ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-I)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Iz ","CA_n005A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-I)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Iz ","CA_n005A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-I)","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Iz ","CA_n005A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A-I)","CA_n5A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2A_Iz ","CA_n005A_n261I ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Az ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Az ","CA_n002A_n005A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Az ","CA_n002A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2A)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Az ","CA_n005A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2G)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Gz ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2G)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Gz ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2G)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Gz ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2G)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Gz ","CA_n002A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2G)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Gz ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2G)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Gz ","CA_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2H)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Hz ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2H)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Hz ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2H)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Hz ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2H)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Hz ","CA_n002A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2H)","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Hz ","CA_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2H)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Hz ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2H)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Hz ","CA_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(2H)","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z2Hz ","CA_n005A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(3A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z3Az ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(3A)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z3Az ","CA_n002A_n005A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(3A)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z3Az ","CA_n002A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(3A)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261z3Az ","CA_n005A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-H)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Hz ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-H)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Hz ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-H)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Hz ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-H)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Hz ","CA_n002A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-H)","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Hz ","CA_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-H)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Hz ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-H)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Hz ","CA_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-H)","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Hz ","CA_n005A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-I)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Iz ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-I)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Iz ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-I)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Iz ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-I)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Iz ","CA_n002A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-I)","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Iz ","CA_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-I)","CA_n2A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Iz ","CA_n002A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-I)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Iz ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-I)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Iz ","CA_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-I)","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Iz ","CA_n005A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G-I)","CA_n5A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_G_Iz ","CA_n005A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Gz ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Gz ","CA_n002A_n005A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Gz ","CA_n002A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Gz ","CA_n002A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Gz ","CA_n005A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-G)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Gz ","CA_n005A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-H)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Hz ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-H)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Hz ","CA_n002A_n005A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-H)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Hz ","CA_n002A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-H)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Hz ","CA_n002A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-H)","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Hz ","CA_n002A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-H)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Hz ","CA_n005A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-H)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Hz ","CA_n005A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-H)","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Hz ","CA_n005A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-I)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Iz ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-I)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Iz ","CA_n002A_n005A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-I)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Iz ","CA_n002A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-I)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Iz ","CA_n002A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-I)","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Iz ","CA_n002A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-I)","CA_n2A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Iz ","CA_n002A_n261I ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-I)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Iz ","CA_n005A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-I)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Iz ","CA_n005A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-I)","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Iz ","CA_n005A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(A-I)","CA_n5A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zA_Iz ","CA_n005A_n261I ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-H)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Hz ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-H)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Hz ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-H)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Hz ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-H)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Hz ","CA_n002A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-H)","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Hz ","CA_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-H)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Hz ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-H)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Hz ","CA_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-H)","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Hz ","CA_n005A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-I)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Iz ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-I)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Iz ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-I)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Iz ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-I)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Iz ","CA_n002A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-I)","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Iz ","CA_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-I)","CA_n2A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Iz ","CA_n002A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-I)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Iz ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-I)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Iz ","CA_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-I)","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Iz ","CA_n005A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(G-I)","CA_n5A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zG_Iz ","CA_n005A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(H-I)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zH_Iz ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(H-I)","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zH_Iz ","CA_n002A_n005A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(H-I)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zH_Iz ","CA_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(H-I)","CA_n2A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zH_Iz ","CA_n002A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(H-I)","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zH_Iz ","CA_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(H-I)","CA_n2A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zH_Iz ","CA_n002A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(H-I)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zH_Iz ","CA_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(H-I)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zH_Iz ","CA_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(H-I)","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zH_Iz ","CA_n005A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n5A-n261(H-I)","CA_n5A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005A_n261zH_Iz ","CA_n005A_n261I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n5B","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005B ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n5B","CA_n2A-n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005B ","CA_n002A_n005A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n5B","CA_n5B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n005B ","CA_n005B ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n7A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n007A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n7A","CA_n2A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n007A ","CA_n002A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n7(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n007z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n7(2A)","CA_n2A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n007z2Az ","CA_n002A_n007A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n12A","-","Ongoing","PC3",null,null,"AT&T,Rogers",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n12A","CA_n2A-n12A","Ongoing","PC3",null,null,"AT&T,Rogers",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A ","CA_n002A_n012A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n12A-n30A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n030A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n12A-n30A","CA_n2A-n12A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n030A ","CA_n002A_n012A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n12A-n30A","CA_n2A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n030A ","CA_n002A_n030A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n12A-n30A","CA_n12A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n030A ","CA_n012A_n030A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n12A-n30A-n66A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n030A_n066A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n12A-n30A-n66A","CA_n2A-n12A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n030A_n066A ","CA_n002A_n012A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n12A-n30A-n66A","CA_n2A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n030A_n066A ","CA_n002A_n030A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n12A-n30A-n66A","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n030A_n066A ","CA_n002A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n12A-n30A-n66A","CA_n12A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n030A_n066A ","CA_n012A_n030A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n12A-n30A-n66A","CA_n12A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n030A_n066A ","CA_n012A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n12A-n30A-n66A","CA_n30A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n030A_n066A ","CA_n030A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n12A-n66A-n77A","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n066A_n077A ","CA_n002A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n12A-n260I","CA_n12A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n260I ","CA_n012A_n260A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n12A-n260K","CA_n12A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n012A_n260K ","CA_n012A_n260G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n14A-n30A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n014A_n030A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n14A-n77(2A)","CA_n14A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n014A_n077z2Az ","CA_n014A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n14A-n260I","CA_n14A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n014A_n260I ","CA_n014A_n260A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n14A-n260L","CA_n14A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n014A_n260L ","CA_n014A_n260H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n29A-n30A","CA_n2A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n029A_n030A ","CA_n002A_n030A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n30A-n77A","CA_n2A-n77A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n030A_n077A ","CA_n002A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n30A-n260L","CA_n30A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n030A_n260L ","CA_n030A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n38A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n038A ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n48B-n66A","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n048B_n066A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2A-n48B-n66A-n77A BCS3","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n048B_n066A_n077A BCS3 ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n2A-n66A-n77A","-","Completed","PC3","RAN5#98","R5-230292","AT&T,Verizon","Verizon,Qualcomm (Jinwen Ma,Kevin Wang)","<RAN5#94-e,RAN5#98","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n066A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n66A-n260I","CA_n2A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n066A_n260I ","CA_n002A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n66A-n260K","CA_n66A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n066A_n260K ","CA_n066A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n66A-n261A","CA_n2A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n066A_n261A ","CA_n002A_n066A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n66A-n261I","CA_n66A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n066A_n261I ","CA_n066A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n66A-n261(2A-I)","CA_n66A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n066A_n261z2A_Iz ","CA_n066A_n261I ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n66A-n261(A-G-I)","CA_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n066A_n261zA_G_Iz ","CA_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n66A-n261(A-I)","CA_n2A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n066A_n261zA_Iz ","CA_n002A_n261I ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2A-n66(3A)","-","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n066z3Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n77A-n260L","CA_n2A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n077A_n260L ","CA_n002A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n77A-n260M","CA_n77A-n260A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n077A_n260M ","CA_n077A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n77A-n261K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n077A_n261K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n2A-n77A-n261M","CA_n77A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n077A_n261M ","CA_n077A_n261H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1b","CA_n2A-n260M","CA_n2A-n260K","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n260M ","CA_n002A_n260K ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1b","CA_n2A-n261(2A-H)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n261z2A_Hz ","CA_n002A_n261A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1b","CA_n2A-n261(4A)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n261z4Az ","CA_n002A_n261A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1b","CA_n2A-n261(G-H)","CA_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002A_n261zG_Hz ","CA_n002A_n261A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n2(2A)-n5A-n30A-n66A","CA_n5A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002z2Az_n005A_n030A_n066A ","CA_n005A_n030A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2(2A)-n29A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002z2Az_n029A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1b","CA_n2(2A)-n77A","CA_n2A-n77A PC2","Pending","PC2",null,null,null,null,null,"NR_PC2_CA_R17_2BDL_2BUL-UEConTest","CA_n002z2Az_n077A ","CA_n002A_n077A PC002 ",null,"v1.3.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1b","CA_n2(2A)-n260L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002z2Az_n260L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1b","CA_n2(2A)-n260M","CA_n2A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n002z2Az_n260M ","CA_n002A_n260H ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1c","CA_n3A-n7A","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n003A_n007A ","_ ","Fallback to CA_n1A-n3A-n7A with UL -","v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n7A-n78A-n258E","CA_n3A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007A_n078A_n258E ","CA_n003A_n258A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n7A-n78A-n258I","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007A_n078A_n258I ","CA_n007A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n7A-n78A-n258K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007A_n078A_n258K ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n7A-n78A-n258L","CA_n7A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007A_n078A_n258L ","CA_n007A_n258G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n7A-n258D","CA_n3A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007A_n258D ","CA_n003A_n258A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n7A-n258M","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007A_n258M ","CA_n003A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n7B-n78A-n258A","CA_n7A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007B_n078A_n258A ","CA_n007A_n258A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n7B-n78A-n258E","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007B_n078A_n258E ","CA_n003A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n7B-n78A-n258J","CA_n78A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007B_n078A_n258J ","CA_n078A_n258H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n7B-n78A-n258M","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007B_n078A_n258M ","CA_n007A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n7B-n258D","CA_n3A-n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007B_n258D ","CA_n003A_n007A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n7B-n258H","CA_n3A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007B_n258H ","CA_n003A_n258H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n7B-n258L","CA_n3A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n007B_n258L ","CA_n003A_n258G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n3A-n18A-n28A-n41A","CA_n18A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n018A_n028A_n041A ","CA_n018A_n028A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n3A-n28A-n41A","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n028A_n041A ","CA_n003A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n3A-n28A-n41A-n78A","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n028A_n041A_n078A ","CA_n003A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n28A-n41A-n257G","CA_n28A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n028A_n041A_n257G ","CA_n028A_n041A ",null,"v1.1.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n3A-n28A-n77A","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n003A_n028A_n077A ","CA_n028A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n3A-n28A-n77A-n79A-n257I","CA_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n028A_n077A_n079A_n257I ","CA_n028A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n28A-n77A-n257H","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n028A_n077A_n257H ","CA_n028A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n3A-n28A-n77(2A)","CA_n77(2A)","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n028A_n077z2Az ","CA_n077z2Az ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n3A-n28A-n77(2A)-n79A-n257G","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n028A_n077z2Az_n079A_n257G ","CA_n003A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (5 bands)","38.101-3:Table 5.5A.1-4","CA_n3A-n28A-n77(2A)-n79A-n257I","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n028A_n077z2Az_n079A_n257I ","CA_n028A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n3A-n28A-n78A BCS2","CA_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n028A_n078A BCS2 ","CA_n003A_n028A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n28A-n78A-n257I","CA_n3A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n028A_n078A_n257I ","CA_n003A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n28A-n79A-n257G","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n028A_n079A_n257G ","CA_n028A_n257A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n28A-n257I","CA_n28A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n003A_n028A_n257I ","CA_n028A_n257H ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n28A-n257I","CA_n28A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n003A_n028A_n257I ","CA_n028A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n41A-n77A-n257I","CA_n41A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n041A_n077A_n257I ","CA_n041A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n41A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n041A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n77A-n79A-n257A","CA_n77A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n077A_n079A_n257A ","CA_n077A_n079A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n77A-n257H","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n003A_n077A_n257H ","CA_n077A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n77(2A)-n79A-n257A","CA_n3A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n077z2Az_n079A_n257A ","CA_n003A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n3A-n77(2A)-n79A-n257I","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n077z2Az_n079A_n257I ","CA_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n77(2A)-n257H","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n003A_n077z2Az_n257H ","CA_n077A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n77(3A)-n257H","CA_n77A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n077z3Az_n257H ","CA_n077A_n257H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n78A-n258D","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n078A_n258D ","CA_n003A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n78A-n258I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n078A_n258I ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n3A-n78A-n258M","CA_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n078A_n258M ","CA_n003A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1c","CA_n3A-n79A BCS1","CA_n3A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n079A BCS1 ","CA_n003A_n079A ",null,"v1.1.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1c","CA_n3A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n003A_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1c","CA_n3A-n258F","CA_n3A-n258E","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n258F ","CA_n003A_n258E ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1c","CA_n3A-n258L","CA_n3A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003A_n258L ","CA_n003A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1c","CA_n3(2A)-n38A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n003z2Az_n038A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n5A-n7A-n28A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n007A_n028A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n5A-n25A-n66A-n78A","CA_n66A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n025A_n066A_n078A ","CA_n066A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n5A-n25A-n77A","CA_n5A-n25A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n025A_n077A ","CA_n005A_n025A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n5A-n25(2A)-n66A-n77A","CA_n25A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n025z2Az_n066A_n077A ","CA_n025A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n5A-n25(2A)-n66(2A)-n77(2A)","CA_n66A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n025z2Az_n066z2Az_n077z2Az ","CA_n066A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n5A-n30A-n77A","-","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n030A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n30A-n260H","CA_n30A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n030A_n260H ","CA_n030A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n30A-n260L","CA_n5A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n030A_n260L ","CA_n005A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n30A-n260M","CA_n30A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n030A_n260M ","CA_n030A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n5A-n48B-n66A-n77A BCS2","CA_n48A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n048B_n066A_n077A BCS2 ","CA_n048A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n5A-n48(2A)-n66A-n77A","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n048z2Az_n066A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n5A-n48(2A)-n77C BCS2","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n048z2Az_n077C BCS2 ","_ ",null,"v1.1.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n5A-n66A-n78A","CA_n66A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n005A_n066A_n078A ","CA_n066A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n66A-n260H","CA_n66A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n066A_n260H ","CA_n066A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n66A-n260M","CA_n66A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n066A_n260M ","CA_n066A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n66A-n261J","CA_n66A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n066A_n261J ","CA_n066A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n66A-n261M","CA_n5A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n066A_n261M ","CA_n005A_n066A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n66A-n261(2A)","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n066A_n261z2Az ","CA_n005A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n66A-n261(A-G-H)","CA_n66A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n066A_n261zA_G_Hz ","CA_n066A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1d","CA_n5A-n66(2A)","CA_n5A-n66A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n066z2Az ","CA_n005A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n77A-n260H","CA_n77A-n260A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n077A_n260H ","CA_n077A_n260A ","Fallback to CA_n5A-n77A-n260I with UL CA_n77A-n260A","v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n77A-n260I","CA_n77A-n260H","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n077A_n260I ","CA_n077A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n77A-n261I","CA_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n077A_n261I ","CA_n005A_n261A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n5A-n77A-n261I","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n077A_n261I ","CA_n005A_n261G ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1d","CA_n5A-n78C","CA_n5A-n78A","Ongoing","PC3",null,null,"China Telecom",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n005A_n078C ","CA_n005A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1d","CA_n5A-n260L","CA_n5A-n260J","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n260L ","CA_n005A_n260J ","Fallback to CA_n5A-n260L with UL CA_n5A-n260K","v1.2.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1d","CA_n5A-n260(3A)","CA_n5A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n005A_n260z3Az ","CA_n005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1d","CA_n5A-n261(2A-H)","CA_n5A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n261z2A_Hz ","CA_n005A_n261H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1d","CA_n5A-n261(A-G)","CA_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n261zA_Gz ","CA_n005A_n261G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1d","CA_n5A-n261(G-H)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n005A_n261zG_Hz ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1d","CA_n5(2A)-n77A","n77 PC2","Pending","PC2",null,null,null,null,null,"NR_PC2_CA_R17_2BDL_2BUL-UEConTest","CA_n005z2Az_n077A "," n077 PC002 ",null,"v1.3.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n7A-n8A-n78A","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007A_n008A_n078A ","CA_n007A_n078A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n7A-n25A-n66(2A)-n78(2A)","CA_n25A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007A_n025A_n066z2Az_n078z2Az ","CA_n025A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n7A-n25(2A)-n66A-n77(2A)","CA_n25A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007A_n025z2Az_n066A_n077z2Az ","CA_n025A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n7A-n25(2A)-n66(2A)-n77A","CA_n25A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007A_n025z2Az_n066z2Az_n077A ","CA_n025A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n7A-n25(2A)-n77A","CA_n7A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007A_n025z2Az_n077A ","CA_n007A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n7A-n46D-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007A_n046D_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n7A-n78A-n258B","CA_n78A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007A_n078A_n258B ","CA_n078A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n7A-n78A-n258H","CA_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007A_n078A_n258H ","CA_n007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n7A-n78A-n258J","CA_n78A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007A_n078A_n258J ","CA_n078A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n7A-n78A-n258L","CA_n7A-n258L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007A_n078A_n258L ","CA_n007A_n258L ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1e","CA_n7A-n257J","CA_n7A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007A_n257J ","CA_n007A_n257A ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n7B-n28A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n007B_n028A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n7B-n78A-n258C","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007B_n078A_n258C ","CA_n007B ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n7B-n78A-n258G","CA_n78A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007B_n078A_n258G ","CA_n078A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n7B-n78A-n258M","CA_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007B_n078A_n258M ","CA_n007B ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1e","CA_n7B-n258G","CA_n7A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007B_n258G ","CA_n007A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1e","CA_n7B-n258M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007B_n258M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n7(2A)-n25A-n66A-n77(2A)","CA_n66A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007z2Az_n025A_n066A_n077z2Az ","CA_n066A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n7(2A)-n25A-n66(2A)-n78(2A)","CA_n7A-n25A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007z2Az_n025A_n066z2Az_n078z2Az ","CA_n007A_n025A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n7(2A)-n25(2A)-n66(2A)-n77(2A)","CA_n25A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007z2Az_n025z2Az_n066z2Az_n077z2Az ","CA_n025A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n7(2A)-n66A-n78(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007z2Az_n066A_n078z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1e","CA_n7(2A)-n77(2A)","CA_n7A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n007z2Az_n077z2Az ","CA_n007A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n8A-n40A-n41A","CA_n8A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n008A_n040A_n041A ","CA_n008A_n041A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n8A-n78A-n257H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n008A_n078A_n257H ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1e","CA_n8A-n257K","CA_n8A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n008A_n257K ","CA_n008A_n257H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n12A-n30A-n260A","CA_n12A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n012A_n030A_n260A ","CA_n012A_n260A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n12A-n30A-n260K","CA_n12A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n012A_n030A_n260K ","CA_n012A_n260G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n12A-n30A-n260L","CA_n30A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n012A_n030A_n260L ","CA_n030A_n260K ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n12A-n66A-n260H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n012A_n066A_n260H ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n12A-n66A-n260M","CA_n12A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n012A_n066A_n260M ","CA_n012A_n260I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1f","CA_n12A-n77A","CA_n12A-n77A","Ongoing","PC3",null,null,"AT&T,Rogers",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n012A_n077A ","CA_n012A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n12A-n77A-n260J","CA_n77A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n012A_n077A_n260J ","CA_n077A_n260J ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n12A-n77A-n260L","CA_n77A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n012A_n077A_n260L ","CA_n077A_n260G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1f","CA_n12A-n260I","CA_n12A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n012A_n260I ","CA_n012A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n14A-n30A-n66A","CA_n14A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n014A_n030A_n066A ","CA_n014A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n14A-n30A-n77A","CA_n14A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n014A_n030A_n077A ","CA_n014A_n030A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n14A-n30A-n260J","CA_n14A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n014A_n030A_n260J ","CA_n014A_n260J ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n14A-n66A-n260A","CA_n14A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n014A_n066A_n260A ","CA_n014A_n066A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n14A-n66A-n260I","CA_n66A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n014A_n066A_n260I ","CA_n066A_n260H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n14A-n66A-n260L","CA_n66A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n014A_n066A_n260L ","CA_n066A_n260J ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n14A-n66(2A)-n77A","CA_n14A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n014A_n066z2Az_n077A ","CA_n014A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n14A-n77A-n260J","CA_n14A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n014A_n077A_n260J ","CA_n014A_n260H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1f","CA_n14A-n260G","CA_n14A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n014A_n260G ","CA_n014A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1f","CA_n14A-n260L","CA_n14A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n014A_n260L ","CA_n014A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n18A-n41A-n77A","CA_n41A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n018A_n041A_n077A ","CA_n041A_n077A ",null,"v1.4.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1g","CA_n20A-n78A","-","Ongoing","PC3",null,null,"Orange","Nokia (Tuomo Saynajakangas)","RAN5#97,RAN5#98","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n020A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1g","CA_n24A-n77C","CA_n24A-n77A","Ongoing","PC3",null,null,"Ligado","Ligado (Ojas Choksi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n024A_n077C ","CA_n024A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n25A-n38A-n66(2A)-n78(2A)","CA_n25A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n038A_n066z2Az_n078z2Az ","CA_n025A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n25A-n41A-n66A BCS1","CA_n41A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n041A_n066A BCS1 ","CA_n041A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n25A-n41A-n66A-n77(2A) BCS4and5","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n041A_n066A_n077z2Az BCS4and005 ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n25A-n41A-n66(2A) BCS1","CA_n41A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n041A_n066z2Az BCS1 ","CA_n041A_n066A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n25A-n41A-n77(2A) BCS4and5","CA_n25A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n041A_n077z2Az BCS4and005 ","CA_n025A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n25A-n41C-n66A BCS1","CA_n41A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n041C_n066A BCS1 ","CA_n041A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n25A-n41C-n66A-n77A","CA_n25A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n041C_n066A_n077A ","CA_n025A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n25A-n41C-n77A","CA_n25A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n041C_n077A ","CA_n025A_n077A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n25A-n41(2A)-n71A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n025A_n041z2Az_n071A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n25A-n41(2A)-n77A","CA_n25A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n041z2Az_n077A ","CA_n025A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1g","CA_n25A-n48C","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n048C ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n25A-n48(2A)-n66A BCS1","CA_n48A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n048z2Az_n066A BCS1 ","CA_n048A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n25A-n66A-n77A BCS4and5","CA_n25A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n066A_n077A BCS4and005 ","CA_n025A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n25A-n66(2A)-n71A-n78A","CA_n66A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n066z2Az_n071A_n078A ","CA_n066A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n25A-n66(2A)-n78(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n066z2Az_n078z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1g","CA_n25A-n71(2A)","CA_n25A-n71A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n071z2Az ","CA_n025A_n071A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1g","CA_n25A-n77(2A)","CA_n25A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n077z2Az ","CA_n025A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1g","CA_n25A-n260(5A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025A_n260z5Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n25(2A)-n38A-n66(2A)-n78A","CA_n25A-n38A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025z2Az_n038A_n066z2Az_n078A ","CA_n025A_n038A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1g","CA_n25(2A)-n41A","CA_n25A-n41A PC2","Pending","PC2",null,null,null,null,null,"NR_PC2_CA_R17_2BDL_2BUL-UEConTest","CA_n025z2Az_n041A ","CA_n025A_n041A PC002 ",null,"v1.3.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n25(2A)-n41A-n77A","CA_n25A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025z2Az_n041A_n077A ","CA_n025A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n25(2A)-n66A-n77A","CA_n66A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n025z2Az_n066A_n077A ","CA_n066A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1g","CA_n25(2A)-n77A","CA_n25A-n77A PC2","Pending","PC2",null,null,null,null,null,"NR_PC2_CA_R17_2BDL_2BUL-UEConTest","CA_n025z2Az_n077A ","CA_n025A_n077A PC002 ",null,"v1.3.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n28A-n39A-n41A","CA_n28A-n39A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n028A_n039A_n041A ","CA_n028A_n039A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n28A-n40A-n79A","CA_n40A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n028A_n040A_n079A ","CA_n040A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n28A-n41A-n77A-n257G","CA_n41A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n028A_n041A_n077A_n257G ","CA_n041A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n28A-n41A-n257I","CA_n28A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n028A_n041A_n257I ","CA_n028A_n257I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n28A-n77A-n79A-n257G","CA_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n028A_n077A_n079A_n257G ","CA_n257G ",null,"v1.1.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n28A-n77A-n257D","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n028A_n077A_n257D ","CA_n028A_n257A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n28A-n77A-n257I","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n028A_n077A_n257I ","CA_n077A_n257G ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n28A-n77(2A)-n257D","CA_n77A-n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n028A_n077z2Az_n257D ","CA_n077A_n257D ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n28A-n77(3A)-n257H","CA_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n028A_n077z3Az_n257H ","CA_n028A_n257G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n28A-n78A-n79A-n257A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n028A_n078A_n079A_n257A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (4 bands)","38.101-3:Table 5.5A.1-3","CA_n28A-n78A-n79A-n257H","CA_n78A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n028A_n078A_n079A_n257H ","CA_n078A_n257G ",null,"v1.1.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n28A-n78A-n257H","CA_n28A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n028A_n078A_n257H ","CA_n028A_n257H ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1h","CA_n28A-n257A","CA_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n028A_n257A ","CA_n028A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n29A-n66A-n77(2A)","CA_n66A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n029A_n066A_n077z2Az ","CA_n066A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n30A-n66A-n77(2A)","CA_n30A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n030A_n066A_n077z2Az ","CA_n030A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n30A-n66A-n260I","CA_n30A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n030A_n066A_n260I ","CA_n030A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n30A-n66A-n260L","CA_n66A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n030A_n066A_n260L ","CA_n066A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n30A-n77A-n260J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n030A_n077A_n260J ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n30A-n77A-n260L","CA_n77A-n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n030A_n077A_n260L ","CA_n077A_n260L ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1h","CA_n30A-n260A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n030A_n260A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1h","CA_n30A-n260K","CA_n30A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n030A_n260K ","CA_n030A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n38A-n66A-n78(2A)","CA_n38A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n038A_n066A_n078z2Az ","CA_n038A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1h","CA_n38A-n258I","CA_n38A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n038A_n258I ","CA_n038A_n258A ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n40A-n41A-n79A","CA_n40A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n040A_n041A_n079A ","CA_n040A_n079A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40A-n77A-n257I","CA_n40A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040A_n077A_n257I ","CA_n040A_n257A ",null,"v1.1.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1i","CA_n40A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n040A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1i","CA_n40A-n78A","CA_n40A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n040A_n078A ","CA_n040A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40A-n78A-n257J","CA_n40A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040A_n078A_n257J ","CA_n040A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40A-n78A-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040A_n078A_n257L ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40A-n78A-n258H","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040A_n078A_n258H ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40A-n78C-n257I","CA_n78A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040A_n078C_n257I ","CA_n078A_n257H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40A-n78C-n257K","CA_n78A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040A_n078C_n257K ","CA_n078A_n257G ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1i","CA_n40A-n78(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n040A_n078z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40A-n78(2A)-n257F","CA_n40A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040A_n078z2Az_n257F ","CA_n040A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40A-n78(2A)-n257J","CA_n40A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040A_n078z2Az_n257J ","CA_n040A_n257I ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1i","CA_n40A-n257D","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040A_n257D ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1i","CA_n40A-n258E","CA_n40A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040A_n258E ","CA_n040A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40B-n77A-n257G","CA_n77A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040B_n077A_n257G ","CA_n077A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1i","CA_n40B-n77C","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040B_n077C ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40B-n77C-n257L","CA_n77A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040B_n077C_n257L ","CA_n077A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40B-n78A-n257I","CA_n78A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040B_n078A_n257I ","CA_n078A_n257G ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40B-n78A-n257K","CA_n78A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040B_n078A_n257K ","CA_n078A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40B-n78A-n257M","CA_n78A-n257M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040B_n078A_n257M ","CA_n078A_n257M ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40B-n78C-n257F","CA_n40B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040B_n078C_n257F ","CA_n040B ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40B-n78C-n257L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040B_n078C_n257L ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40B-n78(2A)-n257A","CA_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040B_n078z2Az_n257A ","CA_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40B-n78(2A)-n257F","CA_n78A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040B_n078z2Az_n257F ","CA_n078A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n40B-n78(2A)-n257J","CA_n78A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040B_n078z2Az_n257J ","CA_n078A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1i","CA_n40B-n257F","CA_n40B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n040B_n257F ","CA_n040B ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1j","CA_n41A-n48B","CA_n41A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n048B ","CA_n041A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n41A-n66A-n71A-n77A BCS4and5","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n066A_n071A_n077A BCS4and005 ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n41A-n66A-n71A-n78A","CA_n66A-n71A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n066A_n071A_n078A ","CA_n066A_n071A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n41A-n66A-n260H","CA_n41A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n066A_n260H ","CA_n041A_n260H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n41A-n66(2A)-n71A-n77A BCS4and5","CA_n41A-n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n066z2Az_n071A_n077A BCS4and005 ","CA_n041A_n066A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n41A-n66(2A)-n71A-n78(2A)","CA_n66A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n066z2Az_n071A_n078z2Az ","CA_n066A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n41A-n71A-n77A","-","Ongoing","PC3",null,null,"Rogers",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n071A_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1j","CA_n41A-n71B BCS4and5","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n071B BCS4and005 ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n41A-n77A-n257H","CA_n41A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n077A_n257H ","CA_n041A_n257H ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1j","CA_n41A-n78(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n078z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","SUL FR1","38.101-1:Table 5.5C-1","SUL_n41A-n98A","SUL_n41A-n98A","Pending","PC3",null,null,null,"CMCC (Luyang Zhao)",null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n098A ","CA_n041A_n098A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1j","CA_n41A-n258(A-H)","CA_n41A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n258zA_Hz ","CA_n041A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1j","CA_n41A-n260(6A)","CA_n41A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041A_n260z6Az ","CA_n041A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (4 bands)","38.101-1:Table 5.5A.3.3-1","CA_n41C-n66A-n71A-n77A BCS4and5","CA_n41C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041C_n066A_n071A_n077A BCS4and005 ","CA_n041C ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n41C-n71A-n77A BCS4and5","CA_n41C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041C_n071A_n077A ","_ ",null,"v1.5.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1j","CA_n41C-n71(2A)","n41 PC1.5","Pending","PC1.5",null,null,null,null,null,"NR_PC2_CA_R17_2BDL_2BUL-UEConTest","CA_n041C_n071z2Az "," n041 PC001.005 ",null,"v1.3.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1j","CA_n41C-n261A","CA_n41A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041C_n261A ","CA_n041A_n261A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1j","CA_n41C-n261(2A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n041C_n261z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n41(2A)-n66A-n77(2A) BCS4and5","CA_n66A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041z2Az_n066A_n077z2Az BCS4and005 ","CA_n066A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1j","CA_n41(2A)-n71(2A) BCS4and5","CA_n41A-n71A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041z2Az_n071z2Az BCS4and005 ","CA_n041A_n071A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1j","CA_n41(2A)-n260(4A)","CA_n41A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041z2Az_n260z4Az ","CA_n041A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1j","CA_n41(A-C)-n77A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n041zA_Cz_n077A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n46A-n48C-n96A","CA_n48B-n96A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046A_n048C_n096A ","CA_n048B_n096A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n46A-n48(2A)-n96D","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046A_n048z2Az_n096D ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1k","CA_n46A-n78A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046A_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n46B-n48B-n96A","CA_n46A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046B_n048B_n096A ","CA_n046A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n46B-n48(3A)-n96E","CA_n46A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046B_n048z3Az_n096E ","CA_n046A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n46C-n48B-n96A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046C_n048B_n096A ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n46C-n48C-n96D","CA_n48A-n96A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046C_n048C_n096D ","CA_n048A_n096A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n46C-n48(2A)-n96E","CA_n48A-n96A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046C_n048z2Az_n096E ","CA_n048A_n096A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1k","CA_n46C-n96E","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046C_n096E ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n46D-n48(2A)-n96D","CA_n48A-n96A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046D_n048z2Az_n096D ","CA_n048A_n096A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1k","CA_n46D-n96B","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046D_n096B ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1k","CA_n46M-n48(3A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046M_n048z3Az ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n46N-n48A-n96B","CA_n46A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046N_n048A_n096B ","CA_n046A_n048A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n46N-n48C-n96E","CA_n48B-n96A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n046N_n048C_n096E ","CA_n048B_n096A ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n48A-n66A-n70A","-","Completed","PC3","RAN5#94-e","R5-221140","DISH Network","DISH Network,WE Certification (Jussi Kuusisto,Aleksi Heino)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048A_n066A_n070A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n48A-n66(2A)-n70A","CA_n48A-n66A","Completed","PC3","RAN5#96-e","R5-225447","DISH Network","DISH Network,WE Certification (Jussi Kuusisto,Aleksi Heino)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048A_n066z2Az_n070A ","CA_n048A_n066A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48A-n260G","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048A_n260G ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48A-n261M","CA_n48A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048A_n261M ","CA_n048A_n261I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48A-n261(A-H)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048A_n261zA_Hz ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48A-n263G","CA_n48A-n263A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048A_n263G ","CA_n048A_n263A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n48B-n66A-n71A","CA_n48A-n71A","Completed","PC3","RAN5#96-e","R5-225447","DISH Network","DISH Network,WE Certification (Jussi Kuusisto,Aleksi Heino)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048B_n066A_n071A ","CA_n048A_n071A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1l","CA_n48B-n96C","CA_n48A-n96A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048B_n096C ","CA_n048A_n096A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48B-n261K","CA_n48A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048B_n261K ","CA_n048A_n261I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48B-n261(2A-I) BCS1","CA_n48A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048B_n261z2A_Iz BCS1 ","CA_n048A_n261I ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48B-n261(2H) BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048B_n261z2Hz BCS1 ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48B-n261(A-G-H)","CA_n48A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048B_n261zA_G_Hz ","CA_n048A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48B-n261(A-H) BCS1","CA_n48A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048B_n261zA_Hz BCS1 ","CA_n048A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48B-n263G","CA_n48A-n263A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048B_n263G ","CA_n048A_n263A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1l","CA_n48C-n96C","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048C_n096C ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n48(2A)-n66A-n77A BCS1","-","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048z2Az_n066A_n077A BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1l","CA_n48(2A)-n71(2A)","-","Completed","PC3","RAN5#96-e","R5-225447","DISH Network","DISH Network,WE Certification (Jussi Kuusisto,Aleksi Heino)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048z2Az_n071z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48(2A)-n260J","CA_n48A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048z2Az_n260J ","CA_n048A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48(2A)-n261(2G)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048z2Az_n261z2Gz ","_ ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48(2A)-n261(A-G-I)","CA_n48A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048z2Az_n261zA_G_Iz ","CA_n048A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48(2A)-n261(H-I)","CA_n48A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048z2Az_n261zH_Iz ","CA_n048A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 IB non-cont","38.101-1:Table 5.5A.2-1","CA_n48(3A) BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048z3Az BCS1 ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1l","CA_n48(4A)-n96E","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048z4Az_n096E ","_ ",null,"v1.1.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48(A-B)-n260M","CA_n48A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048zA_Bz_n260M ","CA_n048A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1k","CA_n48(A-B)-n261L","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n048zA_Bz_n261L ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1m","CA_n66A-n71A BCS1","CA_n66A-n71A","Completed","PC3","RAN5#95-e","R5-223023","DISH Network,Rogers","DISH Network,WE Certification (Jussi Kuusisto,Aleksi Heino)","RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n071A BCS1 ","CA_n066A_n071A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77A-n260A","CA_n66A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077A_n260A ","CA_n066A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77A-n260H","CA_n77A-n260G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077A_n260H ","CA_n077A_n260G ","Fallback to CA_n66A-n77A-n260I with UL CA_n77A-n260G","v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77A-n260J","CA_n77A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077A_n260J ","CA_n077A_n260J ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77A-n260K","CA_n77A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077A_n260K ","CA_n077A_n260J ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77A-n260L BCS1","CA_n77A-n260A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077A_n260L BCS1 ","CA_n077A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77A-n261H","CA_n77A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077A_n261H ","CA_n077A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77A-n261I BCS1","CA_n77A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077A_n261I BCS1 ","CA_n077A_n261I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77A-n261L","CA_n66A-n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077A_n261L ","CA_n066A_n261I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77A-n261M BCS1","CA_n66A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077A_n261M BCS1 ","CA_n066A_n261G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77(2A)-n260H BCS1","CA_n77A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077z2Az_n260H BCS1 ","CA_n077A_n260G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77(2A)-n260J BCS1","CA_n66A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077z2Az_n260J BCS1 ","CA_n066A_n260G ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77(2A)-n260K BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077z2Az_n260K BCS1 ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n66A-n77(2A)-n260L BCS1","CA_n77A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n077z2Az_n260L BCS1 ","CA_n077A_n260A ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1m","CA_n66A-n78A","CA_n66A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n066A_n078A ","CA_n066A_n078A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1l","CA_n66A-n260G","CA_n66A-n260G","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n260G ","CA_n066A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1l","CA_n66A-n260K BCS1","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n260K BCS1 ","_ ","Fallback to CA_n66A-n77A-n260K BCS1 with UL -","v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1l","CA_n66A-n260M","CA_n66A-n260G","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n260M ","CA_n066A_n260G ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1l","CA_n66A-n261I","CA_n66A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n066A_n261I ","CA_n066A_n261G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1l","CA_n66A-n261(A-G-H)","CA_n66A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n261zA_G_Hz ","CA_n066A_n261H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1l","CA_n66A-n261(A-K)","CA_n66A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066A_n261zA_Kz ","CA_n066A_n261G ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 IB non-cont","38.101-1:Table 5.5A.2-1","CA_n66(2A)","-","Completed","PC3","<RAN5#94-e","R5-216445","DISH Network","WE Certification,DISH Network (Aleksi Heino,Jussi Kuusisto)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n066z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (3 bands)","38.101-1:Table 5.5A.3.2-1","CA_n66(2A)-n71A-n77(2A)","CA_n71A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066z2Az_n071A_n077z2Az ","CA_n071A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1l","CA_n66(2A)-n260I","CA_n66A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n066z2Az_n260I ","CA_n066A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1n","CA_n70A-n71(2A)","-","Completed","PC3","<RAN5#94-e","R5-217496","DISH Network","DISH Network,WE Certification (Jussi Kuusisto,Aleksi Heino)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n070A_n071z2Az ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1l","CA_n71A-n260(3A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n071A_n260z3Az ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1n","CA_n77A-n79A","CA_n77A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077A_n079A ","CA_n077A_n079A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n77A-n79A-n257I","CA_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n077A_n079A_n257I ","CA_n077A_n257G ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77A-n257K","CA_n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n077A_n257K ","CA_n257J ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77A-n258H","CA_n77A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077A_n258H ","CA_n077A_n258A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77A-n260I","-","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077A_n260I ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77A-n260L","CA_n77A-n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077A_n260L ","CA_n077A_n260L ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77A-n261L","CA_n77A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n077A_n261L ","CA_n077A_n261A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77A-n261(A-I)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n077A_n261zA_Iz ","_ ",null,"v1.0.0"]
[null,"Rel-15","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77C-n257A","-","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","CA_n077C_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77C-n260G","CA_n77A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077C_n260G ","CA_n077A_n260A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77C-n260L","CA_n77A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077C_n260L ","CA_n077A_n260I ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77C-n261(2A-G)","CA_n77A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077C_n261z2A_Gz ","CA_n077A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77C-n261(A-G-I) BCS1","CA_n77A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077C_n261zA_G_Iz BCS1 ","CA_n077A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77C-n261(G-I) BCS1","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077C_n261zG_Iz BCS1 ","_ ",null,"v1.2.0"]
[null,"Rel-17","NR CA FR1 inter-band (2 bands)","38.101-1:Table 5.5A.3.1-1n","CA_n77(2A)-n79A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077z2Az_n079A ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77(2A)-n257K","CA_n77A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n077z2Az_n257K ","CA_n077A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77(2A)-n260J","CA_n77A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077z2Az_n260J ","CA_n077A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77(2A)-n260M","CA_n77A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077z2Az_n260M ","CA_n077A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1m","CA_n77(3A)-n257I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n077z3Az_n257I ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (3 bands)","38.101-3:Table 5.5A.1-2","CA_n78A-n79A-n257I","CA_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n078A_n079A_n257I ","CA_n257H ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1n","CA_n78A-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n078A_n257M ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1n","CA_n78A-n258I","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n078A_n258I ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1n","CA_n78A-n258K","CA_n78A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n078A_n258K ","CA_n078A_n258H ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1n","CA_n78A-n258L BCS1","CA_n78A-n258K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n078A_n258L BCS1 ","CA_n078A_n258K ",null,"v1.0.0"]
[null,"Rel-15","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1n","CA_n78C-n257A","CA_n78A-n257A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","CA_n078C_n257A ","CA_n078A_n257A ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR1 IB cont","38.101-1:Table 5.5A.1-1","CA_n78D","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n078D ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1n","CA_n78(2A)-n257M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n078z2Az_n257M ","_ ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1o","CA_n79A-n257G","CA_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n079A_n257G ","CA_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1o","CA_n79A-n258A","CA_n79A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n079A_n258A ","CA_n079A_n258A ",null,"v1.0.0"]
[null,"Rel-15","NR CA FR1+FR2 inter-band (2 bands)","38.101-3:Table 5.5A.1-1o","CA_n79C-n257A","-","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","CA_n079C_n257A ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR2 inter-band (2 bands)","38.101-2:Table 5.5A.3-1","CA_n257G-n259M","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n257G_n259M ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR2 inter-band (2 bands)","38.101-2:Table 5.5A.3-1","CA_n257I-n259A","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n257I_n259A ","_ ",null,"v1.0.0"]
[null,"Rel-15","NR CA FR2 IB cont","38.101-2:Table 5.5A.1-1","CA_n257M","CA_n257M","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","CA_n257M ","CA_n257M ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR2 IB non-cont","38.101-2:Table 5.5A.2-1","CA_n258(3A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n258z3Az ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR2 IB non-cont","38.101-2:Table 5.5A.2-1","CA_n258(4A)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n258z4Az ","_ ",null,"v1.0.0"]
[null,"Rel-15","NR CA FR2 IB cont","38.101-2:Table 5.5A.1-1","CA_n260D","CA_n260D","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","CA_n260D ","CA_n260D ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR2 inter-band (2 bands)","38.101-2:Table 5.5A.3-1","CA_n260H-n261A","CA_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n260H_n261A ","CA_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR2 inter-band (2 bands)","38.101-2:Table 5.5A.3-1","CA_n260J-n261K","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n260J_n261K ","_ ",null,"v1.0.0"]
[null,"Rel-17","NR CA FR2 inter-band (2 bands)","38.101-2:Table 5.5A.3-1","CA_n260M-n261J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n260M_n261J ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR2 mix IB cont & non-cont","38.101-2:Table 5.5A.2-2","CA_n260(2A-2O)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n260z2A_2Oz ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR2 IB non-cont","38.101-2:Table 5.5A.2-1","CA_n260(2H)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n260z2Hz ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR2 mix IB cont & non-cont","38.101-2:Table 5.5A.2-2","CA_n260(3A-G)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n260z3A_Gz ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR2 IB non-cont","38.101-2:Table 5.5A.2-1","CA_n260(4P)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n260z4Pz ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR2 mix IB cont & non-cont","38.101-2:Table 5.5A.2-2","CA_n260(A-H)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n260zA_Hz ","_ ",null,"v1.0.0"]
[null,"Rel-15","NR CA FR2 mix IB cont & non-cont","38.101-2:Table 5.5A.2-2","CA_n260(D-I)","-","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","CA_n260zD_Iz ","_ ",null,"v1.0.0"]
[null,"Rel-15","NR CA FR2 IB cont","38.101-2:Table 5.5A.1-1","CA_n261B","CA_n261B","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","CA_n261B ","CA_n261B ",null,"v1.0.0"]
[null,"Rel-15","NR CA FR2 IB cont","38.101-2:Table 5.5A.1-1","CA_n261J","CA_n261J","Ongoing (FB)","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","CA_n261J ","CA_n261J ","Fallback to CA_n261M with UL CA_n261M","v1.0.0"]
[null,"Rel-17","NR CA FR2 mix IB cont & non-cont","38.101-2:Table 5.5A.2-2","CA_n261(2A-G-2O)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n261z2A_G_2Oz ","_ ",null,"v1.2.0"]
[null,"Rel-16","NR CA FR2 mix IB cont & non-cont","38.101-2:Table 5.5A.2-2","CA_n261(A-2D)","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n261zA_2Dz ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR2 mix IB cont & non-cont","38.101-2:Table 5.5A.2-2","CA_n261(A-G-H)","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n261zA_G_Hz ","_ ","Fallback to CA_n261(A-G-I) with UL -","v1.0.0"]
[null,"Rel-15","NR CA FR2 mix IB cont & non-cont","38.101-2:Table 5.5A.2-2","CA_n261(D-H)","-","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","CA_n261zD_Hz ","_ ",null,"v1.0.0"]
[null,"Rel-16","NR CA FR2 mix IB cont & non-cont","38.101-2:Table 5.5A.2-2","CA_n261(G-H)","-","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","CA_n261zG_Hz ","_ ","Fallback to CA_n261(2H) with UL -","v1.0.0"]
[null,"Rel-17","NR CA FR2 IB cont","38.101-2:Table 5.5A.1-1","CA_n263J","-","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","CA_n263J ","_ ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-1A-3A-7A_n7A","DC_3A_n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_001A_003A_007A_n007A ","DC_003A_n007A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-1A-3C-5A_n78A","DC_1A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_001A_003C_005A_n078A ","DC_001A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_1A-1A_n7B","DC_1A_n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_001A_n007B ","DC_001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A-7A_n78A-n257A","DC_5A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_007A_n078A_n257A ","DC_005A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A-7A_n78A-n257E","DC_5A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_005A_007A_007A_n078A_n257E ","DC_005A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A-7A_n78A-n257H","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_005A_007A_007A_n078A_n257H ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A-7A_n78A-n257I","DC_5A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_007A_n078A_n257I ","DC_005A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A-7A_n78A-n257K","DC_3A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_007A_n078A_n257K ","DC_003A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-5A-7A-7A_n78C","DC_1A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_007A_n078C ","DC_001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A-7A_n78C-n257G","DC_5A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_007A_n078C_n257G ","DC_005A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A-7A_n78C-n257J","DC_5A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_007A_n078C_n257J ","DC_005A_n078A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A-7A_n78C-n257L","DC_1A_n78A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_007A_n078C_n257L ","DC_001A_n078A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-5A-7A-7A_n257G","DC_5A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_005A_007A_007A_n257G ","DC_005A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-5A-7A-7A_n257J","DC_5A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_007A_n257J ","DC_005A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-5A-7A-7A_n257L","DC_1A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_007A_n257L ","DC_001A_n257H ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-5A-7A_n78A","DC_7A_n78A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_003A_005A_007A_n078A ","DC_007A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A_n78A-n257E","DC_1A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_005A_007A_n078A_n257E ","DC_001A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A_n78A-n257I","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_005A_007A_n078A_n257I ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A_n78A-n257J","DC_7A_n78A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_n078A_n257J ","DC_007A_n078A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A_n78A-n257K","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_005A_007A_n078A_n257K ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A_n78C-n257F","DC_1A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_n078C_n257F ","DC_001A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A_n78C-n257F","DC_3A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_n078C_n257F ","DC_003A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-5A-7A_n78C-n257K","DC_5A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_n078C_n257K ","DC_005A_n078A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-5A-7A_n78(2A)","DC_7A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_n078z2Az ","DC_007A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-5A-7A_n257F","DC_5A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_005A_007A_n257F ","DC_005A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-5A-7A_n257K","DC_5A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_007A_n257K ","DC_005A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-5A-41A_n79A","DC_5A_n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_005A_041A_n079A ","DC_005A_n079A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-5A_n78A-n257D","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_005A_n078A_n257D ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-5A_n78A-n257H","DC_3A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_n078A_n257H ","DC_003A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-5A_n78A-n257I","DC_5A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_005A_n078A_n257I ","DC_005A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-5A_n78A-n257M","DC_3A_n78A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_n078A_n257M ","DC_003A_n078A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-5A_n78C-n257I","DC_1A_n78A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_n078C_n257I ","DC_001A_n078A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-5A_n78C-n257K","DC_3A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_n078C_n257K ","DC_003A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-5A_n78C-n257M","DC_3A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_n078C_n257M ","DC_003A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-5A_n257H","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_n257H ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-5A_n257M","DC_5A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_005A_n257M ","DC_005A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A-7A_n78A-n257A","DC_1A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_007A_n078A_n257A ","DC_001A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A-7A_n78A-n257H","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_007A_007A_n078A_n257H ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A-7A_n78A-n257I","DC_7A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_007A_n078A_n257I ","DC_007A_n078A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A-7A_n78A-n257L","DC_1A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_007A_n078A_n257L ","DC_001A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A-7A_n78C-n257I","DC_1A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_007A_n078C_n257I ","DC_001A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A-7A_n78C-n257K","DC_1A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_007A_n078C_n257K ","DC_001A_n078A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-7A-7A_n257D","DC_1A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_007A_n257D ","DC_001A_n257D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-7A-7A_n257K","DC_7A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_007A_n257K ","DC_007A_n257G ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (6 bands)","38.101-3:Table 5.5B.4.5-1","DC_1A-3A-7A-8A-40C_n78A","DC_1A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_008A_040C_n078A ","DC_001A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-7A-8A_n78A","DC_8A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_007A_008A_n078A ","DC_008A_n078A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (6 bands)","38.101-3:Table 5.5B.4.5-1","DC_1A-3A-7A-20A_n28A-n78A","DC_1A_n28A","Completed","PC3","<=RAN5#93-e","R5-216625","Orange","Orange (Hajer Khanfir)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_003A_007A_020A_n028A_n078A ","DC_001A_n028A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (6 bands)","38.101-3:Table 5.5B.4.5-1","DC_1A-3A-7A-28A_n5A-n78A","DC_28A_n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_007A_028A_n005A_n078A ","DC_028A_n005A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-7A-28A_n78A-n257H","DC_28A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_028A_n078A_n257H ","DC_028A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-7A-28A_n258B","DC_1A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_028A_n258B ","DC_001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-7A-28A_n258G","DC_7A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_028A_n258G ","DC_007A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-7A-28A_n258I","DC_7A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_028A_n258I ","DC_007A_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-7A-28A_n258L","DC_1A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_028A_n258L ","DC_001A_n258I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-7A_n5A-n78A","DC_1A_n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_007A_n005A_n078A ","DC_001A_n005A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-3A-7A_n28A","DC_3A_n28A","Completed","PC3","<=RAN5#93-e","R5-216625","Orange","Orange (Hajer Khanfir)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_003A_007A_n028A ","DC_003A_n028A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A_n78A-n257D","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_007A_n078A_n257D ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A_n78A-n257G","DC_1A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n078A_n257G ","DC_001A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A_n78A-n257I","DC_7A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n078A_n257I ","DC_007A_n078A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A_n78A-n257M","DC_3A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n078A_n257M ","DC_003A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A_n78A-n258E","DC_1A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n078A_n258E ","DC_001A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A_n78A-n258H","DC_3A_n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n078A_n258H ","DC_003A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A_n78A-n258J","DC_1A_n258H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n078A_n258J ","DC_001A_n258H ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A_n78A-n258L","DC_7A_n258I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n078A_n258L ","DC_007A_n258I ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A_n78C-n257J","DC_3A_n78A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n078C_n257J ","DC_003A_n078A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-7A_n78C-n257L","DC_7A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n078C_n257L ","DC_007A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-7A_n257G","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n257G ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-7A_n257M","DC_1A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n257M ","DC_001A_n257I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-7A_n258E","DC_1A_n258D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n258E ","DC_001A_n258D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-7A_n258J","DC_1A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n258J ","DC_001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-7A_n258L","DC_3A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007A_n258L ","DC_003A_n258A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-7C-28A_n5A","DC_28A_n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_007C_028A_n005A ","DC_028A_n005A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-7C-28A_n258H","DC_7C_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007C_028A_n258H ","DC_007C_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-7C-28A_n258J","DC_1A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007C_028A_n258J ","DC_001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-7C-28A_n258L","DC_1A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007C_028A_n258L ","DC_001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-7C-28A_n258M","DC_3A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007C_028A_n258M ","DC_003A_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-7C_n258C","DC_1A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007C_n258C ","DC_001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-7C_n258H","DC_3A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007C_n258H ","DC_003A_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-7C_n258J","DC_1A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007C_n258J ","DC_001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-7C_n258L","DC_7A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_007C_n258L ","DC_007A_n258I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (6 bands)","38.101-3:Table 5.5B.4.5-1","DC_1A-3A-8A-11A_n28A-n77A","DC_1A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_008A_011A_n028A_n077A ","DC_001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-8A-11A_n257I","DC_11A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_008A_011A_n257I ","DC_011A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-3A-8A_n28A","DC_1A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_008A_n028A ","DC_001A_n028A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-8A_n77A-n79A","DC_1A_n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_008A_n077A_n079A ","DC_001A_n079A ",null,"v1.1.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-8A_n78A-n257G","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_008A_n078A_n257G ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-8A_n257F","DC_8A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_008A_n257F ","DC_008A_n257D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-8A_n257I","DC_8A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_008A_n257I ","DC_008A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-8A_n257M","DC_1A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_008A_n257M ","DC_001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-3A-11A_n77A","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_011A_n077A ","DC_001A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-18A-42A_n78A-n257H","DC_1A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_042A_n078A_n257H ","DC_001A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-18A-42A_n257D","DC_18A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_042A_n257D ","DC_018A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-18A-42A_n257H","DC_18A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_042A_n257H ","DC_018A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-18A-42A_n257K","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_042A_n257K ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-18A-42A_n257L","DC_42A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_042A_n257L ","DC_042A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-18A-42C_n78A-n257I","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_042C_n078A_n257I ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-18A-42C_n257F","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_042C_n257F ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-18A-42C_n257H","DC_42A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_042C_n257H ","DC_042A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-18A-42C_n257J","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_042C_n257J ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-18A-42C_n257L","DC_1A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_042C_n257L ","DC_001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-18A_n28A-n41A","DC_3A_n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_018A_n028A_n041A ","DC_003A_n041A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-18A_n41A-n77(2A)","DC_18A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_018A_n041A_n077z2Az ","DC_018A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-18A_n78A-n257A","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_n078A_n257A ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-18A_n78A-n257I","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_n078A_n257I ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-18A_n257H","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_n257H ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-18A_n257M","DC_18A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_018A_n257M ","DC_018A_n257I ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-19A-21A_n257A","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_003A_019A_021A_n257A ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-19A-42A_n257D","DC_19A_n257A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_003A_019A_042A_n257D ","DC_019A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-19A-42A_n257K","DC_1A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_019A_042A_n257K ","DC_001A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-19A-42A_n257M","DC_3A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_019A_042A_n257M ","DC_003A_n257H ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-19A-42C_n78C","DC_19A_n78A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_003A_019A_042C_n078C ","DC_019A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-19A-42C_n257G","DC_3A_n257A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_019A_042C_n257G ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-19A-42C_n257J","DC_3A_n257I","Ongoing","PC3",null,null,"NTT DOCOMO",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_019A_042C_n257J ","DC_003A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-19A-42C_n257M","DC_42A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_019A_042C_n257M ","DC_042A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-19A_n257G","DC_3A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_019A_n257G ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-19A_n257J","DC_1A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_019A_n257J ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-19A_n257K","DC_19A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_019A_n257K ","DC_019A_n257I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-20A-32A_n78A","DC_20A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_020A_032A_n078A ","DC_020A_n078A ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-3A-20A_n78(2A)","DC_1A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_020A_n078z2Az ","DC_001A_n078A ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-21A-42A_n257G","DC_21A_n257A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_042A_n257G ","DC_021A_n257A ","Fallback to DC_1A-3A-21A-42C_n257G with UL DC_21A_n257A","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-21A-42A_n257I","DC_21A_n257G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_042A_n257I ","DC_021A_n257G ","Fallback to DC_1A-3A-21A-42C_n257I with UL DC_21A_n257G","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-21A-42A_n257K","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_042A_n257K ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-21A-42A_n257M","DC_3A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_042A_n257M ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-21A-42C_n257H","DC_21A_n257H","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_042C_n257H ","DC_021A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-21A-42C_n257J","DC_3A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_042C_n257J ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-21A-42C_n257L","DC_21A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_042C_n257L ","DC_021A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-21A_n77A-n257H","DC_3A_n77A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_n077A_n257H ","DC_003A_n077A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-21A_n77A-n257H","DC_3A_n77A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_n077A_n257H ","DC_003A_n077A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-21A_n78A-n257G","DC_3A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_n078A_n257G ","DC_003A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-21A_n78A-n257H","DC_21A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_n078A_n257H ","DC_021A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-21A_n79A-n257A","DC_1A_n79A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_n079A_n257A ","DC_001A_n079A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-21A_n79A-n257I","DC_21A_n79A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_n079A_n257I ","DC_021A_n079A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-21A_n257G","DC_3A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_n257G ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-21A_n257K","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_n257K ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-21A_n257M","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_021A_n257M ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-28A-42A_n78A-n257G","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_042A_n078A_n257G ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-28A-42A_n257H","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_042A_n257H ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-28A-42A_n257I","DC_42A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_042A_n257I ","DC_042A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-28A-42A_n257L","DC_1A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_042A_n257L ","DC_001A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-28A-42A_n257M","DC_3A_n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_042A_n257M ","DC_003A_n257K ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-28A-42C_n78A-n257H","DC_28A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_042C_n078A_n257H ","DC_028A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-28A-42C_n257G","DC_42C_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_042C_n257G ","DC_042C_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-28A-42C_n257I","DC_28A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_042C_n257I ","DC_028A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-28A-42C_n257K","DC_3A_n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_042C_n257K ","DC_003A_n257K ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-28A-42C_n257L","DC_28A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_042C_n257L ","DC_028A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-28A_n7B-n78A","DC_1A_n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_n007B_n078A ","DC_001A_n007A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-28A_n78A-n257G","DC_28A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_n078A_n257G ","DC_028A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-28A_n78A-n257I","DC_28A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_n078A_n257I ","DC_028A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-28A_n257I","DC_28A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_028A_n257I ","DC_028A_n257I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-28A_n258C","DC_1A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_028A_n258C ","DC_001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-28A_n258H","DC_28A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_028A_n258H ","DC_028A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-28A_n258L","DC_1A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_028A_n258L ","DC_001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-3A-32A_n78C","DC_1A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_032A_n078C ","DC_001A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41A-42A_n77A-n257G","DC_41A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042A_n077A_n257G ","DC_041A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41A-42A_n78A-n257H","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042A_n078A_n257H ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41A-42A_n78A-n257I","DC_41A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042A_n078A_n257I ","DC_041A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41A-42A_n257H","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042A_n257H ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41A-42A_n257J","DC_3A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042A_n257J ","DC_003A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41A-42C_n77A-n257A","DC_41A_n77A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042C_n077A_n257A ","DC_041A_n077A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41A-42C_n77A-n257I","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042C_n077A_n257I ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41A-42C_n78A-n257A","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042C_n078A_n257A ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41A-42C_n78A-n257I","DC_1A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042C_n078A_n257I ","DC_001A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41A-42C_n257A","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042C_n257A ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41A-42C_n257J","DC_1A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042C_n257J ","DC_001A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41A-42C_n257L","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042C_n257L ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41A-42C_n257M","DC_41A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_042C_n257M ","DC_041A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-41A_n28A-n257H","DC_3A_n28A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_041A_n028A_n257H ","DC_003A_n028A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-41A_n28A-n257H","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_041A_n028A_n257H ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-41A_n77A-n257I","DC_41A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_n077A_n257I ","DC_041A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-41A_n78A-n257I","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_n078A_n257I ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-41A_n257F","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_n257F ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-41A_n257M","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041A_n257M ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41C-42A_n77A-n257H","DC_1A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042A_n077A_n257H ","DC_001A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41C-42A_n77A-n257I","DC_3A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042A_n077A_n257I ","DC_003A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41C-42A_n78A-n257G","DC_41C_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042A_n078A_n257G ","DC_041C_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41C-42A_n78A-n257I","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042A_n078A_n257I ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41C-42A_n257H","DC_42A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042A_n257H ","DC_042A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41C-42A_n257J","DC_42A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042A_n257J ","DC_042A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41C-42A_n257L","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042A_n257L ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41C-42A_n257M","DC_41A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042A_n257M ","DC_041A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41C-42C_n77A-n257H","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042C_n077A_n257H ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41C-42C_n78A-n257G","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042C_n078A_n257G ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_1A-3A-41C-42C_n78A-n257I","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042C_n078A_n257I ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41C-42C_n257A","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042C_n257A ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41C-42C_n257G","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042C_n257G ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41C-42C_n257I","DC_41C_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042C_n257I ","DC_041C_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41C-42C_n257L","DC_3A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042C_n257L ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3A-41C-42C_n257M","DC_3A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_042C_n257M ","DC_003A_n257H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-3A-41C_n28A","DC_41C_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_041C_n028A ","DC_041C_n028A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-41C_n77A-n257G","DC_1A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_n077A_n257G ","DC_001A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-41C_n77A-n257I","DC_41C_n77A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_n077A_n257I ","DC_041C_n077A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-41C_n78A-n257G","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_n078A_n257G ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-41C_n78A-n257I","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_n078A_n257I ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-41C_n257F","DC_41C_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_n257F ","DC_041C_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-41C_n257K","DC_41C_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_041C_n257K ","DC_041C_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3A-42A_n28A-n77A","DC_3A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_042A_n028A_n077A ","DC_003A_n028A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-42A_n77A-n257H","DC_1A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042A_n077A_n257H ","DC_001A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-3A-42A_n77(2A)","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_042A_n077z2Az ","DC_001A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-42A_n78A-n257I","DC_42A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042A_n078A_n257I ","DC_042A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-42A_n257K","DC_1A_n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042A_n257K ","DC_001A_n257K ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-42A_n257L","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042A_n257L ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-3A-42C_n77A","DC_3A_n77A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_003A_042C_n077A ","DC_003A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-42C_n77A-n257H","DC_42A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042C_n077A_n257H ","DC_042A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3A-42C_n78A-n257G","DC_3A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042C_n078A_n257G ","DC_003A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-42C_n257G","DC_42C_n257A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042C_n257G ","DC_042C_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-42C_n257I","DC_42A_n257I","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042C_n257I ","DC_042A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-42C_n257K","DC_42C_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042C_n257K ","DC_042C_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-42C_n257M","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042C_n257M ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-42D_n257I","DC_42A_n257H","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042D_n257I ","DC_042A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-42D_n257K","DC_42C_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042D_n257K ","DC_042C_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3A-42D_n257M","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_042D_n257M ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-3A_n5A-n78A","DC_3A_n5A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_n005A_n078A ","DC_003A_n005A ","Fallback to DC_1A-3C_n5A-n78A with UL DC_3A_n5A","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3A_n28A-n257A","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_n028A_n257A ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3A_n28A-n257I","DC_3A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_n028A_n257I ","DC_003A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-3A_n77A-n79A","DC_3A_n79A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_n077A_n079A ","DC_003A_n079A ","Fallback to DC_1A-3A_n28A-n77A-n79A with UL DC_3A_n79A","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3A_n77A-n257H","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_n077A_n257H ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-3A_SUL_n78A-n80A","DC_1A_n80A","Ongoing","PC3",null,null,"NTT DOCOMO",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_n078A_n080A ","DC_001A_n080A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3A_n78A-n257I","DC_1A_n257I","N/A","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_n078A_n257I ","DC_001A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3A_n78A-n257J","DC_3A_n257G","N/A","PC3",null,null,"NTT DOCOMO",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_n078A_n257J ","DC_003A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3A_n78A-n257M","DC_1A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_n078A_n257M ","DC_001A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3A_n78A-n258D","DC_3A_n258D","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_n078A_n258D ","DC_003A_n258D ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3A_n78A-n258L","DC_1A_n258G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_n078A_n258L ","DC_001A_n258G ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3A_n78C-n257I","DC_1A_n78A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_n078C_n257I ","DC_001A_n078A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3A_n78C-n257L","DC_3A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_n078C_n257L ","DC_003A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3A_n79A-n257H","DC_3A_n79A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_n079A_n257H ","DC_003A_n079A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-3A_n257A","DC_1A_n257A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_003A_n257A ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-3A_n257M","DC_1A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003A_n257M ","DC_001A_n257I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-3A_n258H","DC_3A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_n258H ","DC_003A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-3A_n258K","DC_3A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003A_n258K ","DC_003A_n258I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3C-7A-28A_n7A","DC_3C_n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003C_007A_028A_n007A ","DC_003C_n007A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3C-7A-28A_n258H","DC_3C_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007A_028A_n258H ","DC_003C_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3C-7A-28A_n258I","DC_28A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007A_028A_n258I ","DC_028A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3C-7A-28A_n258K","DC_28A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007A_028A_n258K ","DC_028A_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3C-7A-28A_n258M","DC_1A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007A_028A_n258M ","DC_001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-7A_n258A","DC_1A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007A_n258A ","DC_001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-7A_n258G","DC_3C_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007A_n258G ","DC_003C_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-7A_n258I","DC_3C_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007A_n258I ","DC_003C_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-7A_n258L","DC_1A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007A_n258L ","DC_001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-7A_n258M","DC_7A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007A_n258M ","DC_007A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3C-7C-28A_n258G","DC_3A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007C_028A_n258G ","DC_003A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3C-7C-28A_n258I","DC_7A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007C_028A_n258I ","DC_007A_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3C-7C-28A_n258J","DC_7A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007C_028A_n258J ","DC_007A_n258I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3C-7C-28A_n258K","DC_7C_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007C_028A_n258K ","DC_007C_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-3C-7C-28A_n258M","DC_3C_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007C_028A_n258M ","DC_003C_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-7C_n258C","DC_7A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007C_n258C ","DC_007A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-7C_n258G","DC_7C_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007C_n258G ","DC_007C_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-7C_n258I","DC_3C_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007C_n258I ","DC_003C_n258G ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-7C_n258J","DC_7A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007C_n258J ","DC_007A_n258H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-7C_n258L","DC_7A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_007C_n258L ","DC_007A_n258I ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-3C-8A_n78A-n257G","DC_8A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003C_008A_n078A_n257G ","DC_008A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-8A_n257D","DC_1A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_008A_n257D ","DC_001A_n257D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-8A_n257H","DC_1A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_008A_n257H ","DC_001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-8A_n257M","DC_8A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_008A_n257M ","DC_008A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-3C-28A_n7B-n78A","DC_1A_n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003C_028A_n007B_n078A ","DC_001A_n007A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-28A_n258C","DC_28A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_028A_n258C ","DC_028A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-28A_n258H","DC_3A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_028A_n258H ","DC_003A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-3C-28A_n258K","DC_1A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_028A_n258K ","DC_001A_n258G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-3C_n7A","DC_3C_n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003C_n007A ","DC_003C_n007A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-3C_n78A","DC_3A_n78A","Completed","PC3","<=RAN5#93-e","R5-216625","China Unicom","China Unicom (Yu Shi)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_003C_n078A ","DC_003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3C_n78A-n257F","DC_1A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_n078A_n257F ","DC_001A_n078A_n257A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3C_n78A-n257H","DC_3A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_n078A_n257H ","DC_003A_n078A_n257A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-3C_n78A-n257J","DC_3A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_n078A_n257J ","DC_003A_n257I ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-3C_n257E","DC_1A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003C_n257E ","DC_001A_n257D ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-3C_n257K","DC_3A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003C_n257K ","DC_003A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-3C_n257M","DC_3A_n257M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_003C_n257M ","DC_003A_n257M ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-3C_n258F","DC_1A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_n258F ","DC_001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-3C_n258J","DC_1A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_003C_n258J ","DC_001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A-7A_n78A-n257D","DC_1A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_007A_007A_n078A_n257D ","DC_001A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A-7A_n78A-n257F","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_005A_007A_007A_n078A_n257F ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A-7A_n78A-n257I","DC_7A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_007A_007A_n078A_n257I ","DC_007A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A-7A_n78A-n257M","DC_5A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_005A_007A_007A_n078A_n257M ","DC_005A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A-7A_n78A-n257M","DC_5A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_007A_007A_n078A_n257M ","DC_005A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A-7A_n78C-n257K","DC_1A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_007A_007A_n078C_n257K ","DC_001A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A-7A_n78C-n257M","DC_1A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_007A_007A_n078C_n257M ","DC_001A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-5A-7A-7A_n257H","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_005A_007A_007A_n257H ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-5A-7A-7A_n257M","DC_7A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_005A_007A_007A_n257M ","DC_007A_n257A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A_n78A-n257A","DC_1A_n78A","N/A","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_005A_007A_n078A_n257A ","DC_001A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A_n78A-n257H","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_005A_007A_n078A_n257H ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A_n78A-n257I","DC_7A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_007A_n078A_n257I ","DC_007A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A_n78A-n257L","DC_1A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_007A_n078A_n257L ","DC_001A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A_n78C-n257I","DC_1A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_007A_n078C_n257I ","DC_001A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-5A-7A_n78C-n257K","DC_1A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_007A_n078C_n257K ","DC_001A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-5A-7A_n257D","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_005A_007A_n257D ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-5A-7A_n257H","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_007A_n257H ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-5A-7A_n257K","DC_7A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_007A_n257K ","DC_007A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-5A_n78A-n257G","DC_5A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_n078A_n257G ","DC_005A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-5A_n78A-n257J","DC_1A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_005A_n078A_n257J ","DC_001A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-5A_n78A-n257M","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_005A_n078A_n257M ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-5A_n78C-n257H","DC_5A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_n078C_n257H ","DC_005A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-5A_n257H","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_005A_n257H ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-5A_n257M","DC_5A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_005A_n257M ","DC_005A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-7A-7A_n78A-n257E","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_007A_007A_n078A_n257E ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-7A-7A_n78A-n257J","DC_1A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_007A_n078A_n257J ","DC_001A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-7A-7A_n78C-n257H","DC_7A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_007A_n078C_n257H ","DC_007A_n078A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-7A-7A_n78C-n257L","DC_1A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_007A_n078C_n257L ","DC_001A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-7A-7A_n257H","DC_7A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_007A_n257H ","DC_007A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-7A-7A_n257L","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_007A_007A_n257L ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-7A-8A-40C_n78A","DC_8A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_008A_040C_n078A ","DC_008A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-7A-20A_n8A","DC_20A_n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_007A_020A_n008A ","DC_020A_n008A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-7A-28A-32A_n3A","DC_1A_n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_028A_032A_n003A ","DC_001A_n003A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-7A-28A_n78A","DC_28A_n78A","Ongoing","PC3",null,null,"Orange","Huawei,Hisilicon (Chunying Gu,Yuxin Hao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_007A_028A_n078A ","DC_028A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-7A-28A_n257A","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_028A_n257A ","DC_001A_n257A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-7A-28A_n258I","DC_1A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_028A_n258I ","DC_001A_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-7A-28A_n258L","DC_7A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_028A_n258L ","DC_007A_n258I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-7A-38A_n3A","DC_1A_n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_038A_n003A ","DC_001A_n003A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-7A_n8A-n78A","DC_7A_n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_n008A_n078A ","DC_007A_n008A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-7A_n78A-n257A","DC_7A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_n078A_n257A ","DC_007A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-7A_n78A-n257K","DC_1A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_n078A_n257K ","DC_001A_n078A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-7A_n78A-n258D","DC_7A_n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_n078A_n258D ","DC_007A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-7A_n78A-n258H","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_n078A_n258H ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-7A_n78C-n257D","DC_7A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_n078C_n257D ","DC_007A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-7A_n78C-n257E","DC_1A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_n078C_n257E ","DC_001A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-7A_n257E","DC_7A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_n257E ","DC_007A_n257D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-7A_n257L","DC_1A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_n257L ","DC_001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-7A_n258E","DC_1A_n258D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007A_n258E ","DC_001A_n258D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (6 bands)","38.101-3:Table 5.5B.4.5-1","DC_1A-7C-20A-28A-32A_n3A","DC_20A_n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007C_020A_028A_032A_n003A ","DC_020A_n003A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-7C-28A_n78A","DC_28A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_007C_028A_n078A ","DC_028A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-7C-28A_n258G","DC_1A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007C_028A_n258G ","DC_001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-7C-28A_n258J","DC_7A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007C_028A_n258J ","DC_007A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-7C-28A_n258K","DC_28A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007C_028A_n258K ","DC_028A_n258H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-7C_n78A","DC_7C_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_007C_n078A ","DC_007C_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-7C_n258G","DC_1A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007C_n258G ","DC_001A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-7C_n258I","DC_7C_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007C_n258I ","DC_007C_n258I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-7C_n258L","DC_1A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_007C_n258L ","DC_001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (6 bands)","38.101-3:Table 5.5B.4.5-1","DC_1A-8A-11A_n3A-n28A-n77A","DC_11A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_011A_n003A_n028A_n077A ","DC_011A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-8A-11A_n77A-n257D","DC_11A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_008A_011A_n077A_n257D ","DC_011A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-8A-11A_n77(2A)-n79A","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_011A_n077z2Az_n079A ","DC_001A_n077A ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-8A-11A_n77(2A)-n257G","DC_8A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_008A_011A_n077z2Az_n257G ","DC_008A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-8A-11A_n77(2A)-n257I","DC_8A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_011A_n077z2Az_n257I ","DC_008A_n257H ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-8A-11A_n257I","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_011A_n257I ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (6 bands)","38.101-3:Table 5.5B.4.5-1","DC_1A-8A-42A_n3A-n28A-n77(2A)","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_042A_n003A_n028A_n077z2Az ","DC_001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-8A-42A_n28A-n77(2A)","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_042A_n028A_n077z2Az ","DC_001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-8A-42C_n3A-n77A","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_042C_n003A_n077A ","DC_001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-8A_n3A-n77A","DC_8A_n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_n003A_n077A ","DC_008A_n003A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-8A_n28A-n78A","DC_8A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_n028A_n078A ","DC_008A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-8A_n40A-n258F","DC_8A_n40A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_n040A_n258F ","DC_008A_n040A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-8A_n40A-n258L","DC_8A_n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_n040A_n258L ","DC_008A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-8A_n77A-n257I","DC_8A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_008A_n077A_n257I ","DC_008A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-8A_n78A-n257G","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_008A_n078A_n257G ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-8A_n78A-n258F","DC_8A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_n078A_n258F ","DC_008A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-8A_n78A-n258L","DC_8A_n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_n078A_n258L ","DC_008A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-8A_n257G","DC_8A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_008A_n257G ","DC_008A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-8A_n257M","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_n257M ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-8A_n258L","DC_1A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_008A_n258L ","DC_001A_n258G ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-11A-18A_n78(2A)","DC_1A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_011A_018A_n078z2Az ","DC_001A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-11A_n3A-n28A-n77A","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_011A_n003A_n028A_n077A ","DC_001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-11A_n3A-n77(2A)-n79A","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_011A_n003A_n077z2Az_n079A ","DC_001A_n077A ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-11A_n77A-n257G","DC_11A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_011A_n077A_n257G ","DC_011A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-11A_n78(2A)","DC_11A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_011A_n078z2Az ","DC_011A_n078A ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-11A_n257I","DC_11A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_011A_n257I ","DC_011A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-18A-41A_n257A","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_041A_n257A ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-18A-41A_n257I","DC_18A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_041A_n257I ","DC_018A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-18A-41C_n78A","DC_18A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_041C_n078A ","DC_018A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-18A-42A_n78A-n257H","DC_18A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_042A_n078A_n257H ","DC_018A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-18A-42A_n257D","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_042A_n257D ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-18A-42A_n257J","DC_18A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_042A_n257J ","DC_018A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-18A-42C_n78A-n257H","DC_1A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_042C_n078A_n257H ","DC_001A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-18A-42C_n78A-n257I","DC_42A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_042C_n078A_n257I ","DC_042A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-18A-42C_n257H","DC_42C_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_042C_n257H ","DC_042C_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-18A-42C_n257J","DC_18A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_042C_n257J ","DC_018A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-18A-42C_n257M","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_042C_n257M ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-18A_n28A-n77A","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_018A_n028A_n077A ","DC_001A_n077A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-18A_n41A-n78A","DC_1A_n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_018A_n041A_n078A ","DC_001A_n041A ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-18A_n78A-n257I","DC_18A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_n078A_n257I ","DC_018A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-18A_n257I","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_018A_n257I ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-19A-21A-42A_n257D","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_019A_021A_042A_n257D ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-19A-21A-42A_n257I","DC_21A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_021A_042A_n257I ","DC_021A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-19A-21A-42A_n257K","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_021A_042A_n257K ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-19A-21A-42A_n257L","DC_42A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_021A_042A_n257L ","DC_042A_n257I ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-19A-21A-42C_n77A","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_019A_021A_042C_n077A ","DC_001A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-19A-21A-42C_n257I","DC_21A_n257I","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_021A_042C_n257I ","DC_021A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-19A-21A-42C_n257K","DC_42A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_021A_042C_n257K ","DC_042A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_1A-19A-21A-42C_n257M","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_021A_042C_n257M ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-19A-21A_n79A","DC_1A_n79A","Completed","PC3","<=RAN5#93-e","R5-216625","NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_019A_021A_n079A ","DC_001A_n079A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-19A-21A_n257K","DC_19A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_021A_n257K ","DC_019A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-19A-21A_n257L","DC_21A_n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_021A_n257L ","DC_021A_n257J ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-19A-42A_n77A-n257G","DC_1A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_042A_n077A_n257G ","DC_001A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-19A-42A_n78A-n257A","DC_19A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_042A_n078A_n257A ","DC_019A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-19A-42A_n79A-n257G","DC_1A_n79A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_042A_n079A_n257G ","DC_001A_n079A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-19A-42A_n79A-n257I","DC_19A_n79A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_042A_n079A_n257I ","DC_019A_n079A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-19A-42A_n257G","DC_19A_n257A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_042A_n257G ","DC_019A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-19A-42A_n257L","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_042A_n257L ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-19A-42C_n77A","DC_19A_n77A","Ongoing (FB)","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_019A_042C_n077A ","DC_019A_n077A ","Fallback to DC_1A-19A-42C_n77A-n79A with UL DC_19A_n77A","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-19A-42C_n78A-n257H","DC_1A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_042C_n078A_n257H ","DC_001A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-19A-42C_n79A-n257G","DC_19A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_042C_n079A_n257G ","DC_019A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-19A-42C_n79A-n257I","DC_1A_n79A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_042C_n079A_n257I ","DC_001A_n079A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-19A-42C_n257H","DC_42A_n257A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_042C_n257H ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-19A-42C_n257K","DC_1A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_042C_n257K ","DC_001A_n257I ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-19A_n77C","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_019A_n077C ","DC_001A_n077A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-19A_n79A","DC_19A_n79A","Completed","PC3","<=RAN5#93-e","R5-216625","NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_019A_n079A ","DC_019A_n079A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-19A_n79A-n257H","DC_19A_n79A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_n079A_n257H ","DC_019A_n079A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-19A_n79C","DC_19A_n79A","Ongoing (FB)","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_019A_n079C ","DC_019A_n079A ","Fallback to DC_1A-19A-21A-42C_n79C with UL DC_19A_n79A","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-19A_n257K","DC_1A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_019A_n257K ","DC_001A_n257H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-20A-40A_n78A","DC_40A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_020A_040A_n078A ","DC_040A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-20A_n41A","DC_20A_n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_020A_n041A ","DC_020A_n041A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-21A-28A-42C_n77A","DC_21A_n77A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_021A_028A_042C_n077A ","DC_021A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-21A-42A_n77A-n257I","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042A_n077A_n257I ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-21A-42A_n78A-n257G","DC_21A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042A_n078A_n257G ","DC_021A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-21A-42A_n78A-n257I","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042A_n078A_n257I ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-21A-42A_n79A-n257A","DC_21A_n79A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042A_n079A_n257A ","DC_021A_n079A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-21A-42A_n79A-n257I","DC_21A_n79A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042A_n079A_n257I ","DC_021A_n079A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-21A-42A_n257J","DC_21A_n257I","Ongoing","PC3",null,null,"NTT DOCOMO",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042A_n257J ","DC_021A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-21A-42A_n257M","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042A_n257M ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-21A-42C_n77A-n257A","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042C_n077A_n257A ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-21A-42C_n77A-n257H","DC_21A_n77A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042C_n077A_n257H ","DC_021A_n077A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-21A-42C_n78A-n257A","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042C_n078A_n257A ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-21A-42C_n79A-n257A","DC_21A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042C_n079A_n257A ","DC_021A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-21A-42C_n79A-n257I","DC_21A_n79A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042C_n079A_n257I ","DC_021A_n079A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-21A-42C_n257F","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_021A_042C_n257F ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-21A-42C_n257I","DC_21A_n257H","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042C_n257I ","DC_021A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-21A-42C_n257L","DC_1A_n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_042C_n257L ","DC_001A_n257K ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_1A-21A_n28A-n77A-n79A","DC_1A_n79A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_021A_n028A_n077A_n079A ","DC_001A_n079A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-21A_n77A-n79A","DC_1A_n79A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_n077A_n079A ","DC_001A_n079A ","Fallback to DC_1A-21A-42C_n77A-n79A with UL DC_1A_n79A","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-21A_n77A-n257I","DC_21A_n77A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_n077A_n257I ","DC_021A_n077A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-21A_n78C","DC_21A_n78A","Ongoing (FB)","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_021A_n078C ","DC_021A_n078A ","Fallback to DC_1A-19A-21A-42C_n78C with UL DC_21A_n78A","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-21A_n78(2A)","DC_1A_n78A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_021A_n078z2Az ","DC_001A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-21A_n257G","DC_21A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_n257G ","DC_021A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-21A_n257K","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_n257K ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-21A_n257M","DC_21A_n257M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_021A_n257M ","DC_021A_n257M ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-28A-42A_n257G","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_028A_042A_n257G ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-28A-42A_n257I","DC_42A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_028A_042A_n257I ","DC_042A_n257H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-28A-42A_n257M","DC_1A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_028A_042A_n257M ","DC_001A_n257I ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-28A-42C_n78A-n257G","DC_28A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_028A_042C_n078A_n257G ","DC_028A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-28A-42C_n79A","DC_28A_n79A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_028A_042C_n079A ","DC_028A_n079A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-28A-42C_n257K","DC_1A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_028A_042C_n257K ","DC_001A_n257H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-28A-42C_n257L","DC_42A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_028A_042C_n257L ","DC_042A_n257I ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-28A_n3A-n257H","DC_1A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_028A_n003A_n257H ","DC_001A_n257G ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-28A_n7A-n78A","DC_1A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_028A_n007A_n078A ","DC_001A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-28A_n78A-n257H","DC_28A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_028A_n078A_n257H ","DC_028A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-28A_n257K","DC_28A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_028A_n257K ","DC_028A_n257I ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-28A_n258E","DC_1A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_028A_n258E ","DC_001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-28A_n258L","DC_1A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_028A_n258L ","DC_001A_n258I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-38A_n8A","DC_38A_n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_038A_n008A ","DC_038A_n008A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-41A-42A_n78A-n257G","DC_41A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041A_042A_n078A_n257G ","DC_041A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-41A-42A_n257F","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041A_042A_n257F ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-41A-42A_n257I","DC_41A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041A_042A_n257I ","DC_041A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-41A-42A_n257M","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041A_042A_n257M ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-41A-42C_n78A","DC_41A_n78A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_041A_042C_n078A ","DC_041A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-41A-42C_n78A-n257H","DC_42A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041A_042C_n078A_n257H ","DC_042A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-41A-42C_n257F","DC_42C_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041A_042C_n257F ","DC_042C_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-41A-42C_n257I","DC_41A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041A_042C_n257I ","DC_041A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-41A-42C_n257K","DC_42C_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041A_042C_n257K ","DC_042C_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-41A_n28A-n41A","DC_41A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_041A_n028A_n041A ","DC_041A_n028A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-41A_n28A-n257G","DC_41A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041A_n028A_n257G ","DC_041A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-41A_n77A-n257H","DC_1A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041A_n077A_n257H ","DC_001A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-41A_n257D","DC_41A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041A_n257D ","DC_041A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-41A_n257K","DC_41A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041A_n257K ","DC_041A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-41C-42A_n77A-n257H","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_042A_n077A_n257H ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-41C-42A_n77A-n257I","DC_41C_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_042A_n077A_n257I ","DC_041C_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-41C-42A_n78A-n257H","DC_42A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_042A_n078A_n257H ","DC_042A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-41C-42A_n257A","DC_41C_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_042A_n257A ","DC_041C_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-41C-42A_n257J","DC_42A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_042A_n257J ","DC_042A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-41C-42A_n257M","DC_41C_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_042A_n257M ","DC_041C_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-41C-42C_n77A-n257G","DC_41C_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_042C_n077A_n257G ","DC_041C_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-41C-42C_n78A-n257G","DC_41C_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_042C_n078A_n257G ","DC_041C_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_1A-41C-42C_n78A-n257G","DC_42A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_042C_n078A_n257G ","DC_042A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-41C-42C_n257F","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_042C_n257F ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-41C-42C_n257I","DC_42A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_042C_n257I ","DC_042A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_1A-41C-42C_n257J","DC_42C_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_042C_n257J ","DC_042C_n257I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-41C_n3A-n77A","DC_41A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_041C_n003A_n077A ","DC_041A_n077A ",null,"v1.1.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-41C_n28A-n257A","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_n028A_n257A ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-41C_n28A-n257H","DC_41C_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_n028A_n257H ","DC_041C_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-41C_n77A-n257H","DC_41A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_n077A_n257H ","DC_041A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-41C_n78A","DC_41A_n78A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_041C_n078A ","DC_041A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-41C_n257G","DC_41C_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_n257G ","DC_041C_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-41C_n257K","DC_41A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_n257K ","DC_041A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-41C_n257M","DC_41C_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_041C_n257M ","DC_041C_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A-42A_n3A-n77(2A)","DC_42A_n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_042A_n003A_n077z2Az ","DC_042A_n003A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-42A_n77A-n257I","DC_1A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042A_n077A_n257I ","DC_001A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-42A_n79A-n257H","DC_42A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042A_n079A_n257H ","DC_042A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-42A_n257I","DC_1A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042A_n257I ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-42A_n257K","DC_42A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042A_n257K ","DC_042A_n257I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-42C_n3A","DC_42A_n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_042C_n003A ","DC_042A_n003A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A-42C_n77A","DC_1A_n77A","Ongoing (FB)","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_042C_n077A ","DC_001A_n077A ","Fallback to DC_1A-21A-42C_n77A-n79A with UL DC_1A_n77A","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-42C_n78A-n257H","DC_42A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042C_n078A_n257H ","DC_042A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_1A-42C_n79A-n257A","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042C_n079A_n257A ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-42C_n257E","DC_1A_n257A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_042C_n257E ","DC_001A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-42C_n257L","DC_1A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042C_n257L ","DC_001A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-42D_n257D","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042D_n257D ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-42D_n257D","DC_42A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042D_n257D ","DC_042A_n257D ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-42D_n257J","DC_42C_n257A","Ongoing","PC3",null,null,"NTT DOCOMO",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042D_n257J ","DC_042C_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-42D_n257M","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042D_n257M ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-42E_n257J","DC_42A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042E_n257J ","DC_042A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_1A-42E_n257M","DC_1A_n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_042E_n257M ","DC_001A_n257K ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_1A_n3A-n28A-n77(2A)","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_n003A_n028A_n077z2Az ","DC_001A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_1A_n3A-n257G","DC_1A_n3A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_n003A_n257G ","DC_001A_n003A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A_n28A-n77A","DC_1A_n77A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_n028A_n077A ","DC_001A_n077A ","Fallback to DC_1A-3A_n28A-n77A-n79A with UL DC_1A_n77A","v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_1A_n41A-n78A","DC_1A_n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_n041A_n078A ","DC_001A_n041A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_1A_n77A-n257E","DC_1A_n77A-n257A","N/A","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_n077A_n257E ","DC_001A_n077A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_1A_n77C-n257E","DC_1A_n257D","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_n077C_n257E ","DC_001A_n257D ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_1A_n77(3A)","DC_1A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_n077z3Az ","DC_001A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_1A_n78A-n257I","DC_1A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_n078A_n257I ","DC_001A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_1A_n78C-n257A","DC_1A_n78A-n257A","N/A","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_001A_n078C_n257A ","DC_001A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_1A_n78C-n257H","DC_1A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_n078C_n257H ","DC_001A_n257H ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_1A_n78C-n257M","DC_1A_n78A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_n078C_n257M ","DC_001A_n078A_n257I ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_1A_n79A-n257G","DC_1A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_n079A_n257G ","DC_001A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_1A_n257H","DC_1A_n257A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_001A_n257H ","DC_001A_n257A ","Fallback to DC_1A-3A_n78A-n257H with UL DC_1A_n78A-n257A","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_1A_n258M","DC_1A_n258A","Ongoing","PC3",null,null,"Telstra","Ericsson (Niclas Weiler)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_001A_n258M ","DC_001A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-2A-5A-30A-66A_n260G","DC_5A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_030A_066A_n260G ","DC_005A_n260A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-2A-5A-30A-66A_n260J","DC_5A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_030A_066A_n260J ","DC_005A_n260H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-2A-5A-30A-66A_n260M","DC_2A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_030A_066A_n260M ","DC_002A_n260A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-2A-5A-30A-66A_n260M","DC_66A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_030A_066A_n260M ","DC_066A_n260G ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-5A-30A_n260I","DC_5A_n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_030A_n260I ","DC_005A_n260I ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-5A-30A_n260K","DC_2A_n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_030A_n260K ","DC_002A_n260K ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-5A-30A_n260M","DC_2A_n260M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_030A_n260M ","DC_002A_n260M ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-5A-66A-66A_n260J","DC_66A_n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_066A_066A_n260J ","DC_066A_n260J ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-5A-66A-66A_n260L","DC_2A_n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_066A_066A_n260L ","DC_002A_n260L ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-2A-5A-66A_n30A","DC_2A_n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_066A_n030A ","DC_002A_n030A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-5A-66A_n260H","DC_2A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_066A_n260H ","DC_002A_n260H ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-5A-66A_n260L","DC_5A_n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_066A_n260L ","DC_005A_n260L ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A-2A-5A_n77C","DC_2A_n77A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_005A_n077C ","DC_002A_n077A ","Fallback to DC_2A-2A-5A_n77C with UL DC_2A_n77A PC2","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-5A_n260J","DC_2A_n260I","Ongoing","PC3",null,null,"Verizon,AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_002A_005A_n260J ","DC_002A_n260I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-5A_n260M","DC_5A_n260A","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_002A_005A_n260M ","DC_005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_2A-2A-7A-66A-71A_n78A","DC_7A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_007A_066A_071A_n078A ","DC_007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-2A-12A-30A-66A_n260I","DC_30A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_030A_066A_n260I ","DC_030A_n260H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-2A-12A-30A-66A_n260K","DC_30A_n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_030A_066A_n260K ","DC_030A_n260I ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-2A-12A-30A-66A_n260L","DC_30A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_030A_066A_n260L ","DC_030A_n260H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-2A-12A-30A-66A_n260M","DC_66A_n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_030A_066A_n260M ","DC_066A_n260K ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-12A-30A_n260K","DC_12A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_030A_n260K ","DC_012A_n260H ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-12A-30A_n260L","DC_30A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_030A_n260L ","DC_030A_n260G ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-12A-66A-66A_n260H","DC_2A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_066A_066A_n260H ","DC_002A_n260H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-12A-66A-66A_n260J","DC_12A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_066A_066A_n260J ","DC_012A_n260G ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-12A-66A-66A_n260M","DC_66A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_066A_066A_n260M ","DC_066A_n260G ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-12A-66A_n260H","DC_66A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_066A_n260H ","DC_066A_n260G ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-12A-66A_n260J","DC_66A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_066A_n260J ","DC_066A_n260G ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-12A-66A_n260L","DC_66A_n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_066A_n260L ","DC_066A_n260K ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-12A-66A_n260M","DC_66A_n260M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_066A_n260M ","DC_066A_n260M ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-12A_n260L","DC_2A_n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_012A_n260L ","DC_002A_n260L ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_2A-2A-13A-66A_n5A-n77A","DC_66A_n77A PC2","Ongoing","PC2",null,null,"Verizon",null,"RAN5#94-e","ENDC_PC2_R17_xLTE_yNR-UEConTest","DC_002A_002A_013A_066A_n005A_n077A ","DC_066A_n077A PC002 ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-2A-13A_n5A-n77A","DC_13A_n77A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_013A_n005A_n077A ","DC_013A_n077A ","Fallback to DC_2A-2A-13A_n5A-n77A with UL DC_13A_n77A PC2","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-13A_n261J","DC_13A_n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_013A_n261J ","DC_013A_n261G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-13A_n261M","DC_13A_n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_013A_n261M ","DC_013A_n261H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-2A-14A-30A-66A_n260K","DC_2A_n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_014A_030A_066A_n260K ","DC_002A_n260I ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-2A-14A-30A-66A_n260L","DC_30A_n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_014A_030A_066A_n260L ","DC_030A_n260L ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-2A-14A-30A-66A_n260M","DC_30A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_014A_030A_066A_n260M ","DC_030A_n260G ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-14A-30A_n260A","DC_14A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_014A_030A_n260A ","DC_014A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-14A-30A_n260J","DC_30A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_014A_030A_n260J ","DC_030A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-14A-30A_n260M","DC_30A_n260M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_014A_030A_n260M ","DC_030A_n260M ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-14A-66A-66A_n260J","DC_66A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_014A_066A_066A_n260J ","DC_066A_n260A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-14A-66A-66A_n260L","DC_2A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_014A_066A_066A_n260L ","DC_002A_n260H ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-14A-66A_n260H","DC_2A_n260G","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_002A_014A_066A_n260H ","DC_002A_n260G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-14A-66A_n260K","DC_14A_n260A","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_002A_014A_066A_n260K ","DC_014A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-14A-66A_n260L","DC_14A_n260L","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_002A_014A_066A_n260L ","DC_014A_n260L ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-14A-66A_n260M","DC_66A_n260G","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_002A_014A_066A_n260M ","DC_066A_n260G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-14A_n260J","DC_2A_n260J","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_002A_014A_n260J ","DC_002A_n260J ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-29A-30A_n260H","DC_30A_n260H","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_029A_030A_n260H ","DC_030A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-29A-30A_n260L","DC_30A_n260I","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_029A_030A_n260L ","DC_030A_n260I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-29A-30A_n260M","DC_30A_n260G","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_029A_030A_n260M ","DC_030A_n260G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-29A_n260L","DC_2A_n260A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_029A_n260L ","DC_002A_n260A ","Fallback to DC_2A-2A-29A-30A_n260L with UL DC_2A_n260A","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-30A-66A_n260H","DC_30A_n260H","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_030A_066A_n260H ","DC_030A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-2A-30A-66A_n260L","DC_66A_n260H","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_030A_066A_n260L ","DC_066A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-30A_n260G","DC_2A_n260G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_030A_n260G ","DC_002A_n260G ","Fallback to DC_2A-2A-29A-30A_n260G with UL DC_2A_n260G","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-30A_n260J","DC_30A_n260I","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_030A_n260J ","DC_030A_n260I ","Fallback to DC_2A-2A-29A-30A_n260J with UL DC_30A_n260I","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-30A_n260L","DC_30A_n260J","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_030A_n260L ","DC_030A_n260J ","Fallback to DC_2A-2A-29A-30A_n260L with UL DC_30A_n260J","v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-46A_n260K","DC_2A_n260I","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_002A_046A_n260K ","DC_002A_n260I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-46D_n260I","DC_2A_n260I","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_002A_046D_n260I ","DC_002A_n260I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-46D_n260M","DC_2A_n260L","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_002A_046D_n260M ","DC_002A_n260L ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A-2A-66A-66A_n30A","DC_66A_n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_066A_066A_n030A ","DC_066A_n030A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-66A-66A_n260L","DC_66A_n260L","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_066A_066A_n260L ","DC_066A_n260L ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-66A-66A_n260M","DC_2A_n260A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_066A_066A_n260M ","DC_002A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-66A_n260H","DC_66A_n260H","Ongoing","PC3",null,null,"Verizon,AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_002A_066A_n260H ","DC_066A_n260H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-66A_n260K","DC_66A_n260A","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_002A_066A_n260K ","DC_066A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-66A_n261G","DC_66A_n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_066A_n261G ","DC_066A_n261G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-2A-66A_n261M","DC_66A_n261L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_066A_n261M ","DC_066A_n261L ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A-2A_n66A-n77C","DC_2A_n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_n066A_n077C ","DC_002A_n066A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_2A-2A_n260M","DC_2A_n260G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_n260M ","DC_002A_n260G ","Fallback to DC_2A-2A-5A_n260M with UL DC_2A_n260G","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_2A-2A_n261K","DC_2A_n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_002A_n261K ","DC_002A_n261I ",null,"v1.1.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A-5A-5A_n66A","DC_5A_n66A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_005A_005A_n066A ","DC_005A_n066A ","Fallback to DC_2A-5A-5A-66A_n66A with UL DC_5A_n66A","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-5A-30A-66A-66A_n260H","DC_30A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_030A_066A_066A_n260H ","DC_030A_n260H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-5A-30A-66A-66A_n260J","DC_5A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_030A_066A_066A_n260J ","DC_005A_n260A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-5A-30A-66A-66A_n260L","DC_2A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_030A_066A_066A_n260L ","DC_002A_n260H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-5A-30A-66A-66A_n260L","DC_66A_n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_030A_066A_066A_n260L ","DC_066A_n260L ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_2A-5A-30A-66A_n77A","DC_2A_n77A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_030A_066A_n077A ","DC_002A_n077A ","Fallback to DC_2A-5A-30A-66A_n77A with UL DC_2A_n77A PC2","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-5A-30A-66A_n260J","DC_66A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_030A_066A_n260J ","DC_066A_n260H ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-5A-30A-66A_n260K","DC_66A_n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_030A_066A_n260K ","DC_066A_n260J ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-5A-30A-66A_n260M","DC_5A_n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_030A_066A_n260M ","DC_005A_n260I ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-5A-30A_n66A","DC_5A_n66A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_030A_n066A ","DC_005A_n066A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-5A-30A_n260K","DC_30A_n260A","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_005A_030A_n260K ","DC_030A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-5A-30A_n260M","DC_5A_n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_030A_n260M ","DC_005A_n260L ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-5A-48C_n77C","DC_5A_n77A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_048C_n077C ","DC_005A_n077A ","Fallback to DC_2A-5A-48C_n77C with UL DC_5A_n77A PC2","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-5A-66A-66A_n77C","DC_2A_n77A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_066A_066A_n077C ","DC_002A_n077A ","Fallback to DC_2A-5A-66A-66A_n77C with UL DC_2A_n77A PC2","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-5A-66A-66A_n260J","DC_5A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_066A_066A_n260J ","DC_005A_n260G ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-5A-66A-66A_n260M","DC_2A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_066A_066A_n260M ","DC_002A_n260H ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-5A-66A_n7A","DC_2A_n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_066A_n007A ","DC_002A_n007A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_2A-5A-66A_n66A-n77A","DC_66A_n77A PC2","Ongoing","PC2",null,null,"Verizon",null,"RAN5#94-e","ENDC_PC2_R17_xLTE_yNR-UEConTest","DC_002A_005A_066A_n066A_n077A ","DC_066A_n077A PC002 ",null,"v1.3.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-5A-66A_n260I","DC_5A_n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_066A_n260I ","DC_005A_n260I ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-5A-66A_n260M","DC_2A_n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_066A_n260M ","DC_002A_n260L ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-5A_n2A-n77C","DC_2A_n77A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_n002A_n077C ","DC_002A_n077A ","Fallback to DC_2A-5A_n2A-n77C with UL DC_2A_n77A PC2","v1.1.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-5A_n66A-n77C","DC_5A_n77A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_n066A_n077C ","DC_005A_n077A ","Fallback to DC_2A-5A_n66A-n77C with UL DC_5A_n77A PC2","v1.1.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-5A_n260G","DC_2A_n260G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_005A_n260G ","DC_002A_n260G ","Fallback to DC_2A-2A-5A_n260G with UL DC_2A_n260G","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-5A_n260M","DC_5A_n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_n260M ","DC_005A_n260J ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-5A_n261L","DC_2A_n261G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_005A_n261L ","DC_002A_n261G ","Fallback to DC_2A-5A_n261M with UL DC_2A_n261G","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-5A_n261(2A-I)","DC_2A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_005A_n261z2A_Iz ","DC_002A_n261A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-5A_n261(A-G-I)","DC_2A_n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_005A_n261zA_G_Iz ","DC_002A_n261I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-5A_n261(A-J)","DC_2A_n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_005A_n261zA_Jz ","DC_002A_n261H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-5A_n261(H-I)","DC_5A_n261I","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_005A_n261zH_Iz ","DC_005A_n261I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-7A-7A-66A-66A_n78A","DC_7A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_007A_007A_066A_066A_n078A ","DC_007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-7A-7A-66A_n77A","DC_2A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_007A_007A_066A_n077A ","DC_002A_n077A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_2A-7A-13A_n25A-n66A","DC_13A_n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_007A_013A_n025A_n066A ","DC_013A_n066A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-7A-13A_n66A","DC_2A_n66A","Completed","PC3","<RAN5#94-e","R5-216445","Bell,Telus","Huawei (Chunying Gu)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_007A_013A_n066A ","DC_002A_n066A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_2A-7A-66A_n66A-n77A","DC_7A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_007A_066A_n066A_n077A ","DC_007A_n077A ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-7A_n25A-n66A","DC_7A_n25A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_007A_n025A_n066A ","DC_007A_n025A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A-7A_n77A","DC_2A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_007A_n077A ","DC_002A_n077A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-7C-66A_n77A","DC_7A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_007C_066A_n077A ","DC_007A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A-7C_n78(2A)","DC_7A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_007C_n078z2Az ","DC_007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-12A-30A-66A-66A_n260H","DC_66A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_030A_066A_066A_n260H ","DC_066A_n260A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-12A-30A-66A-66A_n260K","DC_2A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_030A_066A_066A_n260K ","DC_002A_n260H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-12A-30A-66A-66A_n260L","DC_2A_n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_030A_066A_066A_n260L ","DC_002A_n260I ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_2A-12A-30A-66A_n77A","DC_2A_n77A PC2","Ongoing","PC2",null,null,"AT&T",null,"RAN5#94-e","ENDC_PC2_R17_xLTE_yNR-UEConTest","DC_002A_012A_030A_066A_n077A ","DC_002A_n077A PC002 ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-12A-30A-66A_n260I","DC_30A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_030A_066A_n260I ","DC_030A_n260H ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-12A-30A-66A_n260J","DC_66A_n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_030A_066A_n260J ","DC_066A_n260J ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-12A-30A-66A_n260L","DC_2A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_030A_066A_n260L ","DC_002A_n260A ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-12A-30A-66A_n260M","DC_12A_n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_030A_066A_n260M ","DC_012A_n260K ",null,"v1.1.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-12A-30A_n260J","DC_12A_n260A","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_012A_030A_n260J ","DC_012A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-12A-30A_n260L","DC_12A_n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_030A_n260L ","DC_012A_n260L ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-12A-30A_n260M","DC_30A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_030A_n260M ","DC_030A_n260G ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-12A-66A-66A_n260G","DC_2A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_066A_066A_n260G ","DC_002A_n260A ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-12A-66A-66A_n260J","DC_66A_n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_066A_066A_n260J ","DC_066A_n260J ",null,"v1.1.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-12A-66A_n2A","DC_66A_n2A","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_012A_066A_n002A ","DC_066A_n002A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-12A-66A_n260I","DC_2A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_066A_n260I ","DC_002A_n260G ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-12A-66A_n260J","DC_66A_n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_066A_n260J ","DC_066A_n260J ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-12A_n2A-n78A","DC_2A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_n002A_n078A ","DC_002A_n078A ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-12A_n260I","DC_2A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_n260I ","DC_002A_n260G ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-12A_n260K","DC_12A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_n260K ","DC_012A_n260H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-12A_n260M","DC_2A_n260M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_012A_n260M ","DC_002A_n260M ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_2A-13A-66A-66A_n5A-n77A","DC_13A_n77A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_013A_066A_066A_n005A_n077A ","DC_013A_n077A ","Fallback to DC_2A-13A-66A-66A_n5A-n77A with UL DC_13A_n77A PC2","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-13A-66A_n77C","DC_66A_n77A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#95-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_013A_066A_n077C ","DC_066A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n260J","DC_66A_n260A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n260J ","DC_066A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n260L","DC_2A_n260H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n260L ","DC_002A_n260H ","Fallback to DC_2A-13A-66A_n260M with UL DC_2A_n260H","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n260M","DC_2A_n260L","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n260M ","DC_002A_n260L ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n260(2H)","DC_2A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n260z2Hz ","DC_002A_n260H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n261H","DC_2A_n261G","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n261H ","DC_002A_n261G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n261J","DC_13A_n261A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n261J ","DC_013A_n261A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n261L","DC_13A_n261L","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n261L ","DC_013A_n261L ","Fallback to DC_2A-13A-66A_n261M with UL DC_13A_n261L","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n261M","DC_66A_n261G","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n261M ","DC_066A_n261G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n261(2G)","DC_66A_n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n261z2Gz ","DC_066A_n261A ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_66A_n261A","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n261(A-I)","DC_2A_n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n261zA_Iz ","DC_002A_n261A ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_2A_n261A","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n261(A-J)","DC_66A_n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n261zA_Jz ","DC_066A_n261I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n261(G-J)","DC_2A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n261zG_Jz ","DC_002A_n261A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-13A-66A_n261(H-I)","DC_66A_n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_066A_n261zH_Iz ","DC_066A_n261H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-13A_n66A-n77A","DC_13A_n77A PC2","Ongoing","PC2",null,null,"Verizon",null,"RAN5#94-e","ENDC_PC2_R17_xLTE_yNR-UEConTest","DC_002A_013A_n066A_n077A ","DC_013A_n077A PC002 ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-13A_n260L","DC_13A_n260G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_n260L ","DC_013A_n260G ","Fallback to DC_2A-13A-66A_n260M with UL DC_13A_n260G","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-13A_n260(2A-2G)","DC_13A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_013A_n260z2A_2Gz ","DC_013A_n260G ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-13A_n260(A-H)","DC_13A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_013A_n260zA_Hz ","DC_013A_n260G ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-13A_n261(2A-I)","DC_13A_n261G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_n261z2A_Iz ","DC_013A_n261G ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_13A_n261G","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-13A_n261(A-2G)","DC_13A_n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_n261zA_2Gz ","DC_013A_n261A ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_13A_n261A","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-13A_n261(A-J)","DC_13A_n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_013A_n261zA_Jz ","DC_013A_n261I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-13A_n261(G-I)","DC_2A_n261H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_013A_n261zG_Iz ","DC_002A_n261H ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_2A_n261H","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-14A-30A-66A-66A_n260I","DC_66A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_014A_030A_066A_066A_n260I ","DC_066A_n260A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-14A-30A-66A-66A_n260K","DC_66A_n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_014A_030A_066A_066A_n260K ","DC_066A_n260K ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-14A-30A-66A-66A_n260L","DC_66A_n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_014A_030A_066A_066A_n260L ","DC_066A_n260I ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_2A-14A-30A-66A_n66A","DC_14A_n66A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_014A_030A_066A_n066A ","DC_014A_n066A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-14A-30A-66A_n260H","DC_2A_n260H","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_030A_066A_n260H ","DC_002A_n260H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-14A-30A-66A_n260K","DC_66A_n260G","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_030A_066A_n260K ","DC_066A_n260G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-14A-30A-66A_n260M","DC_14A_n260A","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_030A_066A_n260M ","DC_014A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-14A-30A_n2A","DC_14A_n2A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_014A_030A_n002A ","DC_014A_n002A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-14A-30A_n260J","DC_2A_n260A","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_030A_n260J ","DC_002A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-14A-30A_n260K","DC_14A_n260J","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_030A_n260K ","DC_014A_n260J ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-14A-66A-66A_n260A","DC_2A_n260A","Completed","PC3","RAN5#94-e","R5-220023","AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_066A_066A_n260A ","DC_002A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-14A-66A-66A_n260J","DC_66A_n260G","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_066A_066A_n260J ","DC_066A_n260G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-14A-66A-66A_n260L","DC_2A_n260I","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_066A_066A_n260L ","DC_002A_n260I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-14A-66A-66A_n260M","DC_66A_n260M","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_066A_066A_n260M ","DC_066A_n260M ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-14A-66A_n260K","DC_2A_n260J","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_066A_n260K ","DC_002A_n260J ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-14A-66A_n260L","DC_14A_n260J","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_066A_n260L ","DC_014A_n260J ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A-14A_n66A","DC_14A_n66A","Completed","PC3","<RAN5#94-e","R5-216445","AT&T","Qualcomm (Kevin Wang)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_n066A ","DC_014A_n066A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-14A_n260I","DC_14A_n260H","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_014A_n260I ","DC_014A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A-28A_n78A","DC_28A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_028A_n078A ","DC_028A_n078A ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-29A-30A-66A_n260I","DC_66A_n260H","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_029A_030A_066A_n260I ","DC_066A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-29A-30A-66A_n260K","DC_30A_n260H","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_029A_030A_066A_n260K ","DC_030A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_2A-29A-30A-66A_n260M","DC_30A_n260H","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_029A_030A_066A_n260M ","DC_030A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-29A-30A_n260G","DC_2A_n260G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_029A_030A_n260G ","DC_002A_n260G ","Fallback to DC_2A-2A-29A-30A_n260G with UL DC_2A_n260G","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-29A-30A_n260M","DC_30A_n260J","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_029A_030A_n260M ","DC_030A_n260J ","Fallback to DC_2A-2A-29A-30A_n260M with UL DC_30A_n260J","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-29A-66A_n260J","DC_2A_n260G","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_029A_066A_n260J ","DC_002A_n260G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-29A-66A_n260L","DC_2A_n260J","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_029A_066A_n260L ","DC_002A_n260J ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-29A_n260J","DC_2A_n260A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_029A_n260J ","DC_002A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-29A_n260M","DC_2A_n260M","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_029A_n260M ","DC_002A_n260M ","Fallback to DC_2A-2A-29A-30A_n260M with UL DC_2A_n260M","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-30A-66A-66A_n260K","DC_30A_n260G","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_030A_066A_066A_n260K ","DC_030A_n260G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-30A-66A-66A_n260M","DC_30A_n260G","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_030A_066A_066A_n260M ","DC_030A_n260G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-30A-66A_n77A","DC_2A_n77A PC2","Ongoing","PC2",null,null,"AT&T",null,"RAN5#94-e","ENDC_PC2_R17_xLTE_yNR-UEConTest","DC_002A_030A_066A_n077A ","DC_002A_n077A PC002 ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-30A-66A_n260I","DC_2A_n260H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_030A_066A_n260I ","DC_002A_n260H ","Fallback to DC_2A-2A-30A-66A_n260I with UL DC_2A_n260H","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-30A-66A_n260K","DC_66A_n260J","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_030A_066A_n260K ","DC_066A_n260J ","Fallback to DC_2A-2A-30A-66A_n260K with UL DC_66A_n260J","v1.2.0"]
[null,"Rel-15","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-30A_n260G","DC_2A_n260A","Ongoing","PC3",null,null,"AT&T","AT&T (Ron Borsato)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_002A_030A_n260G ","DC_002A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-30A_n260L","DC_2A_n260J","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_030A_n260L ","DC_002A_n260J ","Fallback to DC_2A-2A-29A-30A_n260L with UL DC_2A_n260J","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-30A_n260M","DC_30A_n260I","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_030A_n260M ","DC_030A_n260I ","Fallback to DC_2A-2A-29A-30A_n260M with UL DC_30A_n260I","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-46A-46A-46A_n261(A-K)","DC_2A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_046A_046A_046A_n261zA_Kz ","DC_002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-46A-46A_n261M","DC_2A_n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_046A_046A_n261M ","DC_002A_n261G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-46A-46A_n261(A-J)","DC_2A_n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_046A_046A_n261zA_Jz ","DC_002A_n261I ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_2A-46A-66A_n41A-n71A","DC_66A_n71A","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_046A_066A_n041A_n071A ","DC_066A_n071A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-46A-66A_n260K","DC_66A_n260A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_046A_066A_n260K ","DC_066A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-46A_n260H","DC_2A_n260H","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_046A_n260H ","DC_002A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-46A_n261J","DC_2A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_046A_n261J ","DC_002A_n261A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-46A_n261M","DC_2A_n261M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_046A_n261M ","DC_002A_n261M ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-46A_n261(A-L)","DC_2A_n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_046A_n261zA_Lz ","DC_002A_n261G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-46C-66A_n260I","DC_66A_n260G","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_046C_066A_n260I ","DC_066A_n260G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-46C_n41A-n71A","DC_2A_n71A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_046C_n041A_n071A ","DC_002A_n071A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-46C_n260M","DC_2A_n260A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_046C_n260M ","DC_002A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-46D-66A_n41(2A)","DC_66A_n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_046D_066A_n041z2Az ","DC_066A_n041A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-46D-66A_n260J","DC_2A_n260H","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_046D_066A_n260J ","DC_002A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-46D-66A_n260M","DC_2A_n260M","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_046D_066A_n260M ","DC_002A_n260M ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-46D_n260M","DC_2A_n260K","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_046D_n260M ","DC_002A_n260K ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-46E-66A_n260I","DC_2A_n260H","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_046E_066A_n260I ","DC_002A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_2A-46E-66A_n260L","DC_66A_n260L","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_046E_066A_n260L ","DC_066A_n260L ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-48A-66A_n5A","DC_66A_n5A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_048A_066A_n005A ","DC_066A_n005A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-48A-66A_n12A","DC_2A_n12A","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_048A_066A_n012A ","DC_002A_n012A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-48D-66A_n66A","DC_48A_n66A","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_048D_066A_n066A ","DC_048A_n066A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A-48E_n66A","DC_2A_n66A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_048E_n066A ","DC_002A_n066A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A-66A_n260A","DC_2A_n260A","Ongoing","PC3",null,null,"Verizon,AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_066A_n260A ","DC_002A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A-66A_n260M","DC_66A_n260G","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_066A_n260M ","DC_066A_n260G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A-66A_n261I","DC_66A_n261H","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_066A_n261I ","DC_066A_n261H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A-66A_n261M","DC_2A_n261I","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_066A_n261M ","DC_002A_n261I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A-66A_n261(2A-I)","DC_2A_n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_066A_n261z2A_Iz ","DC_002A_n261H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A-66A_n261(A-G-I)","DC_66A_n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_066A_066A_n261zA_G_Iz ","DC_066A_n261G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A-66A_n261(G-J)","DC_66A_n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_066A_n261zG_Jz ","DC_066A_n261H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_2A-66A-71A_n71A","DC_66A_n71A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_066A_071A_n071A ","DC_066A_n071A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A-66A_n30A","DC_66A_n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_066A_n030A ","DC_066A_n030A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_2A-66A_n41A-n261(2A)","DC_2A_n41A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_n041A_n261z2Az ","DC_002A_n041A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A_n260H","DC_66A_n260A","Ongoing","PC3",null,null,"Verizon,AT&T","Verizon,AT&T (Jinwen Ma,Ron Borsato)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_002A_066A_n260H ","DC_066A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A_n260L","DC_2A_n260H","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_n260L ","DC_002A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A_n260M","DC_66A_n260K","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_066A_n260M ","DC_066A_n260K ","Fallback to DC_2A-2A-14A-66A_n260M with UL DC_66A_n260K","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A_n260(A-G)","DC_66A_n260A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_n260zA_Gz ","DC_066A_n260A ","Fallback to DC_2A-66A_n260(2A-2G) with UL DC_66A_n260A","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A_n261H","DC_66A_n261H","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_n261H ","DC_066A_n261H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A_n261(2A-H)","DC_2A_n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_n261z2A_Hz ","DC_002A_n261A ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_2A_n261A","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A_n261(A-G-H)","DC_66A_n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_n261zA_G_Hz ","DC_066A_n261A ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_66A_n261A","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A_n261(A-I)","DC_66A_n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_n261zA_Iz ","DC_066A_n261A ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_66A_n261A","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_2A-66A_n261(G-I)","DC_66A_n261I","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_066A_n261zG_Iz ","DC_066A_n261I ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_66A_n261I","v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A_n7A-n78A","DC_2A_n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_n007A_n078A ","DC_002A_n007A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A_n38A-n71A","DC_2A_n71A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_n038A_n071A ","DC_002A_n071A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_2A_n66A-n78(2A)","DC_2A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_n066A_n078z2Az ","DC_002A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_2A_n258G","DC_2A_n258A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_n258G ","DC_002A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_2A_n260K","DC_2A_n260I","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_n260K ","DC_002A_n260I ","Fallback to DC_2A-2A-5A_n260K with UL DC_2A_n260I","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_2A_n260(2P)","DC_2A_n260P","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_n260z2Pz ","DC_002A_n260P ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_2A_n260(4A-P)","DC_2A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_n260z4A_Pz ","DC_002A_n260A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_2A_n260(A-O-Q)","DC_2A_n260O","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_n260zA_O_Qz ","DC_002A_n260O ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_2A_n260(O-Q)","DC_2A_n260Q","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_n260zO_Qz ","DC_002A_n260Q ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_2A_n261Q","DC_2A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_002A_n261Q ","DC_002A_n261A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_2A_n261(A-I)","DC_2A_n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_n261zA_Iz ","DC_002A_n261A ","Fallback to DC_2A-5A_n261(H-I) with UL DC_2A_n261A","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_2A_n261(G-J)","DC_2A_n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_002A_n261zG_Jz ","DC_002A_n261H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_3A-3A-7A-7A-8A_n1A-n78A-n257A","DC_8A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_007A_008A_n001A_n078A_n257A ","DC_008A_n257A ","This FR1+FR2 config is not testable","v1.1.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-3A-7A-7A-8A_n78A-n257E","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_007A_008A_n078A_n257E ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-3A-7A-7A-8A_n257F","DC_8A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_007A_008A_n257F ","DC_008A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-3A-7A-7A_n1A-n78A-n257A","DC_7A_n1A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_007A_n001A_n078A_n257A ","DC_007A_n001A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-3A-7A-7A_n1A-n78A-n257G","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_007A_n001A_n078A_n257G ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-3A-7A-7A_n1A-n257I","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_007A_n001A_n257I ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-3A-7A-7A_n1A-n257J","DC_3A_n1A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_007A_n001A_n257J ","DC_003A_n001A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-3A-7A-7A_n78A-n257I","DC_7A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_007A_n078A_n257I ","DC_007A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-3A-7A-7A_n78A-n257L","DC_7A_n257J","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_007A_n078A_n257L ","DC_007A_n257J ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-3A-7A-7A_n257G","DC_3A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_007A_n257G ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-3A-7A-8A_n1A","DC_8A_n1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_003A_007A_008A_n001A ","DC_008A_n001A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-3A-7A-8A_n78A-n257E","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_008A_n078A_n257E ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.1.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-3A-7A-8A_n78A-n257I","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_008A_n078A_n257I ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-3A-7A-8A_n257L","DC_7A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_008A_n257L ","DC_007A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3A-3A-7A_n1A","DC_7A_n1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_003A_007A_n001A ","DC_007A_n001A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-3A-7A_n1A-n78A-n257K","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_n001A_n078A_n257K ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-3A-7A_n1A-n257I","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_n001A_n257I ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3A-3A-7A_n8A","DC_3A_n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_n008A ","DC_003A_n008A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-3A-7A_n78A-n257F","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_003A_007A_n078A_n257F ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-3A-7A_n78A-n257K","DC_3A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_n078A_n257K ","DC_003A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-3A-7A_n257I","DC_7A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_007A_n257I ","DC_007A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-3A-7A_n257M","DC_7A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_003A_007A_n257M ","DC_007A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3A-3A-8A_n78A","DC_8A_n78A PC2","Pending","PC2",null,null,null,null,null,"ENDC_PC2_R17_xLTE_yNR-UEConTest","DC_003A_003A_008A_n078A ","DC_008A_n078A PC002 ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-3A-8A_n78A-n257I","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_008A_n078A_n257I ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.1.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-3A-8A_n257M","DC_8A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_008A_n257M ","DC_008A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A-3A_n1A-n257E","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_n001A_n257E ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A-3A_n78A-n257H","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_003A_n078A_n257H ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A-3A_n78A-n257L","DC_3A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_003A_n078A_n257L ","DC_003A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A-7A_n78A-n257D","DC_3A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_007A_n078A_n257D ","DC_003A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A-7A_n78A-n257H","DC_3A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_007A_n078A_n257H ","DC_003A_n078A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A-7A_n78A-n257I","DC_7A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_007A_n078A_n257I ","DC_007A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A-7A_n78A-n257K","DC_3A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_007A_n078A_n257K ","DC_003A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A-7A_n78A-n257M","DC_5A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_007A_n078A_n257M ","DC_005A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A-7A_n78C-n257H","DC_3A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_007A_n078C_n257H ","DC_003A_n078A_n257H ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A-7A_n78C-n257J","DC_5A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_007A_n078C_n257J ","DC_005A_n257A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A-7A_n78C-n257L","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_007A_n078C_n257L ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A-7A_n78C-n257M","DC_5A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_007A_n078C_n257M ","DC_005A_n078A_n257A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-5A-7A-7A_n257H","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_005A_007A_007A_n257H ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-5A-7A-7A_n257M","DC_7A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_005A_007A_007A_n257M ","DC_007A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A_n78A-n257D","DC_5A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_005A_007A_n078A_n257D ","DC_005A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A_n78A-n257H","DC_5A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_005A_007A_n078A_n257H ","DC_005A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A_n78A-n257I","DC_7A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_n078A_n257I ","DC_007A_n078A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A_n78A-n257L","DC_3A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_n078A_n257L ","DC_003A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A_n78C-n257F","DC_3A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_n078C_n257F ","DC_003A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A_n78C-n257H","DC_5A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_n078C_n257H ","DC_005A_n078A ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A_n78C-n257J","DC_7A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_n078C_n257J ","DC_007A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-5A-7A_n78C-n257L","DC_3A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_n078C_n257L ","DC_003A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-5A-7A_n257D","DC_5A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_n257D ","DC_005A_n257D ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-5A-7A_n257K","DC_7A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_005A_007A_n257K ","DC_007A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-5A-7A_n257M","DC_7A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_007A_n257M ","DC_007A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-5A_n78A-n257G","DC_5A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_n078A_n257G ","DC_005A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-5A_n78A-n257M","DC_3A_n78A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_n078A_n257M ","DC_003A_n078A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-5A_n78C-n257H","DC_5A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_n078C_n257H ","DC_005A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-5A_n78C-n257M","DC_5A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_n078C_n257M ","DC_005A_n078A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-5A_n257H","DC_3A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_005A_n257H ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-5A_n257M","DC_5A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_005A_n257M ","DC_005A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-7A-7A-8A_n78A-n257H","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_007A_008A_n078A_n257H ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.1.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-7A-7A-8A_n78A-n257L","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_007A_008A_n078A_n257L ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-7A-7A-8A_n257M","DC_7A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_007A_008A_n257M ","DC_007A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-7A-7A_n1A-n78A-n257A","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_007A_n001A_n078A_n257A ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A-7A_n1A-n257A","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_007A_007A_n001A_n257A ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3A-7A-7A_n8A","DC_3A_n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_007A_n008A ","DC_003A_n008A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A-7A_n78A-n257D","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_007A_007A_n078A_n257D ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A-7A_n78A-n257I","DC_3A_n78A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_007A_n078A_n257I ","DC_003A_n078A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A-7A_n78A-n257J","DC_7A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_007A_n078A_n257J ","DC_007A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A-7A_n78A-n257M","DC_7A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_007A_n078A_n257M ","DC_007A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A-7A_n78C-n257G","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_007A_n078C_n257G ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A-7A_n78C-n257I","DC_3A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_007A_n078C_n257I ","DC_003A_n257G ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A-7A_n78C-n257K","DC_3A_n257J","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_007A_n078C_n257K ","DC_003A_n257J ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-7A-7A_n257E","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_007A_007A_n257E ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-7A-7A_n257I","DC_7A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_007A_n257I ","DC_007A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-7A-7A_n257M","DC_7A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_007A_007A_n257M ","DC_007A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (6 bands)","38.101-3:Table 5.5B.4.5-1","DC_3A-7A-8A-40A_n1A-n78A","DC_8A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_008A_040A_n001A_n078A ","DC_008A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_3A-7A-8A_n28A-n78A","DC_3A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_008A_n028A_n078A ","DC_003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-7A-8A_n40A-n258G","DC_7A_n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_008A_n040A_n258G ","DC_007A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-7A-8A_n40A-n258K","DC_8A_n40A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_008A_n040A_n258K ","DC_008A_n040A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-7A-8A_n78A-n257F","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_008A_n078A_n257F ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.1.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-7A-8A_n78A-n257J","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_008A_n078A_n257J ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.1.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-7A-8A_n78A-n258J","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_008A_n078A_n258J ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-7A-8A_n257G","DC_8A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_008A_n257G ","DC_008A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-7A-8A_n258E","DC_3A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_008A_n258E ","DC_003A_n258A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_3A-7A-20A-28A_n1A","DC_20A_n1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_020A_028A_n001A ","DC_020A_n001A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_3A-7A-20A_n38A-n78A","DC_3A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_020A_n038A_n078A ","DC_003A_n078A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-7A-28A_n78A-n257A","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_028A_n078A_n257A ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-7A-28A_n258B","DC_28A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_028A_n258B ","DC_028A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-7A-28A_n258H","DC_28A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_028A_n258H ","DC_028A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-7A-28A_n258J","DC_28A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_028A_n258J ","DC_028A_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-7A-32A_n28A","DC_7A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_032A_n028A ","DC_007A_n028A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-7A_n1A-n78A-n257D","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n001A_n078A_n257D ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-7A_n1A-n78A-n257K","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n001A_n078A_n257K ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n1A-n257E","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n001A_n257E ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-7A_n28A-n78A","DC_7A_n78A","Completed","PC3","<=RAN5#93-e","R5-216625","Orange","Orange (Hajer Khanfir)","<RAN5#94-e","TEI15_Test 5GS_NR_LTE-UEConTest","DC_003A_007A_n028A_n078A ","DC_007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n40A-n258K","DC_3A_n40A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n040A_n258K ","DC_003A_n040A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n78A-n257A","DC_3A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n078A_n257A ","DC_003A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n78A-n257G","DC_3A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n078A_n257G ","DC_003A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n78A-n257J","DC_3A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n078A_n257J ","DC_003A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n78A-n257M","DC_3A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n078A_n257M ","DC_003A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n78A-n258F","DC_3A_n258E","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n078A_n258F ","DC_003A_n258E ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n78A-n258I","DC_3A_n258I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n078A_n258I ","DC_003A_n258I ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n78A-n258K","DC_7A_n258I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n078A_n258K ","DC_007A_n258I ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n78C-n257F","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n078C_n257F ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n78C-n257J","DC_7A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n078C_n257J ","DC_007A_n257H ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n78C-n257L","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n078C_n257L ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-7A_n78C-n257M","DC_7A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n078C_n257M ","DC_007A_n257I ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-7A_n257H","DC_3A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n257H ","DC_003A_n257H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-7A_n257L","DC_7A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n257L ","DC_007A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-7A_n258J","DC_7A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n258J ","DC_007A_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-7A_n258M","DC_7A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007A_n258M ","DC_007A_n258I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-7C-28A_n258B","DC_3A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007C_028A_n258B ","DC_003A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-7C-28A_n258J","DC_7C_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007C_028A_n258J ","DC_007C_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-7C-28A_n258J","DC_7C_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007C_028A_n258J ","DC_007C_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-7C_n3A-n78A","DC_3A_n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007C_n003A_n078A ","DC_003A_n003A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-7C_n28A-n78A","DC_7A_n78A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_007C_n028A_n078A ","DC_007A_n078A ","Fallback to DC_3A-7C_n28A-n78A with UL DC_7A_n78A PC2","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-7C_n258F","DC_3A_n258F","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007C_n258F ","DC_003A_n258F ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-7C_n258L","DC_7A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_007C_n258L ","DC_007A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_3A-8A-11A_n28A-n77(2A)","DC_11A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_008A_011A_n028A_n077z2Az ","DC_011A_n028A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-8A-11A_n257I","DC_8A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_008A_011A_n257I ","DC_008A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-8A-32A_n78A","DC_3A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_008A_032A_n078A ","DC_003A_n078A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-8A_n1A-n28A","DC_8A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_008A_n001A_n028A ","DC_008A_n028A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-8A_n40A-n258H","DC_8A_n40A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_008A_n040A_n258H ","DC_008A_n040A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-8A_n77A-n79A","DC_3A_n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_008A_n077A_n079A ","DC_003A_n079A ",null,"v1.1.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-8A_n78A-n257J","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_008A_n078A_n257J ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-8A_n78A-n258E","DC_3A_n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_008A_n078A_n258E ","DC_003A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-8A_n257D","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_008A_n257D ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-8A_n258D","DC_8A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_008A_n258D ","DC_008A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-11A_n28A-n77(2A)","DC_3A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_011A_n028A_n077z2Az ","DC_003A_n028A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-18A-42A_n78A-n257G","DC_3A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_018A_042A_n078A_n257G ","DC_003A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-18A-42A_n78A-n257I","DC_18A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_018A_042A_n078A_n257I ","DC_018A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-18A-42A_n257K","DC_18A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_018A_042A_n257K ","DC_018A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-18A-42C_n78A-n257G","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_018A_042C_n078A_n257G ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-18A-42C_n78A-n257I","DC_3A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_018A_042C_n078A_n257I ","DC_003A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-18A-42C_n257G","DC_42C_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_018A_042C_n257G ","DC_042C_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-18A-42C_n257L","DC_18A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_018A_042C_n257L ","DC_018A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-18A-42C_n257M","DC_42C_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_018A_042C_n257M ","DC_042C_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-18A_n41A-n77A","DC_3A_n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_018A_n041A_n077A ","DC_003A_n041A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-18A_n78A-n257A","DC_18A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_018A_n078A_n257A ","DC_018A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-18A_n257H","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_018A_n257H ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_3A-19A-21A-42A_n257A","DC_19A_n257A","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_019A_021A_042A_n257A ","DC_019A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_3A-19A-21A-42C_n77C","DC_21A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_019A_021A_042C_n077C ","DC_021A_n077A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-19A-21A_n78A","DC_19A_n78A","Completed","PC3","<=RAN5#93-e","R5-216625","NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_003A_019A_021A_n078A ","DC_019A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-19A-42A_n1A","DC_42A_n1A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_019A_042A_n001A ","DC_042A_n001A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-19A-42A_n257I","DC_19A_n257A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_019A_042A_n257I ","DC_019A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-19A-42A_n257L","DC_42A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_019A_042A_n257L ","DC_042A_n257G ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_3A-19A-42C_n1A-n78A","DC_19A_n78A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_019A_042C_n001A_n078A ","DC_019A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-19A-42C_n257G","DC_19A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_019A_042C_n257G ","DC_019A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-19A-42C_n257J","DC_3A_n257G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_019A_042C_n257J ","DC_003A_n257G ","Fallback to DC_1A-3A-19A-42C_n257J with UL DC_3A_n257G","v1.2.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-19A-42D_n257D","DC_19A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_019A_042D_n257D ","DC_019A_n257D ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-19A_n77A-n257G","DC_3A_n77A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_019A_n077A_n257G ","DC_003A_n077A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-19A_n77A-n257I","DC_3A_n77A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_019A_n077A_n257I ","DC_003A_n077A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-19A_n78A-n257I","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_019A_n078A_n257I ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-19A_n78A-n257I","DC_19A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_019A_n078A_n257I ","DC_019A_n078A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-19A_n257D","DC_3A_n257D","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_019A_n257D ","DC_003A_n257D ","Fallback to DC_3A-19A-42C_n257D with UL DC_3A_n257D","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-19A_n257K","DC_3A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_019A_n257K ","DC_003A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-19A_n257M","DC_3A_n257M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_019A_n257M ","DC_003A_n257M ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-20A_n8A-n78A","DC_20A_n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_020A_n008A_n078A ","DC_020A_n008A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_3A-21A-42A_n1A-n79A","DC_3A_n1A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_021A_042A_n001A_n079A ","DC_003A_n001A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-21A-42A_n257E","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_021A_042A_n257E ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-21A-42A_n257J","DC_3A_n257H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_021A_042A_n257J ","DC_003A_n257H ","Fallback to DC_1A-3A-21A-42C_n257J with UL DC_3A_n257H","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-21A-42A_n257L","DC_3A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_021A_042A_n257L ","DC_003A_n257I ",null,"v1.2.0"]
[null,"Rel-15","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-21A-42C_n257F","DC_21A_n257A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_003A_021A_042C_n257F ","DC_021A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-21A-42C_n257J","DC_42A_n257H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_021A_042C_n257J ","DC_042A_n257H ","Fallback to DC_1A-3A-21A-42C_n257J with UL DC_42A_n257H","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-21A-42C_n257L","DC_42A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_021A_042C_n257L ","DC_042A_n257I ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-21A-42D_n257A","DC_3A_n257A","Ongoing","PC3",null,null,"NTT DOCOMO",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_021A_042D_n257A ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_3A-21A_n1A-n78A-n79A","DC_21A_n78A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_021A_n001A_n078A_n079A ","DC_021A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-21A_n77A-n257H","DC_21A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_021A_n077A_n257H ","DC_021A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-21A_n78A-n257G","DC_3A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_021A_n078A_n257G ","DC_003A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-21A_n78A-n257I","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_021A_n078A_n257I ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-21A_n79A-n257G","DC_3A_n79A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_021A_n079A_n257G ","DC_003A_n079A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-21A_n79A-n257I","DC_21A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_021A_n079A_n257I ","DC_021A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-21A_n257M","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_021A_n257M ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_3A-28A-41A-42A_n78A-n257H","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041A_042A_n078A_n257H ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_3A-28A-41A-42A_n78A-n257I","DC_41A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041A_042A_n078A_n257I ","DC_041A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_3A-28A-41A-42C_n78A-n257G","DC_41A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041A_042C_n078A_n257G ","DC_041A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_3A-28A-41A-42C_n78A-n257I","DC_42A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041A_042C_n078A_n257I ","DC_042A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_3A-28A-41A-42C_n257H","DC_28A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041A_042C_n257H ","DC_028A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_3A-28A-41A-42C_n257I","DC_42A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041A_042C_n257I ","DC_042A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-28A-41A_n78A-n257I","DC_28A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041A_n078A_n257I ","DC_028A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_3A-28A-41C-42A_n78A-n257G","DC_42A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041C_042A_n078A_n257G ","DC_042A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_3A-28A-41C-42A_n78A-n257I","DC_42A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041C_042A_n078A_n257I ","DC_042A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_3A-28A-41C-42A_n257H","DC_41A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041C_042A_n257H ","DC_041A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_3A-28A-41C-42A_n257I","DC_42A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041C_042A_n257I ","DC_042A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (6 bands)","38.101-3:Table 5.5B.6.5-1","DC_3A-28A-41C-42C_n78A-n257H","DC_41A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041C_042C_n078A_n257H ","DC_041A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (5 bands)","38.101-3:Table 5.5B.5.4-1","DC_3A-28A-41C-42C_n257H","DC_41A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041C_042C_n257H ","DC_041A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-28A-41C_n78A-n257A","DC_41A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041C_n078A_n257A ","DC_041A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-28A-41C_n78A-n257H","DC_28A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041C_n078A_n257H ","DC_028A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-28A-41C_n78A-n257I","DC_41A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041C_n078A_n257I ","DC_041A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-28A-41C_n257I","DC_41A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_041C_n257I ","DC_041A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-28A-42A_n257G","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_042A_n257G ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-28A-42A_n257J","DC_3A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_028A_042A_n257J ","DC_003A_n257H ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-28A-42C_n78A-n257A","DC_42C_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_042C_n078A_n257A ","DC_042C_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-28A-42C_n78A-n257I","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_042C_n078A_n257I ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-28A-42C_n257H","DC_3A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_042C_n257H ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-28A_n1A-n78A","DC_3A_n1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_028A_n001A_n078A ","DC_003A_n001A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3A-28A_n7B","DC_28A_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_n007B ","DC_028A_n007B ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-28A_n77A-n257I","DC_3A_n77A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_n077A_n257I ","DC_003A_n077A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-28A_n78A-n257H","DC_3A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_n078A_n257H ","DC_003A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-28A_n257D","DC_28A_n257A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_003A_028A_n257D ","DC_028A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-28A_n257K","DC_3A_n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_n257K ","DC_003A_n257J ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-28A_n257M","DC_28A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_028A_n257M ","DC_028A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-28A_n258J","DC_28A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_028A_n258J ","DC_028A_n258H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3A-40A_n78A","DC_40A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_040A_n078A ","DC_040A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-41A-42A_n77A-n257G","DC_41A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041A_042A_n077A_n257G ","DC_041A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-41A-42A_n78A-n257G","DC_41A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041A_042A_n078A_n257G ","DC_041A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-41A-42A_n78A-n257I","DC_42A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041A_042A_n078A_n257I ","DC_042A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-41A-42A_n257K","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041A_042A_n257K ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-41A-42C_n77A-n257G","DC_41A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041A_042C_n077A_n257G ","DC_041A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-41A-42C_n77A-n257I","DC_41A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041A_042C_n077A_n257I ","DC_041A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-41A-42C_n78A-n257H","DC_42A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041A_042C_n078A_n257H ","DC_042A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-41A-42C_n257A","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041A_042C_n257A ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-41A-42C_n257J","DC_42C_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041A_042C_n257J ","DC_042C_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-41A-42C_n257M","DC_41A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041A_042C_n257M ","DC_041A_n257H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-41A_n28A-n41A","DC_3A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_041A_n028A_n041A ","DC_003A_n028A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-41A_n41A-n77A","DC_3A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_041A_n041A_n077A ","DC_003A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-41A_n78A-n257I","DC_41A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041A_n078A_n257I ","DC_041A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-41A_n257I","DC_3A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041A_n257I ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-41C-42A_n77A-n257A","DC_3A_n77A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042A_n077A_n257A ","DC_003A_n077A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-41C-42A_n77A-n257H","DC_41A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042A_n077A_n257H ","DC_041A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-41C-42A_n78A-n257A","DC_41A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042A_n078A_n257A ","DC_041A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-41C-42A_n257G","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042A_n257G ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-41C-42A_n257I","DC_41C_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042A_n257I ","DC_041C_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-41C-42A_n257L","DC_41A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042A_n257L ","DC_041A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-41C-42A_n257M","DC_42A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042A_n257M ","DC_042A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-41C-42C_n77A-n257I","DC_42C_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042C_n077A_n257I ","DC_042C_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_3A-41C-42C_n78A-n257H","DC_42C_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042C_n078A_n257H ","DC_042C_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-41C-42C_n79A","DC_3A_n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042C_n079A ","DC_003A_n079A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-41C-42C_n257H","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042C_n257H ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-41C-42C_n257I","DC_42C_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042C_n257I ","DC_042C_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3A-41C-42C_n257M","DC_41A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_042C_n257M ","DC_041A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3A-41C_n28A-n78A","DC_3A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_n028A_n078A ","DC_003A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-41C_n28A-n257H","DC_41A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_n028A_n257H ","DC_041A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3A-41C_n77A","DC_41C_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_041C_n077A ","DC_041C_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-41C_n77A-n257I","DC_41C_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_n077A_n257I ","DC_041C_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-41C_n257F","DC_41A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_n257F ","DC_041A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-41C_n257K","DC_3A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_n257K ","DC_003A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-41C_n257M","DC_3A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_041C_n257M ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3A-42A_n77C","DC_3A_n77A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_003A_042A_n077C ","DC_003A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-42A_n79A-n257A","DC_3A_n79A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042A_n079A_n257A ","DC_003A_n079A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-42A_n79A-n257I","DC_3A_n79A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042A_n079A_n257I ","DC_003A_n079A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-42A_n257G","DC_3A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042A_n257G ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-42A_n257L","DC_3A_n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042A_n257L ","DC_003A_n257K ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-42C_n77A-n257I","DC_3A_n77A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042C_n077A_n257I ","DC_003A_n077A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-42C_n78A-n257I","DC_3A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042C_n078A_n257I ","DC_003A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-42C_n79A-n257G","DC_3A_n79A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042C_n079A_n257G ","DC_003A_n079A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A-42C_n79A-n257I","DC_42A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042C_n079A_n257I ","DC_042A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-42C_n257I","DC_42A_n257A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042C_n257I ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-42C_n257M","DC_42C_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042C_n257M ","DC_042C_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-42D_n257I","DC_3A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042D_n257I ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-42D_n257K","DC_3A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042D_n257K ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-42D_n257L","DC_42C_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042D_n257L ","DC_042C_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-42E_n257F","DC_42A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042E_n257F ","DC_042A_n257D ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3A-42E_n257K","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_042E_n257K ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3A_n1A-n7A","DC_3A_n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_n001A_n007A ","DC_003A_n007A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3A_n1A-n78A-n257G","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_n001A_n078A_n257G ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3A_n7A-n78A","DC_3A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_n007A_n078A ","DC_003A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3A_n7A-n78(2A)","DC_3A_n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_n007A_n078z2Az ","DC_003A_n007A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A_n40A-n258A","DC_3A_n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_n040A_n258A ","DC_003A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A_n40A-n258L","DC_3A_n40A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_n040A_n258L ","DC_003A_n040A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-15","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A_n77A-n257A","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_003A_n077A_n257A ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A_n77(2A)-n257H","DC_3A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_n077z2Az_n257H ","DC_003A_n257H ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A_n78A-n257H","DC_3A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_n078A_n257H ","DC_003A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A_n78A-n257K","DC_3A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_n078A_n257K ","DC_003A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A_n78A-n257M","DC_3A_n78A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_n078A_n257M ","DC_003A_n078A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A_n78A-n258L","DC_3A_n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_n078A_n258L ","DC_003A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A_n78C-n257K","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_n078C_n257K ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A_n78C-n257M","DC_3A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003A_n078C_n257M ","DC_003A_n257I ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A_n79A-n258A","DC_3A_n79A-n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_n079A_n258A ","DC_003A_n079A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3A_n79A-n258K","DC_3A_n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_n079A_n258K ","DC_003A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_3A_n257J","DC_3A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003A_n257J ","DC_003A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3C-5A_n78A","DC_3A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_005A_n078A ","DC_003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_3C-7A-20A_n28A-n78A","DC_7A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007A_020A_n028A_n078A ","DC_007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3C-7A-28A_n258A","DC_3A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007A_028A_n258A ","DC_003A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3C-7A-28A_n258G","DC_3A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007A_028A_n258G ","DC_003A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3C-7A-28A_n258K","DC_28A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007A_028A_n258K ","DC_028A_n258H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3C-7A_n1A","DC_3C_n1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003C_007A_n001A ","DC_003C_n001A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3C-7A_n7A-n78A","DC_7A_n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003C_007A_n007A_n078A ","DC_007A_n007A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3C-7A_n258E","DC_3A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007A_n258E ","DC_003A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3C-7A_n258K","DC_3C_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007A_n258K ","DC_003C_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3C-7A_n258M","DC_3C_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007A_n258M ","DC_003C_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3C-7C-28A_n258B","DC_7A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007C_028A_n258B ","DC_007A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3C-7C-28A_n258G","DC_3C_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007C_028A_n258G ","DC_003C_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3C-7C-28A_n258I","DC_28A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007C_028A_n258I ","DC_028A_n258H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_3C-7C-28A_n258M","DC_3A_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007C_028A_n258M ","DC_003A_n258I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3C-7C_n1A-n78A","DC_7A_n1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003C_007C_n001A_n078A ","DC_007A_n001A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3C-7C_n78(2A)","DC_3A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003C_007C_n078z2Az ","DC_003A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3C-7C_n258E","DC_7C_n258D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007C_n258E ","DC_007C_n258D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3C-7C_n258J","DC_3A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007C_n258J ","DC_003A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3C-7C_n258L","DC_7A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_007C_n258L ","DC_007A_n258H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3C-8A_n1A","DC_8A_n1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003C_008A_n001A ","DC_008A_n001A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_3C-8A_n78A-n257J","DC_8A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_008A_n078A_n257J ","DC_008A_n078A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3C-8A_n257F","DC_3A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_008A_n257F ","DC_003A_n257D ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3C-20A_n1A","DC_20A_n1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003C_020A_n001A ","DC_020A_n001A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_3C-20A_SUL_n78A-n80A","DC_3A_n80A_ULSUP-TDM_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003C_020A_n078A_n080A ","DC_003A_n080A_ULSUP_TDM_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3C-28A_n7B","DC_28A_n7B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003C_028A_n007B ","DC_028A_n007B ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3C-28A_n258K","DC_28A_n258J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_028A_n258K ","DC_028A_n258J ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_3C-28A_n258K","DC_28A_n258K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_028A_n258K ","DC_028A_n258K ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3C_n5A-n78A","DC_3A_n78A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003C_n005A_n078A ","DC_003A_n078A ","Fallback to DC_1A-3C_n5A-n78A with UL DC_3A_n78A","v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_3C_SUL_n41A-n80A","DC_3C_n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003C_n041A_n080A ","DC_003C_n041A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_3C_n78A-n257J","DC_3A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003C_n078A_n257J ","DC_003A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_3C_n257M","DC_3A_n257M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_003C_n257M ","DC_003A_n257M ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_3C_n258K","DC_3A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_003C_n258K ","DC_003A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_4A_n2A","DC_4A_n2A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_004A_n002A ","DC_004A_n002A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_4A_n260(2A-3G)","DC_4A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_004A_n260z2A_3Gz ","DC_004A_n260G ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_4A_n260(2A-H)","DC_4A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_004A_n260z2A_Hz ","DC_004A_n260G ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_4A_n260(3A-O)","DC_4A_n260O","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_004A_n260z3A_Oz ","DC_004A_n260O ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_4A_n260(A-2D)","DC_4A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_004A_n260zA_2Dz ","DC_004A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_4A_n260(A-4G)","DC_4A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_004A_n260zA_4Gz ","DC_004A_n260G ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_4A_n260(A-G)","DC_4A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_004A_n260zA_Gz ","DC_004A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_4A_n260(G-3O)","DC_4A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_004A_n260zG_3Oz ","DC_004A_n260G ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_4A_n261(2A-I)","DC_4A_n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_004A_n261z2A_Iz ","DC_004A_n261G ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_4A_n261(A-H-I)","DC_4A_n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_004A_n261zA_H_Iz ","DC_004A_n261H ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_5A-5A-66A-66A_n2A","DC_5A_n2A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_005A_066A_066A_n002A ","DC_005A_n002A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_5A-7A-7A_n78A-n257A","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_005A_007A_007A_n078A_n257A ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_5A-7A-7A_n78A-n257I","DC_5A_n78A-n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_007A_007A_n078A_n257I ","DC_005A_n078A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_5A-7A-7A_n78C-n257F","DC_7A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_007A_007A_n078C_n257F ","DC_007A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_5A-7A-7A_n78C-n257L","DC_7A_n78A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_007A_007A_n078C_n257L ","DC_007A_n078A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-7A-7A_n257F","DC_7A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_007A_007A_n257F ","DC_007A_n257D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_5A-7A-66A_n66A","DC_66A_n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_007A_066A_n066A ","DC_066A_n066A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_5A-7A_n78A-n257F","DC_5A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_007A_n078A_n257F ","DC_005A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_5A-7A_n78A-n257H","DC_7A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_007A_n078A_n257H ","DC_007A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_5A-7A_n78A-n257K","DC_5A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_007A_n078A_n257K ","DC_005A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_5A-7A_n78C-n257E","DC_5A_n78A-n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_007A_n078C_n257E ","DC_005A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-7A_n257E","DC_7A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_007A_n257E ","DC_007A_n257D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-7A_n257L","DC_5A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_007A_n257L ","DC_005A_n257H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_5A-7C_n66A","DC_5A_n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_007C_n066A ","DC_005A_n066A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_5A-30A-66A-66A_n260A","DC_5A_n260A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_030A_066A_066A_n260A ","DC_005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_5A-30A-66A-66A_n260J","DC_66A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_030A_066A_066A_n260J ","DC_066A_n260G ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_5A-30A-66A-66A_n260M","DC_66A_n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_030A_066A_066A_n260M ","DC_066A_n260L ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_5A-30A-66A_n260H","DC_5A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_030A_066A_n260H ","DC_005A_n260H ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_5A-30A-66A_n260K","DC_30A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_030A_066A_n260K ","DC_030A_n260G ",null,"v1.1.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_5A-30A-66A_n260L","DC_66A_n260A","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_030A_066A_n260L ","DC_066A_n260A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-30A_n260A","DC_5A_n260A","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Samsung (Carolyn Taylor)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_005A_030A_n260A ","DC_005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-30A_n260M","DC_30A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_030A_n260M ","DC_030A_n260G ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_5A-48A_n12A","DC_48A_n12A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_048A_n012A ","DC_048A_n012A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_5A-66A-66A_n7A","DC_66A_n7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_066A_066A_n007A ","DC_066A_n007A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A-66A_n260H","DC_66A_n260H","Ongoing","PC3",null,null,"Verizon,AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_066A_066A_n260H ","DC_066A_n260H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A-66A_n260L","DC_66A_n260I","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_066A_066A_n260L ","DC_066A_n260I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A-66A_n261L","DC_5A_n261K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_066A_066A_n261L ","DC_005A_n261K ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A-66A_n261(2A-G)","DC_66A_n261A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_066A_066A_n261z2A_Gz ","DC_066A_n261A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A-66A_n261(A-G-H)","DC_5A_n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_066A_066A_n261zA_G_Hz ","DC_005A_n261G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A-66A_n261(G-I)","DC_66A_n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_066A_066A_n261zG_Iz ","DC_066A_n261A ","Fallback to DC_5A-66A-66A_n261(H-I) with UL DC_66A_n261A","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_5A-66A_n2A-n77A","DC_66A_n2A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_066A_n002A_n077A ","DC_066A_n002A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_5A-66A_n66A-n77C","DC_5A_n77A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_066A_n066A_n077C ","DC_005A_n077A ","Fallback to DC_5A-66A_n66A-n77C with UL DC_5A_n77A PC2","v1.1.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A_n260G","DC_66A_n260G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_066A_n260G ","DC_066A_n260G ","Fallback to DC_5A-66A-66A_n260G with UL DC_66A_n260G","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A_n260L","DC_5A_n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_066A_n260L ","DC_005A_n260J ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A_n261K","DC_66A_n261K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_066A_n261K ","DC_066A_n261K ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A_n261M","DC_66A_n261I","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_066A_n261M ","DC_066A_n261I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A_n261(4A)","DC_66A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_066A_n261z4Az ","DC_066A_n261A ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A_n261(A-H)","DC_5A_n261H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_066A_n261zA_Hz ","DC_005A_n261H ","Fallback to DC_5A-66A-66A_n261(H-I) with UL DC_5A_n261H","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_5A-66A_n261(H-I)","DC_66A_n261I","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_066A_n261zH_Iz ","DC_066A_n261I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_5A_n48B","DC_5A_n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n048B ","DC_005A_n048A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_5A_n78A-n257G","DC_5A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n078A_n257G ","DC_005A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n257D","DC_5A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_n257D ","DC_005A_n257D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n258Q","DC_5A_n258Q","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_n258Q ","DC_005A_n258Q ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260O","DC_5A_n260O","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e,RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n260O ","DC_005A_n260O ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(2A-2P)","DC_5A_n260O","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n260z2A_2Pz ","DC_005A_n260O ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(2A-D-2O)","DC_5A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n260z2A_D_2Oz ","DC_005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(2A-O-Q)","DC_5A_n260P","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_n260z2A_O_Qz ","DC_005A_n260P ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(3A-2G)","DC_5A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n260z3A_2Gz ","DC_005A_n260G ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(3A-D-O)","DC_5A_n260O","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_n260z3A_D_Oz ","DC_005A_n260O ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(3A-Q)","DC_5A_n260O","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_n260z3A_Qz ","DC_005A_n260O ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(4A-2P)","DC_5A_n260O","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_n260z4A_2Pz ","DC_005A_n260O ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(5A-Q)","DC_5A_n260P","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_n260z5A_Qz ","DC_005A_n260P ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(A-2G-O)","DC_5A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n260zA_2G_Oz ","DC_005A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(A-2O)","DC_5A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n260zA_2Oz ","DC_005A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(A-G-2O)","DC_5A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_n260zA_G_2Oz ","DC_005A_n260G ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(A-I)","DC_5A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n260zA_Iz ","DC_005A_n260H ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(G-2O)","DC_5A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n260zG_2Oz ","DC_005A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n260(O-P)","DC_5A_n260O","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n260zO_Pz ","DC_005A_n260O ",null,"v1.4.0"]
[null,"Rel-15","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n261J","DC_5A_n261A","Ongoing","PC3",null,null,"Verizon","Verizon (Jinwen Ma)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_005A_n261J ","DC_005A_n261A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n261(2A-G-2O)","DC_5A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_n261z2A_G_2Oz ","DC_005A_n261A ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n261(2H)","DC_5A_n261H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n261z2Hz ","DC_005A_n261H ","Fallback to DC_2A-5A_n261(H-I) with UL DC_5A_n261H","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n261(A-3G)","DC_5A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_005A_n261zA_3Gz ","DC_005A_n261A ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n261(A-I)","DC_5A_n261I","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n261zA_Iz ","DC_005A_n261I ","Fallback to DC_2A-5A_n261(H-I) with UL DC_5A_n261I","v1.0.0"]
[null,"Rel-15","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n261(D-I)","DC_5A_n261A","Ongoing","PC3",null,null,"Verizon","Verizon (Jinwen Ma)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_005A_n261zD_Iz ","DC_005A_n261A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_5A_n261(H-I)","DC_5A_n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_005A_n261zH_Iz ","DC_005A_n261A ","Fallback to DC_2A-5A_n261(H-I) with UL DC_5A_n261A","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_7A-7A-8A_n78A-n257A","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_007A_008A_n078A_n257A ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.1.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_7A-7A-8A_n257M","DC_8A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_007A_008A_n257M ","DC_008A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_7A-7A-66A-66A_n78A","DC_7A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_007A_007A_066A_066A_n078A ","DC_007A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_7A-7A-66A_n78A","DC_66A_n78A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_007A_007A_066A_n078A ","DC_066A_n078A ","Fallback to DC_2A-7A-7A-66A_n66A-n78A with UL DC_66A_n78A","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_7A-7A_n1A-n257M","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_007A_n001A_n257M ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_7A-7A_n78A-n257I","DC_7A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_007A_n078A_n257I ","DC_007A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_7A-7A_n78A-n257M","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_007A_007A_n078A_n257M ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_7A-7A_n78C-n257H","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_007A_n078C_n257H ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_7A-7A_n78C-n257M","DC_7A_n257K","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_007A_n078C_n257M ","DC_007A_n257K ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_7A-8A-40A_n1A","DC_8A_n1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_008A_040A_n001A ","DC_008A_n001A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_7A-8A_n1A-n78A-n257A","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_008A_n001A_n078A_n257A ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.1.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_7A-8A_n40A-n258E","DC_8A_n40A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_008A_n040A_n258E ","DC_008A_n040A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_7A-8A_n40A-n258I","DC_8A_n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_008A_n040A_n258I ","DC_008A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_7A-8A_n78A-n257H","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_008A_n078A_n257H ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.1.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_7A-8A_n78A-n258M","DC_7A_n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_008A_n078A_n258M ","DC_007A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_7A-8A_n258J","DC_7A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_008A_n258J ","DC_007A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_7A-12A_n66A-n78A","DC_12A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_012A_n066A_n078A ","DC_012A_n078A ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_7A-20A-28A-38A_n1A","DC_28A_n1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_020A_028A_038A_n001A ","DC_028A_n001A ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_7A-20A_n8A-n78A","DC_20A_n8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_020A_n008A_n078A ","DC_020A_n008A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_7A-28A_n5A-n78A","DC_7A_n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_007A_028A_n005A_n078A ","DC_007A_n005A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_7A-28A_n78A-n257A","DC_28A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_028A_n078A_n257A ","DC_028A_n257A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_7A-28A_n258E","DC_7A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_028A_n258E ","DC_007A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_7A-40A_n1A-n78A","DC_7A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_040A_n001A_n078A ","DC_007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_7A-40A_n1A-n78A","DC_40A_n1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_040A_n001A_n078A ","DC_040A_n001A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_7A-66A_n66A-n78A","DC_66A_n66A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_007A_066A_n066A_n078A ","DC_066A_n066A ","Fallback to DC_2A-7A-7A-66A_n66A-n78A with UL DC_66A_n66A","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_7A-71A_n66A-n78A","DC_71A_n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_071A_n066A_n078A ","DC_071A_n066A ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_7A_n1A-n78A-n257K","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_n001A_n078A_n257K ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_7A_n40A-n78A","DC_7A_n40A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_n040A_n078A ","DC_007A_n040A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_7A_n78A-n79C","DC_7A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_n078A_n079C ","DC_007A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_7A_n78A-n257J","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_007A_n078A_n257J ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_7A_n78A-n257M","DC_7A_n257K","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_n078A_n257M ","DC_007A_n257K ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_7A_n78C","DC_7A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_n078C ","DC_007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_7A_n79A-n257J","DC_7A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_n079A_n257J ","DC_007A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_7A_n79A-n257M","DC_7A_n257J","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_n079A_n257M ","DC_007A_n257J ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_7A_n79A-n258M","DC_7A_n258G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_n079A_n258M ","DC_007A_n258G ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_7A_n257J","DC_7A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007A_n257J ","DC_007A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_7A_n258F","DC_7A_n258D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_007A_n258F ","DC_007A_n258D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_7C-25A-25A-66A_n77A","DC_7A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007C_025A_025A_066A_n077A ","DC_007A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_7C-28A_n3A","DC_7A_n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_007C_028A_n003A ","DC_007A_n003A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_7C-28A_n258F","DC_7A_n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007C_028A_n258F ","DC_007A_n258A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_7C-28A_n258I","DC_7C_n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007C_028A_n258I ","DC_007C_n258I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_7C-66A_n25A","DC_7A_n25A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007C_066A_n025A ","DC_007A_n025A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_7C_n5A-n78A","DC_7A_n78A","Completed","PC3","RAN5#95-e","R5-223209","Telstra","Ericsson (Leif Mattisson)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_007C_n005A_n078A ","DC_007A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_7C_n78A-n258A","DC_7A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007C_n078A_n258A ","DC_007A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_7C_n78A-n258K","DC_7A_n258H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_007C_n078A_n258K ","DC_007A_n258H ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_7C_n258F","DC_7A_n258B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_007C_n258F ","DC_007A_n258B ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_7C_n258J","DC_7A_n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_007C_n258J ","DC_007A_n258H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_7C_n258M","DC_7A_n258M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_007C_n258M ","DC_007A_n258M ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_8A-11A_n3A-n28A-n77A","DC_8A_n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_008A_011A_n003A_n028A_n077A ","DC_008A_n003A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_8A-11A_n77A","DC_11A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_008A_011A_n077A ","DC_011A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_8A-11A_n77(2A)-n257H","DC_11A_n77A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_008A_011A_n077z2Az_n257H ","DC_011A_n077A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_8A-11A_n257D","DC_11A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_008A_011A_n257D ","DC_011A_n257D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_8A-28A_n78A","DC_28A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_008A_028A_n078A ","DC_028A_n078A ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_8A-40C_n78A","DC_8A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_008A_040C_n078A ","DC_008A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_8A-42A_n3A-n28A-n77(2A)","DC_8A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_008A_042A_n003A_n028A_n077z2Az ","DC_008A_n028A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_8A-42C_n3A-n28A","DC_42A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_008A_042C_n003A_n028A ","DC_042A_n028A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_8A-42C_n3A-n77(2A)","DC_42A_n3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_008A_042C_n003A_n077z2Az ","DC_042A_n003A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_8A_n3A-n28A","DC_8A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_008A_n003A_n028A ","DC_008A_n028A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_8A_n3A-n78A","DC_8A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_008A_n003A_n078A ","DC_008A_n078A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_8A_n40A-n258K","DC_8A_n40A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_008A_n040A_n258K ","DC_008A_n040A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_8A_n77(2A)-n257A","DC_8A_n77A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_008A_n077z2Az_n257A ","DC_008A_n077A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_8A_n78A-n257A","DC_8A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_008A_n078A_n257A ","DC_008A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_8A_n257I","DC_8A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_008A_n257I ","DC_008A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_8A_n257I","DC_8A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_008A_n257I ","DC_008A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_11A-18A_n257I","DC_18A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_011A_018A_n257I ","DC_018A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_11A_n77A-n257G","DC_11A_n77A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_011A_n077A_n257G ","DC_011A_n077A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_11A_n77(2A)-n257H","DC_11A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_011A_n077z2Az_n257H ","DC_011A_n257G ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_12A-30A-66A-66A_n260J","DC_12A_n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_030A_066A_066A_n260J ","DC_012A_n260I ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_12A-30A-66A-66A_n260L","DC_30A_n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_030A_066A_066A_n260L ","DC_030A_n260J ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_12A-30A-66A-66A_n260M","DC_30A_n260M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_030A_066A_066A_n260M ","DC_030A_n260M ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_12A-30A-66A_n260I","DC_12A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_030A_066A_n260I ","DC_012A_n260H ",null,"v1.1.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_12A-30A-66A_n260K","DC_12A_n260A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_012A_030A_066A_n260K ","DC_012A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_12A-30A_n5A","DC_12A_n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_030A_n005A ","DC_012A_n005A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_12A-30A_n260K","DC_12A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_030A_n260K ","DC_012A_n260G ",null,"v1.2.0"]
[null,"Rel-15","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_12A-30A_n260M","DC_12A_n260A","Ongoing","PC3",null,null,"AT&T","AT&T (Ron Borsato)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_012A_030A_n260M ","DC_012A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_12A-66A-66A_n2A","DC_66A_n2A","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_012A_066A_066A_n002A ","DC_066A_n002A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_12A-66A-66A_n260K","DC_12A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_066A_066A_n260K ","DC_012A_n260H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_12A-66A_n78(2A)","DC_66A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_066A_n078z2Az ","DC_066A_n078A ",null,"v1.1.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_12A-66A_n260K","DC_66A_n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_066A_n260K ","DC_066A_n260J ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_12A_n7A-n66A","DC_12A_n7A","Ongoing","PC3",null,null,"Rogers",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_n007A_n066A ","DC_012A_n007A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_12A_n7A-n78(2A)","DC_12A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_012A_n007A_n078z2Az ","DC_012A_n078A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_12A_n258P","DC_12A_n258P","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_n258P ","DC_012A_n258P ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_12A_n261C","DC_12A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_n261C ","DC_012A_n261A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_12A_n261L","DC_12A_n261J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_012A_n261L ","DC_012A_n261J ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-46A-46A_n261G","DC_13A_n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_013A_046A_046A_n261G ","DC_013A_n261G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-46A_n261J","DC_13A_n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_013A_046A_n261J ","DC_013A_n261I ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_13A-48A-66A_n77A","DC_66A_n77A PC2","Ongoing","PC2",null,null,"Verizon",null,"RAN5#94-e","ENDC_PC2_R17_xLTE_yNR-UEConTest","DC_013A_048A_066A_n077A ","DC_066A_n077A PC002 ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_13A-48C_n77A","DC_13A_n77A PC2","Ongoing","PC2",null,null,"Verizon",null,"RAN5#94-e","ENDC_PC2_R17_xLTE_yNR-UEConTest","DC_013A_048C_n077A ","DC_013A_n077A PC002 ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_13A-66A-66A_n5A-n77C","DC_66A_n5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_013A_066A_066A_n005A_n077C ","DC_066A_n005A ",null,"v1.1.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A-66A_n260J","DC_66A_n260I","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_066A_066A_n260J ","DC_066A_n260I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A-66A_n260(3A-G)","DC_13A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_013A_066A_066A_n260z3A_Gz ","DC_013A_n260G ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A-66A_n261H","DC_66A_n261G","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_066A_066A_n261H ","DC_066A_n261G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A-66A_n261K","DC_13A_n261K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_013A_066A_066A_n261K ","DC_013A_n261K ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A-66A_n261M","DC_13A_n261J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_013A_066A_066A_n261M ","DC_013A_n261J ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A-66A_n261(2H)","DC_66A_n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_066A_066A_n261z2Hz ","DC_066A_n261H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A-66A_n261(A-L)","DC_66A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_013A_066A_066A_n261zA_Lz ","DC_066A_n261A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A-66A_n261(G-J)","DC_66A_n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_013A_066A_066A_n261zG_Jz ","DC_066A_n261I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_13A-66A_n66A-n77A","DC_13A_n66A","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_013A_066A_n066A_n077A ","DC_013A_n066A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A_n260H","DC_13A_n260G","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_066A_n260H ","DC_013A_n260G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A_n260L","DC_13A_n260L","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_013A_066A_n260L ","DC_013A_n260L ","Fallback to DC_2A-13A-66A_n260M with UL DC_13A_n260L","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A_n260(A-H)","DC_13A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_013A_066A_n260zA_Hz ","DC_013A_n260G ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A_n261I","DC_13A_n261H","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_066A_n261I ","DC_013A_n261H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A_n261L","DC_66A_n261L","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_013A_066A_n261L ","DC_066A_n261L ","Fallback to DC_2A-13A-66A_n261M with UL DC_66A_n261L","v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A_n261(2A-H)","DC_66A_n261G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_066A_n261z2A_Hz ","DC_066A_n261G ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_66A_n261G","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A_n261(A-G-I)","DC_13A_n261G","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_066A_n261zA_G_Iz ","DC_013A_n261G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_13A-66A_n261(G-J)","DC_13A_n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_066A_n261zG_Jz ","DC_013A_n261H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_13A_n5A","DC_13A_n5A","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_n005A ","DC_013A_n005A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_13A_n260J","DC_13A_n260A","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_n260J ","DC_013A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_13A_n260(2G)","DC_13A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_n260z2Gz ","DC_013A_n260G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_13A_n260(3G)","DC_13A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_n260z3Gz ","DC_013A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_13A_n260(A-G)","DC_13A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_n260zA_Gz ","DC_013A_n260G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_13A_n260(G-H)","DC_13A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_n260zG_Hz ","DC_013A_n260G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_13A_n261M","DC_13A_n261A","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_n261M ","DC_013A_n261A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_13A_n261(A-2G)","DC_13A_n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_013A_n261zA_2Gz ","DC_013A_n261A ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_13A_n261A","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_14A-30A-66A-66A_n260G","DC_14A_n260G","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_014A_030A_066A_066A_n260G ","DC_014A_n260G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_14A-30A-66A-66A_n260K","DC_14A_n260A","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_014A_030A_066A_066A_n260K ","DC_014A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_14A-30A-66A-66A_n260L","DC_30A_n260A","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_014A_030A_066A_066A_n260L ","DC_030A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_14A-30A-66A_n260H","DC_66A_n260A","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_014A_030A_066A_n260H ","DC_066A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_14A-30A-66A_n260K","DC_30A_n260K","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_014A_030A_066A_n260K ","DC_030A_n260K ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_14A-30A-66A_n260L","DC_66A_n260J","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_014A_030A_066A_n260L ","DC_066A_n260J ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_14A-30A_n260G","DC_14A_n260A","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_014A_030A_n260G ","DC_014A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_14A-30A_n260J","DC_30A_n260H","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_014A_030A_n260J ","DC_030A_n260H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_14A-66A-66A_n260H","DC_66A_n260G","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_014A_066A_066A_n260H ","DC_066A_n260G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_14A-66A-66A_n260L","DC_66A_n260H","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_014A_066A_066A_n260L ","DC_066A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_14A-66A_n30A","DC_14A_n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_014A_066A_n030A ","DC_014A_n030A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_14A-66A_n260K","DC_14A_n260G","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_014A_066A_n260K ","DC_014A_n260G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_14A_n260K","DC_14A_n260G","Ongoing","PC3",null,null,"AT&T","Bureau Veritas,Sporton (Amy Tao,Ivan Cheng)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_014A_n260K ","DC_014A_n260G ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_18A-28A_n79A","DC_28A_n79A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_018A_028A_n079A ","DC_028A_n079A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_18A-41A_n77A","DC_18A_n77A","Ongoing","PC3",null,null,"KDDI","KDDI (Taiki Matsuyoshi)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_018A_041A_n077A ","DC_018A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_18A-41C_n3A","DC_41A_n3A","Ongoing","PC3",null,null,"KDDI","KDDI (Taiki Matsuyoshi)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_018A_041C_n003A ","DC_041A_n003A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_18A-41C_n257G","DC_18A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_018A_041C_n257G ","DC_018A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_18A-42A_n78A-n257H","DC_42A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_018A_042A_n078A_n257H ","DC_042A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_18A-42A_n257H","DC_18A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_018A_042A_n257H ","DC_018A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_18A-42A_n257M","DC_18A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_018A_042A_n257M ","DC_018A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_18A-42C_n78A-n257H","DC_42C_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_018A_042C_n078A_n257H ","DC_042C_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_18A-42C_n257J","DC_42C_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_018A_042C_n257J ","DC_042C_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_18A_n3A-n41A","DC_18A_n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_018A_n003A_n041A ","DC_018A_n041A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_18A_n28A-n77(2A)","DC_18A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_018A_n028A_n077z2Az ","DC_018A_n077A ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_18A_n257H","DC_18A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_018A_n257H ","DC_018A_n257H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_19A-21A-42A_n1A-n77A","DC_19A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_019A_021A_042A_n001A_n077A ","DC_019A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_19A-21A-42A_n78A-n257G","DC_19A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_021A_042A_n078A_n257G ","DC_019A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_19A-21A-42A_n79A-n257G","DC_19A_n79A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_021A_042A_n079A_n257G ","DC_019A_n079A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_19A-21A-42A_n79A-n257I","DC_21A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_021A_042A_n079A_n257I ","DC_021A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_19A-21A-42A_n257F","DC_19A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_021A_042A_n257F ","DC_019A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_19A-21A-42A_n257J","DC_42A_n257A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_019A_021A_042A_n257J ","DC_042A_n257A ","Fallback to DC_1A-19A-21A-42A_n257J with UL DC_42A_n257A","v1.2.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_19A-21A-42C_n77A-n257G","DC_19A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_021A_042C_n077A_n257G ","DC_019A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_19A-21A-42C_n78A-n257A","DC_21A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_021A_042C_n078A_n257A ","DC_021A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_19A-21A-42C_n78A-n257H","DC_21A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_021A_042C_n078A_n257H ","DC_021A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_19A-21A-42C_n257E","DC_19A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_021A_042C_n257E ","DC_019A_n257D ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_19A-21A-42C_n257J","DC_19A_n257I","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_019A_021A_042C_n257J ","DC_019A_n257I ","Fallback to DC_1A-19A-21A-42C_n257J with UL DC_19A_n257I","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_19A-21A-42C_n257L","DC_21A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_019A_021A_042C_n257L ","DC_021A_n257A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_19A-21A_n1A-n77A","DC_21A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_019A_021A_n001A_n077A ","DC_021A_n077A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_19A-21A_n77C","DC_19A_n77A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_019A_021A_n077C ","DC_019A_n077A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_19A-21A_n79A-n257I","DC_21A_n79A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_021A_n079A_n257I ","DC_021A_n079A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_19A-21A_n257J","DC_19A_n257H","Ongoing","PC3",null,null,"NTT DOCOMO",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_021A_n257J ","DC_019A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_19A-21A_n257L","DC_21A_n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_021A_n257L ","DC_021A_n257J ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (5 bands)","38.101-3:Table 5.5B.4.4-1","DC_19A-42A_n1A-n77A-n79A","DC_19A_n1A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_019A_042A_n001A_n077A_n079A ","DC_019A_n001A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_19A-42A_n78A-n257A","DC_19A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_042A_n078A_n257A ","DC_019A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_19A-42A_n257G","DC_19A_n257A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_042A_n257G ","DC_019A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_19A-42A_n257L","DC_42A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_019A_042A_n257L ","DC_042A_n257I ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_19A-42C_n77A-n257G","DC_19A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_042C_n077A_n257G ","DC_019A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_19A-42C_n78A-n257A","DC_42A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_042C_n078A_n257A ","DC_042A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_19A-42C_n79A-n257I","DC_19A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_042C_n079A_n257I ","DC_019A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_19A-42C_n257M","DC_19A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_019A_042C_n257M ","DC_019A_n257G ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_19A-42D_n257F","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_042D_n257F ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_19A_n77A-n257H","DC_19A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_n077A_n257H ","DC_019A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_19A_n78C-n257D","DC_19A_n78A-n257A","N/A","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_019A_n078C_n257D ","DC_019A_n078A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_19A_n78C-n257D","DC_19A_n257A","N/A","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_019A_n078C_n257D ","DC_019A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_19A_n257I","DC_19A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_n257I ","DC_019A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_19A_n257M","DC_19A_n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_019A_n257M ","DC_019A_n257J ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_20A-38A_n78(2A)","DC_20A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_020A_038A_n078z2Az ","DC_020A_n078A ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_20A_n78(2A)-n92A","DC_20A_n92A_ULSUP-TDM_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_020A_n078z2Az_n092A ","DC_020A_n092A_ULSUP_TDM_n078A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_21A-28A-42A_n257A","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_021A_028A_042A_n257A ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_21A-28A_n257D","DC_21A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_028A_n257D ","DC_021A_n257D ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_21A-42A_n77A-n257A","DC_42A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042A_n077A_n257A ","DC_042A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_21A-42A_n78A-n257G","DC_21A_n78A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042A_n078A_n257G ","DC_021A_n078A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_21A-42A_n257A","DC_21A_n257A","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_021A_042A_n257A ","DC_021A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_21A-42A_n257I","DC_21A_n257G","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042A_n257I ","DC_021A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_21A-42A_n257M","DC_21A_n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042A_n257M ","DC_021A_n257J ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_21A-42C_n77A-n257G","DC_21A_n77A-n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042C_n077A_n257G ","DC_021A_n077A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_21A-42C_n78A-n257G","DC_42A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042C_n078A_n257G ","DC_042A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_21A-42C_n79A-n257H","DC_21A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042C_n079A_n257H ","DC_021A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_21A-42C_n257I","DC_21A_n257I","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042C_n257I ","DC_021A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_21A-42C_n257M","DC_21A_n257L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042C_n257M ","DC_021A_n257L ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_21A-42D_n257F","DC_42A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042D_n257F ","DC_042A_n257D ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_21A-42E_n79A","DC_21A_n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042E_n079A ","DC_021A_n079A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_21A-42E_n257J","DC_42A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042E_n257J ","DC_042A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_21A-42E_n257M","DC_21A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_042E_n257M ","DC_021A_n257H ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_21A_n77A-n257A","DC_21A_n257A","N/A","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_021A_n077A_n257A ","DC_021A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_21A_n79A-n257H","DC_21A_n79A-n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_n079A_n257H ","DC_021A_n079A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_21A_n257I","DC_21A_n257H","Ongoing","PC3",null,null,"NTT DOCOMO","NTT DOCOMO (Takashi Akao)","RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_021A_n257I ","DC_021A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_25A-25A-(n)41AA","DC_25A_n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_025A_025A_znz041AA ","DC_025A_n041A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_25A-(n)41CA","DC_(n)41AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_025A_znz041CA ","DC_znz041AA ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_28A-41A-42A_n78A-n257H","DC_41A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_041A_042A_n078A_n257H ","DC_041A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_28A-41A-42C_n78A-n257G","DC_42C_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_041A_042C_n078A_n257G ","DC_042C_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_28A-41A-42C_n78A-n257I","DC_41A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_041A_042C_n078A_n257I ","DC_041A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_28A-41A-42C_n257I","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_041A_042C_n257I ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_28A-41A_n78A-n257H","DC_28A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_041A_n078A_n257H ","DC_028A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_28A-41C-42A_n78A-n257H","DC_41A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_041C_042A_n078A_n257H ","DC_041A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_28A-41C-42A_n257H","DC_28A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_041C_042A_n257H ","DC_028A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_28A-41C-42A_n257I","DC_42A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_041C_042A_n257I ","DC_042A_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (5 bands)","38.101-3:Table 5.5B.6.4-1","DC_28A-41C-42C_n78A-n257H","DC_42C_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_041C_042C_n078A_n257H ","DC_042C_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_28A-41C-42C_n257A","DC_28A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_041C_042C_n257A ","DC_028A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_28A-41C_n78A-n257G","DC_41A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_041C_n078A_n257G ","DC_041A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_28A-41C_n257G","DC_41C_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_041C_n257G ","DC_041C_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_28A-42A_n78A-n257A","DC_28A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_042A_n078A_n257A ","DC_028A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_28A-42A_n257L","DC_28A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_028A_042A_n257L ","DC_028A_n257A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_28A-42A_n257L","DC_28A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_028A_042A_n257L ","DC_028A_n257G ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_28A-42C_n257G","DC_42C_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_042C_n257G ","DC_042C_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_28A-42C_n257K","DC_42A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_028A_042C_n257K ","DC_042A_n257H ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_28A-42C_n257M","DC_42A_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_028A_042C_n257M ","DC_042A_n257I ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_28A_n7A-n258J","DC_28A_n258A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_028A_n007A_n258J ","DC_028A_n258A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_28A_n7B-n258H","DC_28A_n258G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_028A_n007B_n258H ","DC_028A_n258G ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_28A_n7B-n258M","DC_28A_n258H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_028A_n007B_n258M ","DC_028A_n258H ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_28A_n77(2A)-n257A","DC_28A_n77A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_n077z2Az_n257A ","DC_028A_n077A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_28A_n78A-n257H","DC_28A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_n078A_n257H ","DC_028A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_28A_n257M","DC_28A_n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_028A_n257M ","DC_028A_n257K ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_29A-30A-66A_n77A","DC_30A_n77A PC2","Ongoing","PC2",null,null,"AT&T",null,"RAN5#94-e","ENDC_PC2_R17_xLTE_yNR-UEConTest","DC_029A_030A_066A_n077A ","DC_030A_n077A PC002 ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_29A-30A-66A_n260J","DC_30A_n260H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_029A_030A_066A_n260J ","DC_030A_n260H ","Fallback to DC_2A-29A-30A-66A_n260J with UL DC_30A_n260H","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (4 bands)","38.101-3:Table 5.5B.5.3-1","DC_29A-30A-66A_n260L","DC_30A_n260K","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_029A_030A_066A_n260L ","DC_030A_n260K ","Fallback to DC_2A-29A-30A-66A_n260L with UL DC_30A_n260K","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_29A-30A_n260J","DC_30A_n260H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_029A_030A_n260J ","DC_030A_n260H ","Fallback to DC_2A-2A-29A-30A_n260J with UL DC_30A_n260H","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_29A-66A_n260M","DC_66A_n260J","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_029A_066A_n260M ","DC_066A_n260J ","Fallback to DC_2A-29A-30A-66A_n260M with UL DC_66A_n260J","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_30A-66A-66A_n260J","DC_66A_n260H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_030A_066A_066A_n260J ","DC_066A_n260H ","Fallback to DC_2A-30A-66A-66A_n260J with UL DC_66A_n260H","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_30A-66A-66A_n260L","DC_66A_n260I","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_030A_066A_066A_n260L ","DC_066A_n260I ","Fallback to DC_2A-30A-66A-66A_n260L with UL DC_66A_n260I","v1.2.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_30A-66A_n66A","DC_66A_n66A","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_030A_066A_n066A ","DC_066A_n066A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_30A-66A_n260K","DC_30A_n260J","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_030A_066A_n260K ","DC_030A_n260J ","Fallback to DC_2A-2A-30A-66A_n260K with UL DC_30A_n260J","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_30A_n260K","DC_30A_n260H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_030A_n260K ","DC_030A_n260H ","Fallback to DC_2A-2A-29A-30A_n260K with UL DC_30A_n260H","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_38A_n257G","DC_38A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_038A_n257G ","DC_038A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_38A_n257L","DC_38A_n257L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_038A_n257L ","DC_038A_n257L ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_39A_n79A","DC_39A_n79A","Completed","PC3","<=RAN5#93-e","R5-216625","CMCC","CMCC (Danni Song)","<RAN5#94-e","TEI15_Test 5GS_NR_LTE-UEConTest","DC_039A_n079A ","DC_039A_n079A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_39A_n258G","DC_39A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_039A_n258G ","DC_039A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_39A_n258L","DC_39A_n258L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_039A_n258L ","DC_039A_n258L ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_40A-40A-42A-42A_n257J","DC_40A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_040A_042A_042A_n257J ","DC_040A_n257A ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_40A-40A-42C_n257H","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_040A_042C_n257H ","DC_042A_n257A ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_40A-42A-42A_n257J","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_042A_042A_n257J ","DC_042A_n257A ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_40A-42A_n77A-n257H","DC_42A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_042A_n077A_n257H ","DC_042A_n257A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_40A-42A_n77A-n257K","DC_40A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_042A_n077A_n257K ","DC_040A_n257G ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_40A-42A_n77A-n257L","DC_42A_n257L","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_042A_n077A_n257L ","DC_042A_n257L ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_40A-42A_n77C-n257F","DC_42A_n257E","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_042A_n077C_n257F ","DC_042A_n257E ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_40A-42A_n77C-n257M","DC_40A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_042A_n077C_n257M ","DC_040A_n257H ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_40A-42A_n78A-n257E","DC_40A_n257D","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_042A_n078A_n257E ","DC_040A_n257D ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_40A-42A_n78A-n257J","DC_42A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_042A_n078A_n257J ","DC_042A_n257A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_40A-42A_n78A-n257L","DC_40A_n257L","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_042A_n078A_n257L ","DC_040A_n257L ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_40A-42A_n257K","DC_40A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_042A_n257K ","DC_040A_n257A ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_40A_n77A-n257J","DC_40A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_n077A_n257J ","DC_040A_n257I ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_40A_n77C-n257D","DC_40A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_n077C_n257D ","DC_040A_n257A ","This FR1+FR2 config is not testable","v1.2.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_40A_n77C-n257M","DC_40A_n257K","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_n077C_n257M ","DC_040A_n257K ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_40A_n78A-n257J","DC_40A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_n078A_n257J ","DC_040A_n257H ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_40A_n257M","DC_40A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_n257M ","DC_040A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_40A_n258K","DC_40A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040A_n258K ","DC_040A_n258G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_40C-42A-42A_n257E","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040C_042A_042A_n257E ","DC_042A_n257A ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_40C_n257J","DC_40A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_040C_n257J ","DC_040A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_41A-42A_n78A-n257H","DC_42A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041A_042A_n078A_n257H ","DC_042A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_41A-42A_n257H","DC_41A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041A_042A_n257H ","DC_041A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_41A-42A_n257M","DC_42A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041A_042A_n257M ","DC_042A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_41A-42C_n77A-n257I","DC_41A_n77A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041A_042C_n077A_n257I ","DC_041A_n077A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_41A-42C_n78A-n257I","DC_42A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041A_042C_n078A_n257I ","DC_042A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_41A-42C_n257K","DC_42A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041A_042C_n257K ","DC_042A_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_41A-42C_n257M","DC_42A_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041A_042C_n257M ","DC_042A_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_41A_n28A-n257G","DC_41A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041A_n028A_n257G ","DC_041A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_41A_n77A-n257H","DC_41A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041A_n077A_n257H ","DC_041A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_41A_n257G","DC_41A_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041A_n257G ","DC_041A_n257G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_41A_n258L","DC_41A_n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_041A_n258L ","DC_041A_n258G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_41C-42A_n77A-n257G","DC_41C_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_042A_n077A_n257G ","DC_041C_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_41C-42A_n78A-n257G","DC_42A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_042A_n078A_n257G ","DC_042A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_41C-42A_n78A-n257I","DC_42A_n257I","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_042A_n078A_n257I ","DC_042A_n257I ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_41C-42A_n257L","DC_41A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_042A_n257L ","DC_041A_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_41C-42C_n77A-n257H","DC_41A_n77A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_042C_n077A_n257H ","DC_041A_n077A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_41C-42C_n77A-n257I","DC_42A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_042C_n077A_n257I ","DC_042A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (4 bands)","38.101-3:Table 5.5B.6.3-1","DC_41C-42C_n78A-n257I","DC_41A_n257H","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_042C_n078A_n257I ","DC_041A_n257H ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_41C-42C_n257I","DC_42C_n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_042C_n257I ","DC_042C_n257G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_41C-42C_n257K","DC_41C_n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_042C_n257K ","DC_041C_n257H ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_41C-42C_n257M","DC_42C_n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_042C_n257M ","DC_042C_n257I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_41C_n3A-n257G","DC_41C_n3A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_n003A_n257G ","DC_041C_n003A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_41C_n77A-n257A","DC_41A_n257A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_n077A_n257A ","DC_041A_n257A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_41C_n78A-n257H","DC_41A_n78A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_n078A_n257H ","DC_041A_n078A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_41C_n257D","DC_41A_n257D","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_n257D ","DC_041A_n257D ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_41C_n257K","DC_41C_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_041C_n257K ","DC_041C_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_42A-42A_n257D","DC_42A_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_042A_042A_n257D ","DC_042A_n257A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_42A_n77A-n257E","DC_42A_n257E","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_042A_n077A_n257E ","DC_042A_n257E ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_42A_n77C-n257E","DC_42A_n257D","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_042A_n077C_n257E ","DC_042A_n257D ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_42A_n77C-n257L","DC_42A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_042A_n077C_n257L ","DC_042A_n257G ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-17","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_42A_n78A-n257L","DC_42A_n257L","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_042A_n078A_n257L ","DC_042A_n257L ","This FR1+FR2 config is not testable","v1.4.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_42A_n79A-n257I","DC_42A_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_042A_n079A_n257I ","DC_042A_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (4 bands)","38.101-3:Table 5.5B.4.3-1","DC_42C_n3A-n28A-n77A","DC_42A_n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_042C_n003A_n028A_n077A ","DC_042A_n028A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_42C_n78A-n257H","DC_42C_n257G","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_042C_n078A_n257H ","DC_042C_n257G ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-15","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_42C_n257D","DC_42A_n257A","Ongoing (FB)","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_042C_n257D ","DC_042A_n257A ","Fallback to DC_3A-19A-42C_n257D with UL DC_42A_n257D","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_42C_n257I","DC_42A_n257A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_042C_n257I ","DC_042A_n257A ","Fallback to DC_1A-3A-19A-42C_n257I with UL DC_42A_n257A","v1.0.0"]
[null,"Rel-15","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_42D_n257A","DC_42A_n257A","Ongoing (FB)","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_042D_n257A ","DC_042A_n257A ","Fallback to DC_1A-3A-42D_n257G with UL DC_42A_n257A","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_42D_n257L","DC_42A_n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_042D_n257L ","DC_042A_n257K ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_42E_n257E","DC_42E_n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_042E_n257E ","DC_042E_n257A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_42E_n257H","DC_42A_n257G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_042E_n257H ","DC_042A_n257G ","Fallback to DC_1A-42E_n257H with UL DC_42A_n257G","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46A-46A-46A-66A_n261K","DC_66A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046A_046A_046A_066A_n261K ","DC_066A_n261A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46A-46A-46A-66A_n261(A-I)","DC_66A_n261I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046A_046A_046A_066A_n261zA_Iz ","DC_066A_n261I ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46A-46A-66A_n261I","DC_66A_n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046A_046A_066A_n261I ","DC_066A_n261H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46A-46A-66A_n261M","DC_66A_n261K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046A_046A_066A_n261M ","DC_066A_n261K ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_46A-48A_n66A","DC_48A_n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046A_048A_n066A ","DC_048A_n066A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46A-66A-66A_n260M","DC_66A_n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046A_066A_066A_n260M ","DC_066A_n260K ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46A-66A_n260K","DC_66A_n260J","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_046A_066A_n260K ","DC_066A_n260J ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46A-66A_n261I","DC_66A_n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046A_066A_n261I ","DC_066A_n261G ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46A-66A_n261M","DC_66A_n261J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046A_066A_n261M ","DC_066A_n261J ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_46A_n77A","N/A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046A_n077A ","N/A ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46C-66A-66A_n260L","DC_66A_n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046C_066A_066A_n260L ","DC_066A_n260L ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46C-66A_n260J","DC_66A_n260J","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_046C_066A_n260J ","DC_066A_n260J ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_46C_n78A","N/A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_046C_n078A ","_ ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46D-48D_n260(2A)","DC_48C_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_046D_048D_n260z2Az ","DC_048C_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46D-66A-66A_n260M","DC_66A_n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046D_066A_066A_n260M ","DC_066A_n260I ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_46E-48A_n66A","DC_48A_n66A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046E_048A_n066A ","DC_048A_n066A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46E-66A-66A_n260L","DC_66A_n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_046E_066A_066A_n260L ","DC_066A_n260I ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (3 bands)","38.101-3:Table 5.5B.5.2-1","DC_46E-66A_n260M","DC_66A_n260A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_046E_066A_n260M ","DC_066A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_48A_n260J","DC_48A_n260I","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_048A_n260J ","DC_048A_n260I ","Fallback to DC_48A_n260M with UL DC_48A_n260I","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_48A_n260K","DC_48A_n260A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_048A_n260K ","DC_048A_n260A ","Fallback to DC_48A_n260M with UL DC_48A_n260A","v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_48A_n261(A-G-I)","DC_48A_n261A","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_048A_n261zA_G_Iz ","DC_048A_n261A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_48A_n261(G-H)","DC_48A_n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_048A_n261zG_Hz ","DC_048A_n261A ","Fallback to DC_48A_n261(A-G-I) with UL DC_48A_n261A","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_48C-66A_n77A","DC_66A_n77A PC2","Ongoing","PC2",null,null,"Verizon",null,"RAN5#94-e","ENDC_PC2_R17_xLTE_yNR-UEConTest","DC_048C_066A_n077A ","DC_066A_n077A PC002 ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_48D_n260(3A)","DC_48A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_048D_n260z3Az ","DC_048A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_66A-66A_n2A-n77A","DC_66A_n2A","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_066A_n002A_n077A ","DC_066A_n002A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_66A-66A_n77(2A)","DC_66A_n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_066A_n077z2Az ","DC_066A_n077A ",null,"v1.2.0"]
[null,"Rel-15","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A-66A_n260L","DC_66A_n260A","Ongoing","PC3",null,null,"Verizon,AT&T","Verizon,AT&T (Jinwen Ma,Ron Borsato)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_066A_066A_n260L ","DC_066A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A-66A_n261A","DC_66A_n261A","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_066A_n261A ","DC_066A_n261A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A-66A_n261(A-G)","DC_66A_n261G","Ongoing","PC3",null,null,"Verizon",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_066A_n261zA_Gz ","DC_066A_n261G ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A-66A_n261(G-I)","DC_66A_n261H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_066A_n261zG_Iz ","DC_066A_n261H ","Fallback to DC_5A-66A-66A_n261(H-I) with UL DC_66A_n261H","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_66A_n2A-n78A","DC_66A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n002A_n078A ","DC_066A_n078A ",null,"v1.1.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_66A_n5A-n260K","DC_66A_n5A-n260A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_n005A_n260K ","DC_066A_n005A_n260A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1+FR2 (3 bands)","38.101-3:Table 5.5B.6.2-1","DC_66A_n5A-n261(A-G-I)","DC_66A_n5A-n261A","N/A","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_n005A_n261zA_G_Iz ","DC_066A_n005A_n261A ","This FR1+FR2 config is not testable","v1.0.0"]
[null,"Rel-16","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_66A_n46A","DC_66A_n46A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_n046A ","DC_066A_n046A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_66A_n77A","DC_66A_n77A PC2","Completed","PC2","RAN5#96-e","R5-224494, R5-225126","Verizon,AT&T,Rogers","Verizon ,Qualcomm,Ericsson (Jinwen Ma,Kevin Wang,Leif Mattisson)","<RAN5#94-e,RAN5#94-e","ENDC_UE_PC2_R17_NR_TDD-UEConTest","DC_066A_n077A ","DC_066A_n077A PC002 ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260D","DC_66A_n260A","Ongoing","PC3",null,null,"Verizon","Verizon (Jinwen Ma)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_066A_n260D ","DC_066A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260L","DC_66A_n260H","Ongoing","PC3",null,null,"AT&T",null,"RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_n260L ","DC_066A_n260H ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(2A-3O-P)","DC_66A_n260P","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n260z2A_3O_Pz ","DC_066A_n260P ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(2A-O-2Q)","DC_66A_n260O","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n260z2A_O_2Qz ","DC_066A_n260O ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(2A-P)","DC_66A_n260P","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_n260z2A_Pz ","DC_066A_n260P ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(2O-Q)","DC_66A_n260P","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n260z2O_Qz ","DC_066A_n260P ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(3A-O-P)","DC_66A_n260P","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_n260z3A_O_Pz ","DC_066A_n260P ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(3O-P)","DC_66A_n260P","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n260z3O_Pz ","DC_066A_n260P ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(4A-P-Q)","DC_66A_n260O","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n260z4A_P_Qz ","DC_066A_n260O ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(5A-3O)","DC_66A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n260z5A_3Oz ","DC_066A_n260A ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(8A-2O)","DC_66A_n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_n260z8A_2Oz ","DC_066A_n260A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(A-4G)","DC_66A_n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n260zA_4Gz ","DC_066A_n260G ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(A-G-H)","DC_66A_n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n260zA_G_Hz ","DC_066A_n260H ",null,"v1.4.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(A-P-Q)","DC_66A_n260O","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_n260zA_P_Qz ","DC_066A_n260O ",null,"v1.4.0"]
[null,"Rel-15","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(D-P)","DC_66A_n260A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_066A_n260zD_Pz ","DC_066A_n260A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n260(P-Q)","DC_66A_n260O","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_n260zP_Qz ","DC_066A_n260O ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n261L","DC_66A_n261J","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n261L ","DC_066A_n261J ","Fallback to DC_2A-13A-66A_n261M with UL DC_66A_n261J","v1.2.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n261(2A-D)","DC_66A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n261z2A_Dz ","DC_066A_n261A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n261(3A-G-O)","DC_66A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n261z3A_G_Oz ","DC_066A_n261A ",null,"v1.2.0"]
[null,"Rel-17","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n261(6A-2O)","DC_66A_n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066A_n261z6A_2Oz ","DC_066A_n261A ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n261(A-I)","DC_66A_n261H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_n261zA_Iz ","DC_066A_n261H ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_66A_n261H","v1.0.0"]
[null,"Rel-16","EN-DC FR2 (2 bands)","38.101-3:Table 5.5B.5.1-1","DC_66A_n261(G-I)","DC_66A_n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_066A_n261zG_Iz ","DC_066A_n261A ","Fallback to DC_2A-13A-66A_n261(A-G-I) with UL DC_66A_n261A","v1.0.0"]
[null,"Rel-17","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_66C_n2A","DC_66A_n2A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_066C_n002A ","DC_066A_n002A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1 (3 bands) ","38.101-1:Table 5.5B.1-2","DC_n1A-n3A-n28A","DC_n3A-n28A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n001A_n003A_n028A ","DC_n003A_n028A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1 (3 bands) ","38.101-1:Table 5.5B.1-2","DC_n1A-n3A-n78A","DC_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n001A_n003A_n078A ","DC_n003A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1 (4 bands) ","38.101-1:Table 5.5B.1-3","DC_n1A-n28A-n77A-n79A","DC_n1A-n79A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n001A_n028A_n077A_n079A ","DC_n001A_n079A ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n1A-n41A-n257G","DC_n1A-n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n001A_n041A_n257G ","DC_n001A_n041A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n1A-n77A-n79A-n257A","DC_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n001A_n077A_n079A_n257A ","DC_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n1A-n77(2A)-n257I","DC_n1A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n001A_n077z2Az_n257I ","DC_n001A_n077A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n1A-n78A-n257A","DC_n1A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n001A_n078A_n257A ","DC_n001A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n1A-n78A-n257J","DC_n1A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n001A_n078A_n257J ","DC_n001A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n1A-n78A-n257M","DC_n1A-n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n001A_n078A_n257M ","DC_n001A_n257K ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n1A-n79A-n257I","DC_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n001A_n079A_n257I ","DC_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n5A-n260H","DC_n5A-n260G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n005A_n260H ","DC_n005A_n260G ","Fallback to DC_n2A-n5A-n260I with UL DC_n5A-n260G","v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n5A-n260L","DC_n2A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n005A_n260L ","DC_n002A_n260K ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n5A-n260M","DC_n5A-n260M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n005A_n260M ","DC_n005A_n260M ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n5A-n261K","DC_n2A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n005A_n261K ","DC_n002A_n261H ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n5A-n261(A-G-H)","DC_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n005A_n261zA_G_Hz ","DC_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n12A-n260K","DC_n2A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n012A_n260K ","DC_n002A_n260G ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n12A-n260M","DC_n12A-n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n012A_n260M ","DC_n012A_n260L ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n14A-n260I","DC_n14A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n014A_n260I ","DC_n014A_n260I ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n14A-n260L","DC_n2A-n14A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n014A_n260L ","DC_n002A_n014A ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n30A-n260H","DC_n2A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n030A_n260H ","DC_n002A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n30A-n260M","DC_n30A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n030A_n260M ","DC_n030A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n66A-n260J","DC_n2A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n066A_n260J ","DC_n002A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n66A-n260L","DC_n2A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n066A_n260L ","DC_n002A_n260K ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n66A-n261(A-G-I)","DC_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n066A_n261zA_G_Iz ","DC_n002A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n77A-n260I","DC_n77A-n260G","Ongoing","PC3",null,null,"AT&T,Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n077A_n260I ","DC_n077A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n77A-n260K","DC_n77A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n077A_n260K ","DC_n077A_n260J ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n77A-n260M","DC_n2A-n260M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n077A_n260M ","DC_n002A_n260M ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n2A-n77A-n261K","DC_n77A-n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n077A_n261K ","DC_n077A_n261A ","Fallback to DC_n2A-n77A-n261M with UL DC_n77A-n261A","v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n2A-n261I","DC_n2A-n261G","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n261I ","DC_n002A_n261G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n2A-n261(A-2G)","DC_n2A-n261G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n261zA_2Gz ","DC_n002A_n261G ","Fallback to DC_n2A-n261(A-G-I) with UL DC_n2A-n261G","v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n2A-n261(A-L)","DC_n2A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002A_n261zA_Lz ","DC_n002A_n261A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n2(2A)-n260I","DC_n2A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n002z2Az_n260I ","DC_n002A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n3A-n7A-n78A-n258B","DC_n3A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n007A_n078A_n258B ","DC_n003A_n258A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n3A-n7A-n78A-n258J","DC_n3A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n007A_n078A_n258J ","DC_n003A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n3A-n7A-n78A-n258K","DC_n7A-n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n007A_n078A_n258K ","DC_n007A_n258I ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n3A-n7A-n258D","DC_n3A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n007A_n258D ","DC_n003A_n258A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n3A-n7A-n258J","DC_n3A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n007A_n258J ","DC_n003A_n258G ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n3A-n7B-n78A-n258B","DC_n7A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n007B_n078A_n258B ","DC_n007A_n258A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n3A-n7B-n78A-n258J","DC_n3A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n007B_n078A_n258J ","DC_n003A_n258G ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n3A-n7B-n78A-n258K","DC_n78A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n007B_n078A_n258K ","DC_n078A_n258H ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n3A-n7B-n258E","DC_n7A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n007B_n258E ","DC_n007A_n258A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n3A-n7B-n258J","DC_n7A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n007B_n258J ","DC_n007A_n258A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n3A-n18A-n257H","DC_n18A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n018A_n257H ","DC_n018A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n3A-n28A-n77A-n257I","DC_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n028A_n077A_n257I ","DC_n028A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n3A-n28A-n77(2A)-n257G","DC_n3A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n028A_n077z2Az_n257G ","DC_n003A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n3A-n28A-n78A-n257G","DC_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n028A_n078A_n257G ","DC_n028A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n3A-n28A-n79A-n257I","DC_n28A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n028A_n079A_n257I ","DC_n028A_n257I ",null,"v1.1.0"]
[null,"Rel-16","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n3A-n28A-n257I","DC_n28A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_n003A_n028A_n257I ","DC_n028A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n3A-n77A-n79A-n257G","DC_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n077A_n079A_n257G ","DC_n077A_n257A ",null,"v1.1.0"]
[null,"Rel-16","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n3A-n77A-n257A","DC_n3A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_n003A_n077A_n257A ","DC_n003A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n3A-n77(2A)-n79A-n257H","DC_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n077z2Az_n079A_n257H ","DC_n077A_n257G ",null,"v1.1.0"]
[null,"Rel-16","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n3A-n78A-n257I","DC_n78A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_n003A_n078A_n257I ","DC_n078A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n3A-n78A-n258H","DC_n3A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n078A_n258H ","DC_n003A_n258A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n3A-n78A-n258L","DC_n78A-n258I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n078A_n258L ","DC_n078A_n258I ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n3A-n79A-n257H","DC_n79A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003A_n079A_n257H ","DC_n079A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n3(2A)-n257G","DC_n3A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n003z2Az_n257G ","DC_n003A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n5A-n30A-n260L","DC_n5A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n005A_n030A_n260L ","DC_n005A_n260K ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n5A-n30A-n260M","DC_n30A-n260M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n005A_n030A_n260M ","DC_n030A_n260M ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n5A-n66A-n260K","DC_n5A-n66A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n005A_n066A_n260K ","DC_n005A_n066A ","Fallback to DC_n5A-n66A-n260M with UL DC_n5A-n66A","v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n5A-n66A-n260L","DC_n66A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n005A_n066A_n260L ","DC_n066A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n5A-n66A-n261(2G)","DC_n5A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n005A_n066A_n261z2Gz ","DC_n005A_n261G ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n5A-n66A-n261(H-I)","DC_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n005A_n066A_n261zH_Iz ","DC_n005A_n261A ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n5A-n77A-n260I","DC_n5A-n260I","Ongoing","PC3",null,null,"AT&T,Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n005A_n077A_n260I ","DC_n005A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n5A-n77A-n260L","DC_n77A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n005A_n077A_n260L ","DC_n077A_n260J ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n5A-n77A-n261M","DC_n5A-n261G","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n005A_n077A_n261M ","DC_n005A_n261G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n5A-n260K","DC_n5A-n260G","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n005A_n260K ","DC_n005A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n5A-n261L","DC_n5A-n261I","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n005A_n261L ","DC_n005A_n261I ","Fallback to DC_n5A-n77A-n261M with UL DC_n5A-n261I","v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n5A-n261(4A)","DC_n5A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n005A_n261z4Az ","DC_n005A_n261A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1 (2 bands) ","38.101-1:Table 5.5B.1-1","DC_n7A-n46C","DC_n7A-n46A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n007A_n046C ","DC_n007A_n046A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n7A-n78A-n258J","DC_n78A-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n007A_n078A_n258J ","DC_n078A_n258H ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n7A-n78A-n258M","DC_n78A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n007A_n078A_n258M ","DC_n078A_n258A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n7B-n78A-n258C","DC_n7A-n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n007B_n078A_n258C ","DC_n007A_n078A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n7B-n78A-n258I","DC_n7A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n007B_n078A_n258I ","DC_n007A_n258A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n7B-n258H","DC_n7B-n258H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n007B_n258H ","DC_n007B_n258H ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR1 (2 bands)","38.101-3:Table 5.5B.4a.1-1","DC_n8A_1A","DC_n8A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n008A_001A ","DC_n008A_001A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n8A-n257K","DC_n8A-n257K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n008A_n257K ","DC_n008A_n257K ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n12A-n30A-n260I","DC_n12A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n012A_n030A_n260I ","DC_n012A_n030A ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n12A-n30A-n260K","DC_n12A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n012A_n030A_n260K ","DC_n012A_n260J ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n12A-n66A-n260J","DC_n12A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n012A_n066A_n260J ","DC_n012A_n260A ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n12A-n66A-n260M","DC_n12A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n012A_n066A_n260M ","DC_n012A_n260H ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n12A-n77A-n260H","DC_n12A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n012A_n077A_n260H ","DC_n012A_n260G ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n12A-n77A-n260K","DC_n12A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n012A_n077A_n260K ","DC_n012A_n077A ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n12A-n77A-n260M","DC_n77A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n012A_n077A_n260M ","DC_n077A_n260J ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n14A-n30A-n260J","DC_n14A-n30A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n014A_n030A_n260J ","DC_n014A_n030A ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n14A-n30A-n260M","DC_n14A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n014A_n030A_n260M ","DC_n014A_n260G ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n14A-n66A-n260H","DC_n14A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n014A_n066A_n260H ","DC_n014A_n260G ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n14A-n66A-n260M","DC_n66A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n014A_n066A_n260M ","DC_n066A_n260I ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n14A-n77A-n260K","DC_n14A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n014A_n077A_n260K ","DC_n014A_n260A ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n14A-n77A-n260L","DC_n77A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n014A_n077A_n260L ","DC_n077A_n260K ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n14A-n260I","DC_n14A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n014A_n260I ","DC_n014A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n18A-n28A-n257H","DC_n18A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n018A_n028A_n257H ","DC_n018A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n18A-n77(2A)-n257G","DC_n18A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n018A_n077z2Az_n257G ","DC_n018A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n18A-n78A-n257I","DC_n78A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n018A_n078A_n257I ","DC_n078A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n25A-n258G","DC_n25A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n025A_n258G ","DC_n025A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n25A-n260M","DC_n25A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n025A_n260M ","DC_n025A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n28A-n41A-n257I","DC_n28A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n028A_n041A_n257I ","DC_n028A_n257G ",null,"v1.0.0"]
[null,"Rel-16","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n28A-n77A-n257A","DC_n28A-n77A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_n028A_n077A_n257A ","DC_n028A_n077A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n28A-n77(2A)-n79A-n257G","DC_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n028A_n077z2Az_n079A_n257G ","DC_n079A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (4 bands) ","38.101-3:Table 5.5B.7-3","DC_n28A-n77(2A)-n79A-n257I","DC_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n028A_n077z2Az_n079A_n257I ","DC_n079A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n28A-n77(2A)-n257I","DC_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n028A_n077z2Az_n257I ","DC_n077A_n257G ",null,"v1.0.0"]
[null,"Rel-16","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n28A-n78A-n257G","DC_n78A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_n028A_n078A_n257G ","DC_n078A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n30A-n66A-n260H","DC_n30A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n030A_n066A_n260H ","DC_n030A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n30A-n66A-n260K","DC_n66A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n030A_n066A_n260K ","DC_n066A_n260K ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n30A-n66A-n260M","DC_n66A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n030A_n066A_n260M ","DC_n066A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n30A-n77A-n260L","DC_n77A-n260K","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n030A_n077A_n260L ","DC_n077A_n260K ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n30A-n77A-n260L","DC_n77A-n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n030A_n077A_n260L ","DC_n077A_n260L ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n40A-n77A-n257E","DC_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n040A_n077A_n257E ","DC_n077A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n40A-n77A-n257I","DC_n40A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n040A_n077A_n257I ","DC_n040A_n257H ",null,"v1.4.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n40A-n77A-n257L","DC_n77A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n040A_n077A_n257L ","DC_n077A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n40A-n78A-n257G","DC_n40A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n040A_n078A_n257G ","DC_n040A_n257G ",null,"v1.4.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n40A-n78A-n257K","DC_n78A-n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n040A_n078A_n257K ","DC_n078A_n257J ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n40A-n78A-n257M","DC_n40A-n257M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n040A_n078A_n257M ","DC_n040A_n257M ",null,"v1.4.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n40A-n78C-n257F","DC_n40A-n257E","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n040A_n078C_n257F ","DC_n040A_n257E ",null,"v1.4.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n40A-n78C-n257K","DC_n40A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n040A_n078C_n257K ","DC_n040A_n257I ",null,"v1.4.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n40A-n257L","DC_n40A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n040A_n257L ","DC_n040A_n257A ",null,"v1.4.0"]
[null,"Rel-17","NE-DC FR1 (2 bands)","38.101-3:Table 5.5B.4a.1-1","DC_n41A_8A","DC_n41A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n041A_008A ","DC_n041A_008A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n41A-n77A-n257H","DC_n41A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n041A_n077A_n257H ","DC_n041A_n257H ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n41A-n77(2A)-n257H","DC_n77A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n041A_n077z2Az_n257H ","DC_n077A_n257A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n41A-n257H","DC_n41A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n041A_n257H ","DC_n041A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n41C-n258(G-H)","DC_n41A-n258G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n041C_n258zG_Hz ","DC_n041A_n258G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n41(2A)-n257I","DC_n41A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n041z2Az_n257I ","DC_n041A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1 (2 bands) ","38.101-1:Table 5.5B.1-1","DC_n46A-n48A","DC_n46A-n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n046A_n048A ","DC_n046A_n048A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1 (2 bands) ","38.101-1:Table 5.5B.1-1","DC_n46N-n48B","DC_n46A-n48B","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n046N_n048B ","DC_n046A_n048B ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n48A-n261(2A-G)","DC_n48A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n048A_n261z2A_Gz ","DC_n048A_n261A ",null,"v1.4.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n48A-n261(G-H)","DC_n48A-n261H","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n048A_n261zG_Hz ","DC_n048A_n261H ","Fallback to DC_n48A-n261(H-I) with UL DC_n48A-n261H","v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n48B-n260G","DC_n48A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n048B_n260G ","DC_n048A_n260A ",null,"v1.1.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n48B-n261K","DC_n48A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n048B_n261K ","DC_n048A_n261H ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1 (2 bands) ","38.101-1:Table 5.5B.1-1","DC_n48C-n96E","DC_n48A-n96A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n048C_n096E ","DC_n048A_n096A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n48C-n260M","DC_n48A-n260G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n048C_n260M ","DC_n048A_n260G ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n48(2A)-n261I","DC_n48A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n048z2Az_n261I ","DC_n048A_n261G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n48(2A)-n261(2A-I)","DC_n48A-n261G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n048z2Az_n261z2A_Iz ","DC_n048A_n261G ",null,"v1.4.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n48(3A)-n260G","DC_n48A-n260A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n048z3Az_n260G ","DC_n048A_n260A ",null,"v1.4.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n48(A-B)-n260J","DC_n48A-n260I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n048zA_Bz_n260J ","DC_n048A_n260I ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n48(A-B)-n261J","DC_n48A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n048zA_Bz_n261J ","DC_n048A_n261H ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n66A-n77A-n260J","DC_n66A-n260A","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n066A_n077A_n260J ","DC_n066A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n66A-n77A-n260L","DC_n66A-n260G","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n066A_n077A_n260L ","DC_n066A_n260G ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n66A-n77A-n261K","DC_n77A-n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n066A_n077A_n261K ","DC_n077A_n261A ","Fallback to DC_n66A-n77A-n261M with UL DC_n77A-n261A","v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n66A-n260G","DC_n66A-n260A","Ongoing","PC3",null,null,"Verizon,AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n066A_n260G ","DC_n066A_n260A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n66A-n260L","DC_n66A-n260K","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n066A_n260L ","DC_n066A_n260K ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n66A-n261M","DC_n66A_n261H","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n066A_n261M ","DC_n066A_n261H ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n66A-n261(4A)","DC_n66A-n261A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n066A_n261z4Az ","DC_n066A_n261A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n66(2A)-n260K","DC_n66A-n260J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n066z2Az_n260K ","DC_n066A_n260J ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n77A-n79A-n257G","DC_n79A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n077A_n079A_n257G ","DC_n079A_n257G ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n77A-n257A_3A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n077A_n257A_003A ","DC_n257A_003A ",null,"v1.2.0"]
[null,"Rel-16","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n77A-n257J","DC_n77A-n257J","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_n077A_n257J ","DC_n077A_n257J ",null,"v1.0.0"]
[null,"Rel-16","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n77A-n257L","DC_n77A-n257H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_n077A_n257L ","DC_n077A_n257H ",null,"v1.0.0"]
[null,"Rel-16","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n77A-n261A","DC_n77A-n261A","Ongoing","PC3",null,null,"Verizon",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_n077A_n261A ","DC_n077A_n261A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n77A-n261(2A-I)","DC_n77A-n261A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n077A_n261z2A_Iz ","DC_n077A_n261A ","Fallback to DC_n77A-n261(A-G-I) with UL DC_n77A-n261A","v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n77A-n261(A-I)","DC_n77A-n261G","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n077A_n261zA_Iz ","DC_n077A_n261G ","Fallback to DC_n77A-n261(A-G-I) with UL DC_n77A-n261G","v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n77C-n260M","DC_n77A-n260M","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n077C_n260M ","DC_n077A_n260M ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n77C-n261(2A-H)","DC_n77A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n077C_n261z2A_Hz ","DC_n077A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n77C-n261(A-H)","DC_n77A-n261H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n077C_n261zA_Hz ","DC_n077A_n261H ",null,"v1.4.0"]
[null,"Rel-17","NR-DC FR1+FR2 (3 bands) ","38.101-3:Table 5.5B.7-2","DC_n77(2A)-n79A-n257H","DC_n79A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n077z2Az_n079A_n257H ","DC_n079A_n257A ",null,"v1.0.0"]
[null,"Rel-16","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n77(2A)-n257G","DC_n77A-n257G","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_n077z2Az_n257G ","DC_n077A_n257G ",null,"v1.0.0"]
[null,"Rel-16","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n77(2A)-n257L","DC_n77A-n257L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_n077z2Az_n257L ","DC_n077A_n257L ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n77(2A)-n260J","DC_n77A-n260H","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n077z2Az_n260J ","DC_n077A_n260H ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n77(2A)-n260M","DC_n77A-n260L","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n077z2Az_n260M ","DC_n077A_n260L ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR1 (5 bands)","38.101-3:Table 5.5B.4a.4-1","DC_n78A_1A-3A-5A-7A-7A","DC_n78A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n078A_001A_003A_005A_007A_007A ","DC_n078A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR1 (3 bands)","38.101-3:Table 5.5B.4a.2-1","DC_n78A_3A-7A-7A","DC_n78A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n078A_003A_007A_007A ","DC_n078A_003A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n78A-n257(2A)","DC_n78A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n078A_n257z2Az ","DC_n078A_n257A ",null,"v1.2.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n78C-n257H","DC_n78A-n257A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n078C_n257H ","DC_n078A_n257A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n78C-n258C","DC_n78A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n078C_n258C ","DC_n078A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n78C-n258M","DC_n78A-n258A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n078C_n258M ","DC_n078A_n258A ",null,"v1.0.0"]
[null,"Rel-17","NR-DC FR1+FR2 (2 bands) ","38.101-3:Table 5.5B.7-1","DC_n79A-n257L","DC_n79A-n257I","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n079A_n257L ","DC_n079A_n257I ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257A_3A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257A_003A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257G_1A-3A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257G_001A_003A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257G_1A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257G_001A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257H_1A-3C","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257H_001A_003C ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257H_3C-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257H_003C_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257I_1A-3A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_003A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_1A-3C","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_003C ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_1A-3C","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_003C ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_1A-3C","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_003C ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_1A-3C-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_003C_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_1A-3C-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_003C_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_1A-3C-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_003C_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_1A-5A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_005A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_1A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_1A-5A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_005A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_1A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_1A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_1A-5A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_005A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_1A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_1A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_1A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_1A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_1A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_1A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_1A-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_1A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_001A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_3A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_3A","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_3A","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_3A","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_3A-5A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_005A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_3A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_3A-5A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_005A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_3A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_3A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_3A-5A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_005A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_3A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257I_3A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_3A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_3A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_3A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_3A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_3A-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_3A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_3C","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003C ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_3C","DC_n257A_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003C ","DC_n257A_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_3C","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003C ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_3C","DC_n257G_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003C ","DC_n257G_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_3C","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003C ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_3C","DC_n257H_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003C ","DC_n257H_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_3C","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003C ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_3C","DC_n257I_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003C ","DC_n257I_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_3C-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003C_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_3C-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_003C_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257I_5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257I_8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257I_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_1A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_1A","DC_n257G_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A ","DC_n257G_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_1A","DC_n257H_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A ","DC_n257H_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_1A","DC_n257I_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A ","DC_n257I_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_1A","DC_n257J_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A ","DC_n257J_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-3A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-3A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-3A","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-3A","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-3A","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-3A","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3A-5A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_005A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3A-5A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_005A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257J_1A-3A-5A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_005A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257J_1A-3A-5A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_005A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257J_1A-3A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257J_1A-3A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257J_1A-3A-5A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_005A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257J_1A-3A-5A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_005A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257J_1A-3A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257J_1A-3A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3A-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3A-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-3C","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003C ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-3C","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003C ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-3C","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003C ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-3C","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003C ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-3C","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003C ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-3C","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003C ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3C-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003C_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3C-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003C_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-3C-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_003C_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-5A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_005A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-5A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_005A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-5A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_005A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_1A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_1A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_001A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3A","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3A","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3A","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3A","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_3A-5A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_005A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_3A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_3A-5A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_005A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_3A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_3A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_3A-5A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_005A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_3A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257J_3A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_3A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_3A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_3A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_3A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_3A-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_3A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3C","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003C ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3C","DC_n257A_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003C ","DC_n257A_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3C","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003C ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3C","DC_n257G_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003C ","DC_n257G_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3C","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003C ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3C","DC_n257H_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003C ","DC_n257H_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3C","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003C ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3C","DC_n257I_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003C ","DC_n257I_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3C","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003C ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_3C","DC_n257J_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003C ","DC_n257J_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_3C-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003C_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_3C-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_003C_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257J_5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257J_8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257J_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_1A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_1A","DC_n257G_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A ","DC_n257G_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_1A","DC_n257H_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A ","DC_n257H_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_1A","DC_n257I_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A ","DC_n257I_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_1A","DC_n257J_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A ","DC_n257J_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_1A","DC_n257K_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A ","DC_n257K_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3A","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3A","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3A","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3A","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3A","DC_n257K_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A ","DC_n257K_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3A-5A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_005A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3A-5A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_005A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257K_1A-3A-5A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_005A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257K_1A-3A-5A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_005A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257K_1A-3A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257K_1A-3A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257K_1A-3A-5A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_005A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257K_1A-3A-5A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_005A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257K_1A-3A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257K_1A-3A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3A-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3A-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3C","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003C ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3C","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003C ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3C","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003C ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3C","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003C ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3C","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003C ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3C","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003C ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-3C","DC_n257K_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003C ","DC_n257K_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3C-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003C_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3C-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003C_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-3C-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_003C_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-5A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_005A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-5A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_005A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-5A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_005A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_1A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_1A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_001A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3A","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3A","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3A","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3A","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3A","DC_n257K_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A ","DC_n257K_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_3A-5A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_005A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_3A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_3A-5A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_005A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_3A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_3A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_3A-5A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_005A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_3A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257K_3A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_3A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_3A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_3A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_3A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_3A-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_3A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3C","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3C","DC_n257A_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C ","DC_n257A_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3C","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3C","DC_n257G_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C ","DC_n257G_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3C","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3C","DC_n257H_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C ","DC_n257H_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3C","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3C","DC_n257I_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C ","DC_n257I_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3C","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3C","DC_n257J_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C ","DC_n257J_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3C","DC_n257K_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C ","DC_n257K_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_3C","DC_n257K_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C ","DC_n257K_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_3C-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_3C-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_003C_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257K_5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257K_8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257K_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_1A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_1A","DC_n257G_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A ","DC_n257G_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_1A","DC_n257H_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A ","DC_n257H_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_1A","DC_n257I_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A ","DC_n257I_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_1A","DC_n257J_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A ","DC_n257J_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_1A","DC_n257K_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A ","DC_n257K_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_1A","DC_n257L_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A ","DC_n257L_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3A","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3A","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3A","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3A","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3A","DC_n257K_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A ","DC_n257K_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3A","DC_n257L_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A ","DC_n257L_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3A-5A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_005A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3A-5A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_005A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257L_1A-3A-5A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_005A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257L_1A-3A-5A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_005A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257L_1A-3A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257L_1A-3A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257L_1A-3A-5A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_005A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257L_1A-3A-5A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_005A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257L_1A-3A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257L_1A-3A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3A-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3A-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3C","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003C ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3C","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003C ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3C","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003C ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3C","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003C ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3C","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003C ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3C","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003C ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3C","DC_n257K_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003C ","DC_n257K_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-3C","DC_n257L_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003C ","DC_n257L_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3C-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003C_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3C-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003C_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-3C-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_003C_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-5A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_005A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-5A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_005A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-5A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_005A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_1A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_1A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_001A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3A","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3A","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3A","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3A","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3A","DC_n257K_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A ","DC_n257K_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3A","DC_n257L_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A ","DC_n257L_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_3A-5A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_005A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_3A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_3A-5A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_005A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_3A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_3A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_3A-5A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_005A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_3A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257L_3A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_3A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_3A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_3A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_3A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_3A-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_3A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257A_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257A_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257G_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257G_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257H_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257H_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257I_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257I_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257J_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257J_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257K_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257K_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257K_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257K_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257L_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257L_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_3C","DC_n257L_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C ","DC_n257L_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_3C-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_3C-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_003C_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257L_5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257L_8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257L_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_1A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_1A","DC_n257G_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A ","DC_n257G_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_1A","DC_n257H_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A ","DC_n257H_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_1A","DC_n257I_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A ","DC_n257I_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_1A","DC_n257J_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A ","DC_n257J_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_1A","DC_n257K_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A ","DC_n257K_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_1A","DC_n257L_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A ","DC_n257L_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_1A","DC_n257M_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A ","DC_n257M_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3A","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3A","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3A","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3A","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3A","DC_n257K_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A ","DC_n257K_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3A","DC_n257L_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A ","DC_n257L_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3A","DC_n257M_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A ","DC_n257M_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3A-5A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_005A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3A-5A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_005A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257M_1A-3A-5A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_005A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257M_1A-3A-5A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_005A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257M_1A-3A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257M_1A-3A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257M_1A-3A-5A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_005A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257M_1A-3A-5A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_005A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257M_1A-3A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (5 bands)","38.101-3:Table 5.5B.5a.4-1","DC_n257M_1A-3A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3A-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3A-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3C","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003C ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3C","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003C ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3C","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003C ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3C","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003C ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3C","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003C ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3C","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003C ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3C","DC_n257K_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003C ","DC_n257K_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3C","DC_n257L_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003C ","DC_n257L_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-3C","DC_n257M_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003C ","DC_n257M_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3C-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003C_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3C-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003C_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-3C-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_003C_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-5A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_005A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-5A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_005A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-5A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_005A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_1A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-7A-7A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_007A_007A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-8A","DC_n257A_1A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_008A ","DC_n257A_001A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_1A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_001A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3A","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3A","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3A","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3A","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3A","DC_n257K_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A ","DC_n257K_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3A","DC_n257L_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A ","DC_n257L_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3A","DC_n257M_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A ","DC_n257M_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_3A-5A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_005A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_3A-5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_3A-5A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_005A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_3A-5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_3A-5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_3A-5A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_005A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_3A-5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (4 bands)","38.101-3:Table 5.5B.5a.3-1","DC_n257M_3A-5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_3A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_3A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_3A-7A-7A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_007A_007A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_3A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_3A-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_3A-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003A_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257A_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257A_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257G_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257G_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257G_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257G_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257H_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257H_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257H_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257H_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257I_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257I_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257I_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257I_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257J_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257J_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257J_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257J_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257K_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257K_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257K_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257K_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257L_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257L_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257L_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257L_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257M_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257M_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_3C","DC_n257M_3C","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C ","DC_n257M_003C ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_3C-8A","DC_n257A_3A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C_008A ","DC_n257A_003A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_3C-8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_003C_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_5A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_005A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_5A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_005A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_5A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_005A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_5A-7A-7A","DC_n257A_5A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_005A_007A_007A ","DC_n257A_005A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (3 bands)","38.101-3:Table 5.5B.5a.2-1","DC_n257M_5A-7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_005A_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_7A-7A","DC_n257A_7A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_007A_007A ","DC_n257A_007A ",null,"v1.0.0"]
[null,"Rel-17","NE-DC FR2 (2 bands)","38.101-3:Table 5.5B.5a.1-1","DC_n257M_8A","DC_n257A_8A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_n257M_008A ","DC_n257A_008A ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)3AA","DC_(n)3AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_znz003AA ","DC_znz003AA ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)5AA","DC_(n)5AA","Ongoing","PC3",null,null,"AT&T",null,"<RAN5#94-e","NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz005AA ","DC_znz005AA ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)7AA","DC_(n)7AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_znz007AA ","DC_znz007AA ",null,"v1.2.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)12AA","DC_(n)12AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz012AA ","DC_znz012AA ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)38AA","DC_(n)38AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz038AA ","DC_znz038AA ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41AA","DC_(n)41AA","Ongoing","PC3",null,null,"Legacy","Ericsson (Niclas Weiler)","<RAN5#94-e","TEI15_Test 5GS_NR_LTE-UEConTest","DC_znz041AA ","DC_znz041AA ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41AA","DC_(n)41AA PC2","Ongoing","PC2",null,null,"Legacy","Ericsson (Niclas Weiler)","<RAN5#94-e","TEI16_Test,ENDC_UE_PC2_TDD_TDD-UEConTest","DC_znz041AA ","DC_znz041AA PC002 ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41AA BCS1","DC_(n)41AA","Ongoing","PC3",null,null,"Legacy","Ericsson (Niclas Weiler)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_znz041AA BCS1 ","DC_znz041AA ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41AA BCS2","DC_(n)41AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz041AA BCS2 ","DC_znz041AA ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_(n)41AA-n78A","DC_41A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz041AA_n078A ","DC_041A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41AB","DC_41A_n41A","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz041AB ","DC_041A_n041A ","Fallback to DC_(n)41CA with UL DC_41A_n41A","v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41AB","DC_(n)41AA","Ongoing (FB)","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz041AB ","DC_znz041AA ","Fallback to DC_(n)41CA with UL DC_(n)41AA","v1.0.0"]
[null,"Rel-15","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41CA","DC_41A_n41A","Ongoing","PC3",null,null,"Legacy","Ericsson (Niclas Weiler)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_znz041CA ","DC_041A_n041A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41CA","DC_(n)41AA","Ongoing","PC3",null,null,"Legacy","Ericsson (Niclas Weiler)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_znz041CA ","DC_znz041AA ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41CA BCS1","DC_41A_n41A","Ongoing","PC3",null,null,"Legacy","Ericsson (Niclas Weiler)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_znz041CA BCS1 ","DC_041A_n041A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41CA BCS1","DC_(n)41AA","Ongoing","PC3",null,null,"Legacy","Ericsson (Niclas Weiler)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_znz041CA BCS1 ","DC_znz041AA ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41CA BCS2","DC_41A_n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz041CA BCS2 ","DC_041A_n041A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41CA BCS2","DC_(n)41AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz041CA BCS2 ","DC_znz041AA ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_(n)41CA-n78A","DC_41A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz041CA_n078A ","DC_041A_n078A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41DA","DC_41A_n41A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_znz041DA ","DC_041A_n041A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41DA","DC_(n)41AA","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_znz041DA ","DC_znz041AA ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41DA BCS1","DC_41A_n41A","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_znz041DA BCS1 ","DC_041A_n041A ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41DA BCS1","DC_(n)41AA","Pending","PC3",null,null,null,null,null,"TEI15_Test, 5GS_NR_LTE-UEConTest","DC_znz041DA BCS1 ","DC_znz041AA ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41DA BCS2","DC_41A_n41A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz041DA BCS2 ","DC_041A_n041A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)41DA BCS2","DC_(n)41AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz041DA BCS2 ","DC_znz041AA ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 (3 bands)","38.101-3:Table 5.5B.4.2-1","DC_(n)41DA-n78A","DC_41A_n78A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz041DA_n078A ","DC_041A_n078A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)48AA","DC_(n)48AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz048AA ","DC_znz048AA ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)48CA","DC_48A_n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz048CA ","DC_048A_n048A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)48CA","DC_(n)48AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz048CA ","DC_znz048AA ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)48DA","DC_48A_n48A","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz048DA ","DC_048A_n048A ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)48DA","DC_(n)48AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz048DA ","DC_znz048AA ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)66AA","DC_(n)66AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_znz066AA ","DC_znz066AA ",null,"v1.0.0"]
[null,"Rel-15","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)71AA","DC_(n)71AA","Completed","PC3","<=RAN5#93-e","R5-216625","Legacy","Samsung (Carolyn Taylor)","<RAN5#94-e","TEI15_Test, 5GS_NR_LTE-UEConTest","DC_znz071AA ","DC_znz071AA ",null,"v1.0.0"]
[null,"Rel-16","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)71AA BCS1","DC_(n)71AA","Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R16-UEConTest","DC_znz071AA BCS1 ","DC_znz071AA ",null,"v1.0.0"]
[null,"Rel-17","EN-DC FR1 IB cont","38.101-3:Table 5.3B.1.2-1","DC_(n)71AA BCS2",null,"Pending","PC3",null,null,null,null,null,"NR_CADC_NR_LTE_DC_R17-UEConTest","DC_znz071AA BCS2 "," ",null,"v1.4.0"]
[null,"Rel-17","EN-DC FR1 (2 bands)","38.101-3:Table 5.5B.4.1-1","DC_1A_n78C","DC_1A_n78A PC2","Pending","PC2",null,null,null,null,null,"ENDC_UE_PC2_R17_NR_TDD-UEConTest",null,null,null,"v1.5.0"]

{"sheet":"V2X bands","index":3,"n_rows":15,"n_cols":17,"rows_kept":15,"cut":false,"hidden":false,"merged":[[4,11,4,12],[5,2,5,10],[6,2,6,10],[7,2,7,10],[0,0,2,0],[0,2,0,10],[1,2,1,10],[3,2,3,10],[4,2,4,10]]}
[{"$f":"COUNTA(V2XbandsTblID[Marked config])&\" band items marked\"","v":"0 band items marked"},null,"3GPP RAN WG5 status for 5G NR V2X bands",null,null,null,null,null,null,null,null,null,null,{"$f":"PRD21version","v":"PRD21 v1.5.0"}]
[null,null,"Based on:  TS 38.101-1 v17.7.0 (Sep 2022)"]
[]
[null,null,"Completed: Green row indicates that the 5G NR V2X band is complete in the RAN5 test specifications. Available for testing."]
[null,null,"Ongoing: Yellow row indicates that the 5G NR V2X band for PC3 is ongoing and assigned to at least one \"Interested Deployer\" and at least one \"Responsible Company assignment\". CRs can be submitted to RAN5 test specifications."]
[null,null,"Ongoing: White row with black text indicates that the 5G NR V2X band is ongoing but pending assignment to a \"Responsible Company\". No CRs shall be submitted to the RAN5 specifications unless the company volunteers to be assigned as \"Responsible Company\"."]
[null,null,"Pending: White row with red text indicates that the 5G NR V2X band is pending assignment to \"Interested Company\". No CRs shall be submitted to the RAN5 specifications."]
[null,null,"Note 1: Power classes beyond PC3 applies to all CBWs of the NR band and are indicated by a \"PCx\" suffix in the NR band column and in the power class column, where x is the power class e.g. \"PC2\" for power class 2."]
["Marked config","Release introduced in TS 38.101-x","Type of band","TS and Source Table","NR V2X band","CBWs \nSCS[kHz]:[MHz]+...+[MHz]","PC3 Status","Power Class (Note 1)","RAN5 Completion Meeting\n(Note 1)","RAN5 Completion Reference\n(Note 1)","Interested Deployer","Responsible Company (contact)","Assignment\n[RAN5 meeting]","Applicable RAN5 WI code(s)  for CRs\n(Note 1)","Band Sort Key","Comments","Introduced in PRD version"]
[null,"Rel-17","V2X FR1","38.101-1:Table 5.2E.1-1","n14","SCS15:5+10\nSCS30:10","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XbandsTblID[[#This Row],[NR V2X band]])","v":" n014 "},"n14 CBWs 5 and 10 MHz are also used for NR operation (see \"NR bands\" worksheet for NR status)","v1.2.0"]
[null,"Rel-17","V2X FR1","38.101-1:Table 5.2E.1-1","n14 PC1",null,"Pending","PC1",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XbandsTblID[[#This Row],[NR V2X band]])","v":" n014 PC001 "},null,"v1.2.0"]
[null,"Rel-16","V2X FR1","38.101-1:Table 5.2E.1-1","n38","SCS15:10+20+30+40\nSCS30:10+20+30+40\nSCS60:10+20+30+40","Pending","PC3",null,null,null,null,null,"5G_V2X_NRSL_eV2XARC-UEConTest",{"$f":"SortKey(V2XbandsTblID[[#This Row],[NR V2X band]])","v":" n038 "},"n38 CBWs 10, 20, 30 and 40 MHz are also used for NR operation (see \"NR bands\" worksheet for NR status)","v1.2.0"]
[null,"Rel-16","V2X FR1","38.101-1:Table 5.2E.1-1","n47","SCS15:10+20+30+40\nSCS30:10+20+30+40\nSCS60:10+20+30+40","Pending","PC3",null,null,null,null,null,"5G_V2X_NRSL_eV2XARC-UEConTest",{"$f":"SortKey(V2XbandsTblID[[#This Row],[NR V2X band]])","v":" n047 "},null,"v1.2.0"]
[null,"Rel-17","V2X FR1","38.101-1:Table 5.2E.1-1","n47 PC2",null,"Pending","PC2",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XbandsTblID[[#This Row],[NR V2X band]])","v":" n047 PC002 "},null,"v1.2.0"]
[null,"Rel-17","V2X FR1","38.101-1:Table 5.2E.1-1","n79","SCS15:10+20+30+40\nSCS30:10+20+30+40\nSCS60:10+20+30+40","Pending","PC3","","",null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XbandsTblID[[#This Row],[NR V2X band]])","v":" n079 "},"n79 CBWs 10, 20, 30 and 40 MHz are also used for NR operation (see \"NR bands\" worksheet for NR status)","v1.2.0"]

{"sheet":"V2X Configurations","index":4,"n_rows":39,"n_cols":17,"rows_kept":39,"cut":false,"hidden":false,"merged":[[6,2,6,10],[7,2,7,10],[0,0,2,0],[3,0,7,0],[3,11,6,12],[0,2,0,10],[1,2,1,10],[3,2,3,10],[4,2,4,10],[5,2,5,10]]}
[{"$f":"COUNTA(V2XconfigTblID[Marked config])&\" configs marked\"","v":"0 configs marked"},null,"3GPP RAN WG5 status NR V2X configurations",null,null,null,null,null,null,null,null,null,null,{"$f":"PRD21version","v":"PRD21 v1.5.0"}]
[null,null,"Based on:  TS 38.101-1 v17.7.0 and TS 38.101-3 v17.7.0 (Sep 2022)"]
[]
[null,null,"Completed: Green row indicates that the 5G NR V2X configuration is complete in the RAN5 test specifications. Available for testing."]
[null,null,"Ongoing: Yellow row indicates that the 5G NR V2X configuration is assigned to at least one \"Interested Company\" or is a fallback to an ongoing configuration, and at least one \"Responsible Company\". CRs can be submitted to RAN5 test specifications."]
[null,null,"Ongoing: White row with black text indicates that the 5G NR V2X configuration is ongoing but not yet assigned to any \"Responsible Company\". No CRs shall be submitted to the RAN5 specifications unless the company volunteers to be assigned as \"Responsible Company\"."]
[null,null,"Pending: White row with red text indicates that the 5G NR V2X configuration is is pending assignment to \"Interested Deployer\". No CRs shall be submitted to the RAN5 specifications."]
[null,null,"Note 1: Power classes beyond PC3 are indicated by a \"PCx\" suffix in the \"Configuration\" and \"Power class\" columns, where x is the power class e.g. \"PC2\" for power class 2. Power classes beyond PC3 are only indicated for the items without any \"BCS\" suffix but applies to all bandwidth combination sets of the configuration (BCS1, BCS2 etc)."]
["Marked config","Release introduced in TS 38.101-x","Type of configuration","TS and Source Table","Configuration","Working mode","PC3 Status","Power Class (Note 1)","RAN5 Completion Meeting\n(Note 1)","RAN5 Completion Reference\n(Note 1)","Interested Deployer","Responsible Company (contact)","Assignment\n[RAN5 meeting]\n","Applicable RAN5 WI code(s)  for CRs\n(Note 1)","DL Sort Key","Comments","Introduced in PRD version"]
[null,"Rel-16","NR V2X FR1","38.101-3:Table 5.5E.2-1","V2X_(n)47AA","PC5-PC5","Pending","PC3",null,null,null,null,null,"5G_V2X_NRSL_eV2XARC-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_znz047AA "},null,"v1.2.0"]
[null,"Rel-16","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_20A-n38A","Uu-PC5","Pending","PC3",null,null,null,null,null,"5G_V2X_NRSL_eV2XARC-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_020A_n038A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_39A-n47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_039A_n047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_39A-n47A PC2","Uu-PC5","Pending","PC2",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_039A_n047A PC002 "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_3A-n47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_003A_n047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_3A-n47A PC2","Uu-PC5","Pending","PC2",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_003A_n047A PC002 "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_40A-n47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_040A_n047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_40A-n47A PC2","Uu-PC5","Pending","PC2",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_040A_n047A PC002 "},null,"v1.2.0"]
[null,"Rel-16","NR V2X FR1","38.101-3:Table 5.5E.3-1","V2X_47A_n47A","PC5-PC5","Pending","PC3",null,null,null,null,null,"5G_V2X_NRSL_eV2XARC-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_047A_n047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-1:Table 5.3E.2-1","V2X_n1A-n47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n001A_n047A "},null,"v1.3.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_n39A-47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n039A_047A "},null,"v1.3.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_n39A-47A PC2","Uu-PC5","Pending","PC2",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n039A_047A PC002 "},null,"v1.3.0"]
[null,"Rel-17","NR V2X FR1","38.101-1:Table 5.3E.2-1","V2X_n39A-n47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n039A_n047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_n40A-47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n040A_047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_n40A-47A PC2","Uu-PC5","Pending","PC2",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n040A_047A PC002 "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-1:Table 5.3E.2-1","V2X_n40A-n47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n040A_n047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-1:Table 5.3E.2-1","V2X_n41A-n47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n041A_n047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-1:Table 5.3E.2-1","V2X_n5A-n47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n005A_n047A "},null,"v1.3.0"]
[null,"Rel-16","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_n71A-47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"5G_V2X_NRSL_eV2XARC-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n071A_047A "},null,"v1.2.0"]
[null,"Rel-16","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_n71A-47A PC2","Uu-PC5","Pending","PC2",null,null,null,null,null,"5G_V2X_NRSL_eV2XARC-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n071A_047A PC002 "},null,"v1.2.0"]
[null,"Rel-16","NR V2X FR1","38.101-1:Table 5.3E.2-1","V2X_n71A-n47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"5G_V2X_NRSL_eV2XARC-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n071A_n047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_n78A-47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n078A_047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_n78A-47A PC2","Uu-PC5","Pending","PC2",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n078A_047A PC002 "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-1:Table 5.3E.2-1","V2X_n78A-n47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n078A_n047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_n79A-47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n079A_047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-3:Table 5.5E.4.1-1","V2X_n79A-47A PC2","Uu-PC5","Pending","PC2",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n079A_047A PC002 "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-1:Table 5.3E.2-1","V2X_n79A-n47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n079A_n047A "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-1:Table 5.3E.2-2","V2X_n79B","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n079B "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-1:Table 5.3E.2-2","V2X_n79B PC2","Uu-PC5","Pending","PC2",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n079B PC002 "},null,"v1.2.0"]
[null,"Rel-17","NR V2X FR1","38.101-1:Table 5.3E.2-1","V2X_n8A-n47A","Uu-PC5","Pending","PC3",null,null,null,null,null,"NR_SL_enh-UEConTest",{"$f":"SortKey(V2XconfigTblID[[#This Row],[Configuration]])","v":"V002X_n008A_n047A "},null,"v1.3.0"]

{"sheet":"Revision History","index":5,"n_rows":60,"n_cols":9,"rows_kept":60,"cut":false,"hidden":false,"merged":[[45,2,58,2],[45,0,58,0],[5,1,12,1],[13,1,28,1],[29,1,44,1],[45,1,58,1],[0,6,0,7],[0,8,0,15],[5,0,12,0],[13,0,28,0],[29,0,44,0],[5,2,12,2],[13,2,28,2],[29,2,44,2]]}
["RAN5 meeting","Date","PRD21 version","Introduced changes",null,null,"PRD21 contacts:",null,"songdan@chinamobile.com"]
["RAN5#99","2023-Mar","v1.5.0","1. 5G NR CADC Configuration worksheet: Added missing PC2 configurations for RAN5 WI ENDC_PC2_R17_xLTE_yNR-UEConTest (33 configurations) and removed configurations removed from the associated RAN4 work item when it was closed."]
[]
[]
["RAN5#98","2023-Mar","v1.4.1","Removed unused Microsoft library to avoid error message \"Compile error: Can't find find project or library\" when the workbook is opened on a computer using older version of Microsoft Windows."]
["RAN5#98","2023-Mar","v1.4.0","1. Update of new NR bands introduced for RAN5 work items, and NR CA, NR-DC, NE-DC and EN-DC configurations introduced in TS 38.101-x v17.8.0 (Dec 2022)"]
[null,null,null,"2. 5G NR CADC Configurations worksheet: Moved the power class suffix \"PC2\",\"PC1.5\" etc. from the configuration column to the UL configuration column. Note 1 updated to refer to the UL configuration."]
[null,null,null,"3. Introduction worksheet: Corrected header text in all summary tables (removed \"LTE CA\")"]
[null,null,null,"4. 5G NR CADC Configurations worksheet: Corrected release for PC2 configurations currently indicated as Rel-15 to the release of the associated RAN5 work item introducing them."]
[null,null,null,"5. Introduction worksheet: Text updated to also refer to V2X bands and configurations (R5-231281)"]
[null,null,null,"6. 5G NR CADC Configurations worksheet: Remove DL/UL configuration combinations for the case the DL and UL FR2 bandwidth class (BWC) belongs to different fallback groups as specified in TS 38.101-2 Table 5.3A.4-1. Example: Removed configurations CA_n3A-n77(2A)-n257G with  UL configuration CA_n3A-n257D as FR2 BWC D belongs to fallback group 2 while BWC G belongs to fallback group 3."]
[null,null,null,"7.  Set status column for all EN-DC configurations with NR FR1+FR2 to N/A with comment column set to \"This FR1+FR2 config is not testable\". "]
[null,null,null,"8. Updated based on RAN5#97 submitted CDS documents:\n        PC3 NR bands: R5-230064\n        CBW extensions: R5-230665\n        PC3 NR CA configurations: R5-230254,R5-230291,R5-230292,R5-230293,R5-230664,R5-231217,R5-231230\n        PC3 EN-DC: R5-230758,R5-230759,R5-230760,R5-230761,R5-231282,R5-231283,R5-230188,\n                                  R5-230758,R5-230759,R5-230760,R5-231282,R5-231283\n        PC2 EN-DC: R5-230663"]
["RAN5#97","2022-Sep","v1.3.0","1. Updated V2X bands and V2X configurations based on TS 38.101-x v17.7.0 (Sep 2022). Update of new configurations for NR bands, NR CADC configurations introduced in TS 38.101-x v17.7.0 (Sep 2022) has not been done as RAN5 endorsed proposal to limit 5G NR CADC configurations to the ones requested by interested deployer to include from RAN5#98 and forward (i.e. all pending configurations in current list will be removed from v1.4.0 of PRD21)."]
[null,null,null,"2. Updates based on interested operator/deployer and responsible company assignment requests up to and at RAN5#97. Filter on \"RAN5#97\" in column \"Assignment [RAN5 meeting]\" in NR band and CADC worksheets to show the new assignments."]
[null,null,null,"3. 5G NR CADC worksheet: Updates of PC2 and PC1.5 configurations based on RAN5#97 work plans for PC2 and PC1.5 work items."]
[null,null,null,"4. NR band worksheet: Split of n79 CBW(10,20,30.70.90) into 79 CBW(10,20) and n79 CBW(30.70.90) ."]
[null,null,null,"5. NR band bands and 5G NR CADC worksheets: Renamed \"Interested operator\" to \"Interested deployer\" and updated Note 2 for the case the interested deployer is not an MNO then then the type of deployer is described in the comments column. See the railway bands n100 and n101 as an example."]
[null,null,null,"6. V2X bands and V2X Configurations worksheets: Renamed \"Interested company\" to \"Interested deployer\""]
[null,null,null,"7. NR band worksheet: As agreed in proposal 1 in R5-224256 at RAN5#96-e the Rel-15 NR bands n50 and n86 is marked as interested operator = \"Legacy\" and add CAICT as responsible company."]
[null,null,null,"8. 5G NR CADC worksheet: Correct completed power classes column adding PC2 for DC_2A_n77A, DC_5A_n77A, DC_13A_n77A, DC_66A_n77A (were completed as per change 15 below at RAN5#96-e)."]
[null,null,null,"9. V2X band and V2X configuration worksheets:  Updated of working mode for V2X_(n)47AA and V2X_47A_n47A to PC5-PC5.  Added PC2 WI code for V2X_n39A-47A."]
[null,null,null,"10 . NR band worksheet: Add missing Rel-17 FDD band n85, SDL band n67 and TDD band n104 as new pending configurations (WI:NR_lic_bands_BW_R17-UEConTest)."]
[null,null,null,"11 . 5G NR CADC worksheet: Rel-16 EN-DC configuration DC_48A-(n)48AA moved from 38.101-3 Table 5.3B.1.3-1 to Table 5.3B.1.3-2 in 38.101-3 v16.13.0. The new Table 5.3B.1.3-2 added to the introduction worksheet."]
[null,null,null,"12 . 5G NR CADC worksheet: Changed status from \"Ongoing(FB)\" to \"Pending\" (R5-227259) for NR CA configurations with intra-band non-contiguous UL CA that was incorrectly set to \"Ongoing(FB)\" with reference to NR CA configuration without UL CA. Impacted NR CA configurations are: CA_n41(2A) with UL:CA_n41(2A), CA_n66A-n77(2A) with UL:CA_n77(2A), CA_n66A-n77(2A) BCS1with UL:CA_n77(2A), CA_n66(2A)-n77(2A) with UL:CA_n77(2A), CA_n66(2A)-n77(2A) BCS1 with UL:CA_n77(2A), CA_n78(2A) with UL:CA_n78(2A), CA_n78(2A) BCS1 with UL:CA_n78(2A), CA_n78(2A) BCS2 with UL:CA_n78(2A)."]
[null,null,null,"13. NR bands and 5G NR CADC worksheets: Split into separate rows per power class, and adding new filtering selection for filtering by power classes."]
[null,null,null,"14. V2X bands and V2X Configurations worksheets: Split into separate rows per power class."]
[null,null,null,"15. 5G NR CADC worksheet: For configuration type \"EN-DC FR1+FR2\" set status to \"N/A\" and adding \"This FR1+FR2 config is not testable\" to the comments column."]
[null,null,null,"16. Updated based on RAN5#97 submitted CDS documents:\n        PC3 NR bands: R5-225951, R5-226274, R5-226275\n        PC2 NR bands: R5-227635, R5-227636\n        PC1.5 NR bands: R5-227633, R5-227634, R5-227637, R5-227638\n        CBW extensions: R5-226867,R5-226871,R5-227115\n        PC3 NR CA configurations: R5-226403,R5-226404,R5-226405,R5-227303,R5-227629\n       "]
["RAN5#96-e","2022-Aug","v1.2.0","1. Updated based on TS 38.101-x v17.6.0 (June 2022) \nUpdates based on interested operator and responsible company assignment requests up to and at RAN5#96-e."]
[null,null,null,"2. Fixed configuration syntax for Rel-15 EN-DC configurations DC_2A-66A_(n)71AA, DC_2A_(n)71AA and DC_66A_(n)71AA to DC_2A-66A-(n)71AA, DC_2A-(n)71AA and DC_66A-(n)71AA and removed associated duplicates in Rel-16."]
[null,null,null,"3. For legacy configurations started before the concept of \"Interested operators\" was introduced the column \"Interested operator\" is set to \"Legacy\"."]
[null,null,null,"4. Added TS 38.101-1 Table 5.5B.1-2 (NR-DC FR1, three bands) and Table 5.5B.1-3 (NR-DC FR1, four bands) to introduction worksheet."]
[null,null,null,"5. Removed  36 5G NR CADC configurations to align with TS 38.101-x. See attached note for details."]
[null,null,null,"6. Corrected  2 5G NR CADC configurations to align with TS 38.101-x. See attached note for details."]
[null,null,null,"7. NR SUL bands n80 and n83 set to completed in NR bands worksheet as associated with completed NR CA SUL configurations including the SUL bands (Ref:R5-225269)."]
[null,null,null,"8. NR band worksheet: Added assignment date to the legacy Rel-15 NR bands not have any RAN5 meeting shown in PRD21 v1.1.0. Corrected Rel--17 NR bands and CBW extensions without any interested operator from \"Ongoing\" to \"Pending\""]
[null,null,null,"9. NR band worksheet: Added new PC2 WI code NR_PC2_UE_FDD-UEConTest for NR bands n1 and n2."]
[null,null,null,"10. NR band worksheet: Added NR bands n90, n91, n92, n93 and n94 (NR_bands_BW_R16-UEConTest) . "]
[null,null,null,"11. Added PC2 WI code \"PC2: NR_RF_FR1_enh-UEConTest\" to the following DL/UL configurations:\n   CA_n41C/CA_n41C\n   CA_n41C BCS1/CA_n41C\n   CA_n41C BCS2/CA_n41C\n   CA_n41C BCS4and5/CA_n41C\n   CA_n41(2A)/CA_n41(2A)\n   CA_n41(2A) BCS1/ CA_n41(2A)\n   CA_n77C/CA_n77C\n   CA_n77C BCS1/ CA_n77C\n   CA_n78C/CA_n78C\n   CA_n78C BCS1/CA_n78C\n   CA_n78(2A)/CA_n78(2A)\n   CA_n78(2A) BCS1/CA_n78(2A)\n   CA_n78(2A) BCS2/CA_n78(2A)"]
[null,null,null,"12.Extended the scope to V2X bands and configurations adding new \"V2X bands\" and \"V2X Configurations\" worksheets. Updated \"introduction\" worksheet to show overview of V2X bands and configurations (Ref: R5-225269)."]
[null,null,null,"13.NR bands worksheet: Corrected covered CBWs for n65 initial item removing CBW 50 MHz as 50MHz is introduced as an separate CBW extension item \"n65 CBW (50)\"."]
[null,null,null,"14.NR bands worksheet:  PC3 status of n40 CBW (90,100), n65 CBW (50) and n80 CBW (40) channel bandwidth extensions changed \"Ongoing (CBW)\" in accordance to R5-225269 due to introducing mandatory highest CBW."]
[null,null,null,"15.Updated based on RAN5#96-e submitted CDS documents:\n        CBW extensions: R5-224021, R5-224022\n        PC3 CADC configurations: R5-224147, R5-224148, R5-224230, R5-224616, R5-225447\n        PC2 CADC configurations: R5-224367, R5-224494"]
[null,null,null,"16.Corrected status of CA_n1A-n78A with UL CA for PC3 (BCS0 UL CA was completed together with the DL only case)."]
["RAN5#95-e","2022-May","v1.1.0","Updated based on TS 38.101-x v17.5.0 (March 2022)\nUpdates based on interested operator and responsible company assignment requests up to and at RAN5#95-e."]
[null,null,null,"1. Removed  37 5G NR CADC configurations to align with TS 38.101-x. See attached note for details.\n"]
[null,null,null,"2. Table 5.5A.3.1-1  for two bands NR CA FR1 in TS 38.101-1 has been split into Tables 5.5A.3.1-1a to 5.5A.3.1-1n. In PRD21 are the configurations grouped by the reference to \"Table 5.5A.3.1-1a-n\" "]
[null,null,null,"3. Table 5.5A.1-1a for two bands NR CA between FR1 and FR2 in TS 38.101-3  has been split into Tables 5.5A.1-1a to 5.5A.1-1o. In PRD21 are those configurations grouped by the reference to \"Table 5.5A.1-1a-o\" "]
[null,null,null,"4. Added 8083 new 5G NR CADC configurations to align with TS 38.101-x. Filter on v1.0.0 in column \"Introduced in PRD version\" in \"5G NR CADC Configurations\" worksheet to see the list of the new configurations."]
[null,null,null,"5. Added missing n96 (Rel-16) initial channel bandwidths to the \"NR bands\" worksheet (introduced in TS 38.101-1 Rel-16)"]
[null,null,null," 6. Added references to WI code \"ENDC_PC2_R17_xLTE_yNR-UEConTest\" for new PC2 EN_DC configurations introduced at RAN5#95-e."]
[null,null,null," 7. Removed completion indication for DC_41A_n41A and DC_(n)41AA and PC2. Completion of WI ENDC_UE_PC2_TDD_TDD-UEConTest in WP R5-203332 did not complete those two configurations. "]
[null,null,null," 8. The marking of range of configurations updated to handle the case when range of rows selected is not contiguous due to a filter is applied. Only the contiguous configurations from the first selected row is marked."]
[null,null,null," 9. Corrected PC3 status from \"Pending\" to \"Ongoing(FB)\" for fallback configurations to interested operator assigned configurations."]
[null,null,null," 10. For the case Microsoft Outlook is not supported as email client then instructions and text to copy and paste to an email in the supported email client is provided."]
[null,null,null," 11. For NR CADC configuration worksheet updated description for configuration highlighted in yellow to also include the case of fallback configurations with a responsible company assigned."]
[null,null,null," 12. Updated based on RAN5#95-e submitted CDS documents to NR band and CBW list: R5-222357, R5-222358, R5-223500, R5-223501, R5-223502"]
[null,null,null," 13. Updated based on RAN5#95-e submitted CDS documents to CADC list: R5-222236, R5-222237, R5-222238, R5-222239, R5-222240, R5-222282, R5-223023, R5-223151, R5-223203, R5-223204, R5-223205, R5-223206, R5-223207, R5-223208, R5-223209, R5-223210, R5-223211"]
["RAN5#94-e","2022-Mar","v1.0.0","Initial version"]

{"sheet":"Assignment template","index":6,"n_rows":1,"n_cols":5,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Band/Config","UL config/CBW","Interested Operator","RAN5 responsible Company","Contact"]