Companies are to share their inputs on the excel spreadsheet in /tsg\_ran/WG1\_RL1/TSGR1\_106b-e/Inbox/drafts/8.1.2.3/RRC parameters/ herein.

## Inputs on version 00

Please share your inputs, if any, in the following table

Table 1 Inputs: Initial version

|  |  |
| --- | --- |
| **Company** | **Input** |
| Qualcomm | For the row “new beam identification threshold for TRP 2”, suggest to add the following FFS. The use case for separate thresholds is unclear.  FFS: whether this parameter can reuse “new beam identification threshold for TRP 1”, i.e. same threshold for both TRPs  For the row #8 and 9, suggest to add PCI field to indicate SSB is from which cell.  resource list (including periodic CSI-RS resource configuration indexes and/or SS/PBCH block indexes and corresponding PCI if different from serving cell PCI) for M-TRP new beam identification set 1 |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Inputs on version xx

Please share your inputs, if any, in the following table

....