**3GPP TSG RAN WG2#119-e R2-22XXXXX**

**E-Meeting, 17 - 29 August, 2022**

Title: [Draft] Reply LS on transferring SDT configuration and SRS positioning Inactive configuration from DU to CU

Response to: -

Release: Release 17

Work Item: NR\_SmallData\_INACTIVE-Core, NR\_pos\_enh

Source: Google (to be RAN2)

To: RAN3

Cc:

**Contact Person:**

Name: Frank Wu

Tel. Number: -

E-mail Address: frankwu@google.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

Attachments:

**1. Overall Description:**

RAN2 thanks RAN3 for the LS on transferring SDT configuration and SRS positioning Inactive configuration from DU to CU and would like to provide the following information for RAN3 consideration.

1. *SDT-MAC-PHY-CG-Config-r17* and *SRS-PosRRC-InactiveConfig-r17* IEs are the ones to be referred to in the RAN3 specification.
2. The two IEs should be defined in F1-AP as an "OCTET STRING" for the CU to transparently include the two IEs in the *RRCRelease* message.

**2. Actions:**

**To RAN3 group.**

**ACTION:** RAN2 respectfully asks RAN3 to take the above into consideration in the RAN3 specification.

**3. Date of Next RAN WG3 Meetings:**

RAN2 #119bis-e 10 – 19 October 2022 Electronic Meeting

RAN2 Meeting #120 14 – 18 November 2022 Canada