**3GPP TSG-WG SA2 Meeting #154-AH *S2-2301010r04***

**e-Meeting, January 16 – 20, 2023 (revision of S2-230xxxx)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **23.501** | **CR** | **4039** | **rev** | **-** | **Current version:** | **18.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Resolving EN on emergency services. | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Samsung | | | | | | | | | |
| ***Source to TSG:*** | SA2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | VMR | | | | |  | ***Date:*** | | | 2023-01-16 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Following EN is available in the spec:  Editor's note: Handling of UEs accessing emergency service while served by a MBSR, including when the MBSR becomes unable/not allowed to provide the relay service, is FFS.  This tdoc proposes to resolve this EN with a clarification that UEs served by that MBSR can be handed over to another RAN node or based on implementation MBSR release can be delayed. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Resolve the EN | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | EN is not resolved. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.35A.3.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* \* First change (all new) \* \* \* \*

5.35A.3.1 UE mobility between a fixed cell and MBSR cell

The procedure of Inter-gNB-DU Mobility as defined in TS 38.401 [42] or the handover procedure using the Xn/N2 reference points as defined in TS 23.502 [3] can be used.

For UEs in RRC\_IDLE and RRC\_INACTIVE state when a MBSR goes out-of-service, procedure for cell (re-)selection as specified in TS 38.304 [50] for RRC\_IDLE and RRC\_INACTIVE is used.

For UEs in RRC Connected state, if the MBSR goes out-of-service due to e.g. MBSR moves to an area where the MBSR is not allowed to provide the relay service, the procedure for IAB node release as specified in TS 38.401 [42] is used.

The IAB-donor-CU triggers handover procedure for the UEs accessing emergency service and being served by the MBSR, if MBSR is about to become unavailable to provide the services..

\* \* \* \* End of changes \* \* \* \*