**3GPP TSG-SA3 Meeting #104-e *S3-213004***

e-meeting, 16 - 27 August 2021

**Title: [DRAFT] Reply LS on QoE report handling at QoE pause**

**Response to: LS R2-2106775** **on QoE report handling at QoE pause**

**Release: Rel-17**

**Work Item: NR\_QoE-Core**

**Source: Lenovo [to be SA3]**

**To: RAN2**

**Cc: SA4, SA5**

**Contact person: Andreas Kunz**

 **akunz@lenovo.com**

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** **None**

# 1 Overall description

SA3 thanks RAN2 for their LS on QoE report handling at QoE pause. SA3 discussed the potential security issue raised for Option 1 (“Application layer is responsible for storing QoE reports when the UE receives QoE pause indication”) and arrived at the following conclusion:

SA3 does not see any security issue with any of the Options listed in the LS (including Option 1).

# 2 Actions

**To RAN2:**

**ACTION:** SA3 kindly asks RAN2 to take the above information into account in their future work.

# 3 Dates of next TSG SA WG 3 meetings

SA3#105-e 8 - 12 November 2021 Electronic meeting

SA3#106 7 - 11 February 2022 EU