**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correction of clause title for GeographicCoordinates type  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The title of the clause describing the GeographicalCoordinates type is incorrect. This contribution proposes to fix the title of the clause. |
|  |  |
| ***Summary of change:*** | This contribution proposes to change the title of the clause to match the ASN type. |
|  |  |
| ***Consequences if not approved:*** | The clause title will not align with the ASN Type. |
|  |  |
| ***Clauses affected:*** | 7.3.3.2.12 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | s3i240012 |

## \*\*\*\* START OF FIRST CHANGE (MAIN DOCUMENT) \*\*\*\*

##### 7.3.3.2.12 Type: GeographicalCoordinates

The GeographicalCoordinates type is derived from the data present in the GeographicalCoordinates type defined in TS 29.572 [24] clause 6.1.6.2.4.

Table 7.3.3.2.12-1 contains the details for the GeographicalCoordinates type.

Table 7.3.3.2.12-1: Definition of type GeographicalCoordinates

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Field name | Type | Cardinality | Description | M/C/O |
| latitude | UTF8String | 1 | Shall contain a string representation of the latitude. | M |
| longitude | UTF8String | 1 | Shall contain a string representation of the longitude. | M |
| mapDatumInformation | OGCURN | 0..1 | The reference datum used for the GeographicalCoordinates. Shall be present if known by the operator. | C |
| NOTE: The order of the latitude and longitude parameters in the localy defined GeographicalCoordinates type are different than the order of the parameters defined by the GeographicalCoordinates type defined in TS 29.572 [24] clause 6.1.6.2.4. |

## \*\*\*\* END OF MAIN DOCUMENT CHANGES \*\*\*\*

## \*\*\*\* END OF ALL CHANGES \*\*\*\*