**3GPP TSG-SA5 Meeting #129e *S5-201600***

**e-meeting, 24 February – 4 March 2020**

|  |
| --- |
| *CR-Form-v11.4* |
| **CHANGE REQUEST** |
|  |
|  | **28.533** | **CR** | **0064** | **rev** | **2** | **Current version:** | **16.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Update of Management service description and diagram |
|  |  |
| ***Source to WG:*** | Huawei, Nokia |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | NETSLICE |  | ***Date:*** | 2020-02-12 |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | MnS is provided by MnS Producer and consumed by MnS Consumer is not clearly described in Clause 4.1. |
|  |  |
| ***Summary of change:*** | Correct Figure 4.1.1 and text to clear desribe that MnS is provided by MnS Producer and consumed by MnS Consumer. |
|  |  |
| ***Consequences if not approved:*** | The figure 4.1.1 and test in cluse 4.1 is confusing for relation of MnS, MnS Producer and MnS Consumer; |
|  |  |
| ***Clauses affected:*** | 4.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |

|  |  |
| --- | --- |
| ***This CR's revision history:*** | S5-201552 is the revision of S5-201362S5-201600 is the revision of S5-201552 and S5-201419 |

|  |
| --- |
| **1st Change** |

# 4 Management framework

## 4.1 Management Services

An Management Service (MnS) offers capabilities for management and orchestration of network and service. The entity producing an MnS is called MnS producer. The entity consuming an MnS is called MnS consumer. An MnS provided by an MnS producer can be consumed by any entity with appropriate authorisation and authentication.

An MnS producer offers its services via a standardized service interface composed of individually specified MnS components.



Figure 4.1.1: MnS producer and MnS consumer

|  |
| --- |
| **End of Change** |