Definition of Constrained Device

The definition we now have in the TS is this:

***Constrained UE:*** *a UE (with or without MSGin5G Client) which may not have capability to connect to the 3GPP network.*

This definition is vague.

A regular MSGin5G UE that has an MSGin5G Client and is capable of connecting to the 3GPP network is a constrained UE under the current definition. Every device UE we are considering is a Constrained UE under this definition!

Proposal:

***Constrained UE:*** *an MSGin5G UE which does not have capability to connect to the 3GPP network.*