**3GPP TSG-SA WG6 Meeting #51-e S6-222752**

**e-meeting, 10th – 19th October 2022 (revision of S6-22xxxx)**

**Title: Reply LS on Clarification of Edge Node Sharing**

**Response to: LS S6-222618 on LS reply to 3GPP SA6 on Clarification of Edge Node Sharing from GSMA OPG**

**Release: Release-18**

**Work Item: FS\_eEDGEAPP**

**Source:** **3GPP TSG SA WG6#51-e**

**To: GSMA OPG**

**Cc: 3GPP SA, SA2**

**Contact person: Sapan Shah**

 **sapan.shah@samsung.com**

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** **None**

# 1 Overall description

3GPP SA6 thanks GSMA OPG for their reply LS on edge node sharing considering the mapping of GSMA OP and 3GPP EDGEAPP architecture.

**Question:**

*“Only one registration is performed between the UE-A and OP–A. The UE-A is then redirected towards the content hosted by OP - B with who edge sharing is performed. GSMA OPG would like to receive 3GPP SA6 feedback if the current procedure is acceptable.”*

**Answer:**

3GPP SA6 agrees that only one registration is performed between user client in UE-A and OP-A. And upon receiving the discovery request from UE-A, the OP-A redirect the UE-A by providing application endpoint of shared edge node in OP-B.

# 2 Actions

**To GSMA OPG**

**ACTION:** SA6 requests GSMA to consider above answer into their work, and further requests to share result of their study as indicated in their LS response.

# 3 Dates of next TSG SA WG 6 meetings

SA6#52-e 14th November – 18th November 2022 meeting

SA6#52-bis-e 16th January – 25th January 2023 meeting