**3GPP TSG-SA3 Meeting #99e *S3-201118***

**e-meeting, 11 – 15 May 2020** Revision of S3-20xxxx

**Title:** LS on resolving the gaps in NSSAA procedure

**Response to:**

**Release:** Rel-16

**Work Item:** FS\_ eNS\_SEC

**Source:** SA3

**To:** SA2

**Cc:**

**Contact Person:**

#### Name: Juan Deng

**Tel. Number:**

E-mail Address: dengjuan5@huawei.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:**

**1. Overall Description:**

SA3 has been studying in Network Slice-Specific Authentication and Authorization procedure and identifies that GPSI is needed by the AAA to inform the core network which UE the AAA intends to communicate/re-authenticate/revoke, i.e., GPSI is a must in the NSSAA.

Essentially there may be a gap for a UE in the case where the UE supports NSSAA and has subscribed S-NSSAI which is subject to NSSAA and has not been allocated a GPSI.

**2. Actions:**

**To SA2 group.**

**ACTION:** SA3 kindly asks the SA2 group to take the above information into account and solve the gap in any appropriate way.

**3. Date of Next TSG-SA WG5 Meetings:**

SA3#100bis 17 – 21 August 2020 US, US

SA3#101 09 – 13 November 2020 India, IN